# SANE: Backends (Drivers)

The following table summarizes the backends/drivers distributed with sane-backends-1.0.27, and the hardware or software they support.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

## Summary

Device type | Number of devices
--- | ---
Total | Supported | Untested | Unsupported
Sum | Complete | Good | Basic | Minimal
Scanners | 2444 | 1551 | 696 | 717 | 114 | 24 | 405 | 488
Still cameras | 5 | 5 | 1 | 2 | 2 | 0 | 0 | 0
Video Cameras | 8 | 3 | 0 | 1 | 0 | 2 | 3 | 2
Meta backends | 2 | n/a
APIs | 6 | n/a

## Scanners

Backends: abaton, agfafocus, apple, artec, artec_eplus48u, as6e, avision, bh, canon, canon630u, canon_dr, canon_pp, cardscan, coolscan, coolscan2, coolscan3, dell1600n_net, epjitsu, epson, epson2, epsonds, fujitsu, genesys, gt68xx, hp, hp3500, hp3900, hp4200, hp5400, hp5590, hpljm1005, hpsj5s, hs2p, ibm, kodak, kodakaio, kvs20xx, kvs40xx, kvs1025, leo, lexmark, ma1509, magicolor, matsushita, microtek, microtek2, mustek, mustek_pp, mustek_usb, mustek_usb2, nec, niash, p5, pie, pieusb, pixma, plustek, plustek_pp, ricoh, rts8891, s9036, sceptre, sharp, sm3600, sm3840, SnapScan, sp15c, st400, tamarack, teco1, teco2, teco3, template, u12, umax, umax1220u, umax_pp, unsupported, xerox_mfp

### Backend: abaton (unmaintained)

Manual page: sane-abaton

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Abaton | Scan 300/GS | SCSI |  | Complete | All known modes and functions supported
Scan 300/S | SCSI |  | Untested | Untested, use with caution

### Backend: agfafocus (unmaintained)

Manual page: sane-agfafocus

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
AGFA | Focus GS Scanner | SCSI |  | Untested | 6 bit gray
Focus Lineart Scanner | SCSI |  | Untested | Lineart only? Untested.
Focus II | SCSI |  | Untested | gray only
Focus Color | SCSI |  | Good | 3-pass
Focus Color Plus | SCSI |  | Good | 3-pass
Siemens | S9036 | SCSI |  | Untested | gray only

### Backend: apple (unmaintained)

Manual page: sane-apple

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Apple | Apple Scanner | SCSI |  | Good | 4bit, 16 shades of gray
OneScanner | SCSI |  | Basic | 8bit, 256 shades of gray. The backend needs work especially in the quantization code but it may work.
Color OneScanner | SCSI |  | Minimal | truecolor (needs much work) but it scans in non color modes.

### Backend: artec (unmaintained)

Link(s): http://www4.infi.net/~cpinkham/sane/sane-artec-doc.html
Manual page: sane-artec

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Artec/Ultima | AT3 | SCSI |  | Complete | all modes working
A6000C | SCSI |  | Complete | all modes working
A6000C PLUS | SCSI |  | Complete | f/w <= v1.92 basic, f/w >= v1.93 OK
AT6 | SCSI |  | Good | Scan head needs to return home before another scan can be started.
AT12 | SCSI |  | Complete | all modes working
AM12S | SCSI |  | Complete | all modes working
BlackWidow | BW4800SP | SCSI |  | Complete | rebadged Artec AT3
Plustek | OpticPro 19200S | SCSI |  | Complete | rebadged Artec AM12S

### Backend: artec_eplus48u (unmaintained)

Manual page: sane-artec_eplus48u

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Artec/Ultima | E+ 48U | USB | 0x05d8/0x4003 | Good | CIS scanner based on the GT6816 chip. Apparently all other devices are re-badged Artec scanners.
E+ Pro | USB | 0x05d8/0x4004 | Minimal | Works up to 600dpi, but not 1200. Needs better calibration. See bug #310490
Medion/Lifetec/Tevion/Cytron | MD9693 | USB | 0x05d8/0x4003 | Good |
MD9705 | USB | 0x05d8/0x4003 | Good |
MD4394 | USB | 0x05d8/0x4003 | Good | Only scanners with product id 0x4003 will work; try the gt68xx backend, if your scanner has product id 0x4002
Trust | Easy Webscan 19200 | USB | 0x05d8/0x4006 | Good |
240H Easy Webscan Gold | USB | 0x05d8/0x4007 | Basic | Works up to 600 dpi
Memorex | MEM 48U | USB | 0x05d8/0x4005 | Good |
Microstar | MR 9791 | USB | 0x05d8/0x4003 | Good |
UMAX | AstraSlim SE | USB | 0x05d8/0x4009 | Good |
AstraSlim 1200 SE | USB | 0x05d8/0x4010 | Good |
Yakumo | Scan50 | USB | 0x05d8/0x4011 | Good |

### Backend: as6e (0.5 (unmaintained))

Link(s): http://as6edriver.sourceforge.net/
Manual page: sane-as6e

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Artec/Ultima | AS6E | Parport |  | Basic | Requires the program 'as6edriver' to run.
Trust | Easy Scan 9600 Plus | Parport |  | Basic | Requires the program 'as6edriver' to run.
Dexxa | 4800 | Parport |  | Basic | Requires the program 'as6edriver' to run.

### Backend: avision (Build: 296)

Link(s): http://exactcode.com/site/open_source/saneavision/
Manual page: sane-avision

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Avision | AV100CS | SCSI |  | Untested |
AV100IIICS | SCSI |  | Untested |
AV100S | SCSI |  | Untested |
AV120 | USB | 0x0638/0x0a27 | Complete | sheetfed scanner
AV121 | USB | 0x0638/0x0a3c | Good | sheetfed scanner
AV122 | USB | 0x0638/0x0a33 | Good | sheetfed duplex scanner
AV122 C2 | USB | 0x0638/0x0a93 | Good | sheetfed duplex scanner
AV210 | USB | 0x0638/0x0a24 | Complete | sheetfed scanner
AV210 | USB | 0x0638/0x0a25 | Complete | sheetfed scanner
AV210C2 | USB | 0x0638/0x0a3a | Complete | sheetfed scanner
AV210C2-G | USB | 0x0638/0x0a2f | Complete | sheetfed scanner
AV210D2+ | USB | 0x0638/0x1a35 | Complete | sheetfed scanner
AV220 | USB | 0x0638/0x0a23 | Complete | duplex! sheetfed scanner
AV220C2 | USB | 0x0638/0x0a2a | Complete | duplex! sheetfed scanner
AV220D2 | USB | 0x0638/0x0a2b | Basic | duplex! sheetfed scanner
AV220D2 | USB | 0x0638/0x1a31 | Untested | duplex! sheetfed scanner
AV220+ | USB | 0x0638/0x0a2c | Complete | duplex! sheetfed scanner
AV220C2-G | USB | 0x0638/0x0a2d | Complete | duplex! sheetfed scanner
AV220C2-B | USB | 0x0638/0x0a2e | Complete | duplex! sheetfed scanner
AV220-G | USB | 0x0638/0x0a94 | Complete | duplex! sheetfed scanner
AV240SC | SCSI |  | Untested |
AV260CS | SCSI |  | Untested |
AV360CS | SCSI |  | Untested |
AV363CS | SCSI |  | Untested |
AV420CS | SCSI |  | Untested |
AV6120 | SCSI |  | Untested |
AV610 | USB | 0x0638/0x0a18 | Good |
AV600U Plus | USB | 0x0638/0x0a18 | Good |
AV610C2 | USB | 0x0638/0x0a5e | Good |
AM3000 Series | USB | 0x0638/0x0a41 | Basic | MFD
DS610CU Scancopier | USB | 0x0638/0x0a16 | Good | 1 pass, 600 dpi, A4
AV620CS | SCSI |  | Complete | 1 pass, 600 dpi
AV620CS Plus | SCSI |  | Complete | 1 pass, 1200 dpi
AV630CS | SCSI |  | Complete | 1 pass, 1200 dpi
AV630CSL | SCSI |  | Untested | 1 pass, 1200 dpi
AV6240 | SCSI |  | Complete | 1 pass, ??? dpi
AV600U | USB | 0x0638/0x0a13 | Good | 1 pass, 600 dpi
AV660S | SCSI |  | Untested | 1 pass, ??? dpi
AV680S | SCSI |  | Untested | 1 pass, ??? dpi
AV690U | SCSI |  | Untested | 1 pass, 2400 dpi
AV800S | SCSI |  | Untested | 1 pass, ??? dpi
AV810C | SCSI |  | Untested | 1 pass, ??? dpi
AV820 | SCSI |  | Untested | 1 pass, ??? dpi
AV820C | SCSI |  | Complete | 1 pass, ??? dpi
AV820C Plus | SCSI |  | Complete | 1 pass, ??? dpi
AV830C | SCSI |  | Complete | 1 pass, ??? dpi
AV830C Plus | SCSI |  | Untested | 1 pass, ??? dpi
AV880 | SCSI |  | Untested | 1 pass, ??? dpi
AV880C | SCSI |  | Untested | 1 pass, ??? dpi
AV3200C | SCSI |  | Complete | 1 pass, ??? dpi
AV3200SU | USB | 0x0638/0x0a4e | Complete | 1 pass, ??? dpi
AV3730SU | USB | 0x0638/0x0a4f | Complete | 1 pass, ??? dpi
AV3750SU | USB | 0x0638/0x0a65 | Complete | 1 pass, ??? dpi
AV3800C | SCSI |  | Complete | 1 pass, ??? dpi
AV3850SU | USB | 0x0638/0x0a66 | Complete | 1 pass, ??? dpi
FB6000E | SCSI |  | Complete | 1 pass, 1200 dpi, A3 - duplex! - zero edge!
FB6080E | USB | 0x0638/0x0a82 | Complete | 1 pass, 1200 dpi, A3 - duplex! - zero edge!
FB2080E | USB | 0x0638/0x0a84 | Basic | 1 pass, 600 dpi, zero-edge
AV8000S | SCSI |  | Complete | 1 pass, 1200 dpi, A3
AV8050U | USB | 0x0638/0x0a4d | Complete | 1 pass, 1200 dpi, A3 - duplex!
AV8300 | USB | 0x0638/0x0a40 | Complete | 1 pass, 1200 dpi, A3 - duplex!
AV8350 | USB | 0x0638/0x0a68 | Complete | 1 pass, 1200 dpi, A3 - duplex!
IT8300 | USB | 0x0638/0x0a61 | Good | 1 pass, 1200 dpi, A3 - duplex!, LCD screen, paper sensors
@V2500 | USB | 0x0638/0x0aa1 | Untested |
@V5100 | USB | 0x0638/0x0a45 | Good | 1 pass, 1200 dpi, A3 - duplex!, LCD screen, paper sensors
AVA3 | SCSI |  | Basic | 1 pass, 600 dpi, A3
Hewlett-Packard | ScanJet 5300C | USB | 0x03f0/0x0701 | Complete | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi
ScanJet 5370C | USB | 0x03f0/0x0701 | Good | 1 pass, 2400 dpi - some FW revisions have x-axis image scaling problems over 1200 dpi
ScanJet 7400c | USB | 0x03f0/0x0801 | Good | 1 pass, 2400 dpi - dual USB/SCSI interface
ScanJet 7450c | USB | 0x03f0/0x0801 | Good | 1 pass, 2400 dpi - dual USB/SCSI interface
ScanJet 7490c | USB | 0x03f0/0x0801 | Good | 1 pass, 1200 dpi - dual USB/SCSI interface
ScanJet 8200 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8250 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8270 | USB | 0x03f0/0x3905 | Good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8290 | USB | 0x03f0/0x0b01 | Good | 1 pass, 4800 (?) dpi - USB 2.0 and SCSI - only SCSI tested so far
ScanJet 8300 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8350 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0
ScanJet 8390 | USB | 0x03f0/0x3805 | Good | 1 pass, 4800 (?) dpi - USB 2.0
Minolta | Dimage Scan Dual I | SCSI |  | Basic |
Scan Multi Pro | SCSI |  | Untested |
Dimage Scan Dual II | USB | 0x0638/0x026a | Good | 1 pass, film-scanner
Elite II | USB | 0x0686/0x4004 | Untested | 1 pass, film-scanner
Dimage Scan Dual III | USB | 0x0686/0x400d | Good | 1 pass, film-scanner
Dimage Scan Elite 5400 | USB | 0x0686/0x400e | Good | 1 pass, film-scanner
Minolta-QMS | SC-110 | USB | 0x0638/0x0a15 | Untested |
SC-215 | USB | 0x0638/0x0a16 | Good |
Mitsubishi | MCA-ADFC | SCSI |  | Untested |
S1200C | SCSI |  | Untested |
S600C | SCSI |  | Untested |
SS600 | SCSI |  | Good |
Fujitsu | ScanPartner | SCSI |  | Untested |
ScanPartner 10 | SCSI |  | Untested |
ScanPartner 10C | SCSI |  | Untested |
ScanPartner 15C | SCSI |  | Untested |
ScanPartner 300C | SCSI |  | Untested |
ScanPartner 600C | SCSI |  | Untested |
ScanPartner 620C | SCSI |  | Good |
ScanPartner Jr | SCSI |  | Untested |
ScanStation | SCSI |  | Untested |
fi-4010CU | USB | 0x04c5/0x1029 | Untested |
fi-5015C | USB | 0x04c5/0x10ef | Good |
Kodak | i30 | USB | 0x040a/0x6001 | Untested |
i40 | USB | 0x040a/0x6002 | Basic |
i50 | USB | 0x040a/0x6003 | Untested |
i55 | USB | 0x040a/0x6003 | Untested |
i60 | USB | 0x040a/0x6004 | Untested |
i65 | USB | 0x040a/0x6004 | Untested |
i80 | USB | 0x040a/0x6005 | Good |
iVina | 1200U | USB | 0x0638/0x0268 | Untested |
Visioneer | Strobe XP 450 | USB | 0x04a7/0x0424 | Complete | sheetfed scanner
Strobe XP 450-G | USB | 0x04a7/0x0491 | Complete | sheetfed scanner
Strobe XP 470 | USB | 0x04a7/0x0479 | Complete | sheetfed scanner
Strobe XP 470-G | USB | 0x04a7/0x048f | Complete | sheetfed scanner
9320 | USB | 0x04a7/0x0420 | Complete | sheetfed scanner
9450 | USB | 0x04a7/0x0421 | Complete | sheetfed scanner
9450-G | USB | 0x04a7/0x047a | Complete | sheetfed scanner
9550 | USB | 0x04a7/0x0422 | Complete | sheetfed scanner
9650 | USB | 0x04a7/0x0390 | Complete | sheetfed scanner
9650-G | USB | 0x04a7/0x047b | Complete | sheetfed scanner
9750 | USB | 0x04a7/0x0423 | Complete | sheetfed scanner
9750-G | USB | 0x04a7/0x0493 | Complete | sheetfed scanner
Patriot 430 | USB | 0x04a7/0x0497 | Complete | sheetfed scanner
Patriot 470 | USB | 0x04a7/0x048f | Complete | sheetfed scanner
Patriot 680 | USB | 0x04a7/0x0498 | Complete | sheetfed scanner
Patriot 780 | USB | 0x04a7/0x0499 | Complete | sheetfed scanner
Xerox | DocuMate150 | USB | 0x04a7/0x049c | Good |
DocuMate152 | USB | 0x04a7/0x0477 | Good |
DocuMate162 | USB | 0x04a7/0x049d | Good |
DocuMate250 | USB | 0x04a7/0x0448 | Good |
DocuMate250-G | USB | 0x04a7/0x0490 | Good |
DocuMate252 | USB | 0x04a7/0x0449 | Good |
DocuMate252-G | USB | 0x04a7/0x048c | Good |
DocuMate232 | USB | 0x04a7/0x0476 | Good |
DocuMate262 | USB | 0x04a7/0x044c | Good |
DocuMate262-G | USB | 0x04a7/0x048d | Good |
DocuMate262i | USB | 0x04a7/0x04a7 | Good |
DocuMate272 | USB | 0x04a7/0x0475 | Untested |
DocuMate272-G | USB | 0x04a7/0x048e | Untested |
DocuMate510 | USB | 0x04a7/0x0446 | Untested |
DocuMate512 | USB | 0x04a7/0x0495 | Untested |
DocuMate510-G | USB | 0x04a7/0x047c | Untested |
DocuMate520 | USB | 0x04a7/0x0447 | Untested |
DocuMate520-G | USB | 0x04a7/0x0492 | Untested |
DocuMate632 | USB | 0x04a7/0x0498 | Untested |
DocuMate752 | USB | 0x04a7/0x0478 | Untested |
DocuMate752 | USB | 0x04a7/0x049a | Untested |
OKI | S700 Scancopier | USB | 0x0638/0x0a16 | Good | 1 pass, 600 dpi, A4
Bell+Howell | 2000F | SCSI |  | Basic | 1 pass, ??? dpi, A4
Kyocera | FS-1016MFP | USB | 0x0482/0x0335 | Untested | 1 pass, ??? dpi, A4

### Backend: bh (1.0-4 (unmaintained))

Link(s): http://www.martoneconsulting.com/sane-bh.html
Manual page: sane-bh
Comment: Supports Copiscan II scanners with Remote SCSI Controller (RSC) interface

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Bell and Howell | COPISCAN II 6338 | SCSI |  | Good | Duplex Scanner with ACE - development model
COPISCAN II 2135 | SCSI |  | Untested | Simplex Scanner
COPISCAN II 2137(A) | SCSI |  | Good | Simplex Scanner (with ACE) - limited testing
COPISCAN II 2138A | SCSI |  | Untested | Simplex Scanner with ACE
COPISCAN II 3238 | SCSI |  | Untested | Simplex Scanner
COPISCAN II 3338(A) | SCSI |  | Untested | Simplex Scanner (with ACE)

### Backend: canon (1.12)

Link(s): http://www.rzg.mpg.de/~mpd/sane/
Manual page: sane-canon

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Canon | CanoScan 300 | SCSI |  | Good | 1 pass; flatbed scanner
CanoScan 600 | SCSI |  | Good | 1 pass; flatbed scanner
CanoScan 620S | SCSI |  | Good | 1 pass; flatbed scanner
CanoScan 1200S | SCSI |  | Good | 1 pass; flatbed scanner
CanoScan 2700F | SCSI |  | Good | 1 pass; film scanner
CanoScan 2710S | SCSI |  | Good | 1 pass; 36bit film scanner
IX-4015 | SCSI |  | Good | 1 pass; flatbed scanner
Apple | Color OneScanner 600/27 | SCSI |  | Good | Rebadged CanoScan 300

### Backend: canon630u (0.1 (unmaintained))

Link(s): http://canon-fb630u.sourceforge.net/
Manual page: sane-canon630u

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Canon | CanoScan fb630u | USB | 0x04a9/0x2204 | Good | OK
CanoScan fb636u | USB | 0x04a9/0x2204 | Good | OK

### Backend: canon_dr (51)

Link(s): http://www.thebility.com/canon/
Manual page: sane-canon_dr
Comment: Backend updated for SANE release 1.0.25, see sane-canon_dr manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Canon | CR-25 | USB | 0x1083/0x161a | Untested | Please test!
CR-50 | USB |  | Untested | Please test!
CR-55 | USB | 0x1083/0x160c | Untested | Please test!
CR-80 | USB |  | Untested | Please test!
CR-135i | USB SCSI | 0x1083/0x1639 | Untested | Please test!
CR-180 | USB SCSI | 0x04a9/0x1602 | Untested | Please test!
CR-180II | USB SCSI | 0x04a9/0x1602 | Untested | Same as CR-180? Please test!
CR-190i | USB SCSI | 0x1083/0x162b | Untested | Please test!
DR-1210C | USB | 0x04a9/0x2222 | Untested | Older version? Please test!
DR-1210C | USB | 0x1083/0x160f | Untested | Later version? Please test!
DR-2010C | USB | 0x1083/0x161b | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width, 300/600dpi horizontal. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration, other resolutions.
DR-2010M | USB |  | Complete | DR-2010C with a different label, same USB IDs
DR-2050C | USB | 0x04a9/0x160a | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration.
DR-2050SP | USB | 0x04a9/0x160a | Untested | Same as DR-2050C? Please test!
DR-2080C | USB SCSI | 0x04a9/0x1601 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration
DR-2510C | USB | 0x1083/0x1617 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width, 300/600dpi horizontal. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration, other resolutions
DR-2510M | USB |  | Untested | Mac version of DR-2510C? Please test!
DR-2580C | USB SCSI | 0x04a9/0x1608 | Complete | Hardware provides: Gray/Color, Simplex/Duplex, Full-width. Driver provides: Binary, Despeckle, Deskew, Cropping, Calibration
DR-3010C | USB | 0x1083/0x161d | Good | Minimal testing, settings copied from DR-2510C
DR3020 | SCSI |  | Untested | Please test!
DR-3020C | SCSI |  | Untested | Please test!
DR-3060 | SCSI |  | Untested | Please test!
DR-3080C | SCSI |  | Untested | Almost works, need to investigate traces from windows driver
DR-3080CII | USB SCSI | 0x04a9/0x1609 | Untested | Almost works, need to investigate traces from windows driver
DR-4010C | USB | 0x1083/0x1614 | Good | Binary/HT/Gray/Color, Simplex/Duplex working. Multistream unsupported.
DR4080U | USB |  | Untested | Please test!
DR-4580U | USB |  | Untested | Please test!
DR-5010C | USB | 0x04a9/0x1606 | Basic | ADF and Duplex work, needs more testing
DR-5020 | SCSI |  | Good | LineArt, Duplex working, cannot read buttons or screen?
DR-5060F | SCSI |  | Basic | Grayscale works, LineArt might
DR-5080C | SCSI |  | Untested | Please test!
DR-6010C | USB SCSI | 0x1083/0x1626 | Untested | Please test!
DR-6030C | USB SCSI | 0x1083/0x1638 | Untested | Please test!
DR-6050C | USB SCSI | 0x1083/0x1624 | Good | Simplex, duplex, all resolutions, binary/ht/gray working. Can't wake from stand-by mode
DR-6080 | USB SCSI | 0x04a9/0x1607 | Good | Simplex, duplex, all resolutions, binary/ht/gray, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported
DR-7080C | USB SCSI | 0x04a9/0x1604 | Good | ADF and flatbed work
DR-7090C | USB SCSI | 0x1083/0x1620 | Good | ADF and flatbed work
DR-7550C | USB SCSI | 0x1083/0x1623 | Untested | Assumed compatible with DR-6050C
DR-7580 | USB SCSI | 0x04a9/0x160b | Good | Simplex, duplex, all resolutions, binary/ht/gray, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported
DR-9050C | USB SCSI | 0x1083/0x1622 | Good | Simplex, duplex, all resolutions, binary/ht/gray working. Can't wake from stand-by mode
DR-9080C | USB SCSI | 0x04a9/0x1603 | Good | Simplex, duplex, all resolutions, binary/ht/gray/color, async mode, dropout-color, multifeed/staple detection, deskew, buttons and JPEG working. Imprinter, barcode, custom gamma and multistream unsupported
DR-X10C | USB SCSI | 0x1083/0x1618 | Untested | Please test!
DR-C120 | USB | 0x1083/0x1651 | Untested |
DR-C125 | USB | 0x1083/0x1640 | Good |
DR-C130 | USB | 0x1083/0x164a | Untested |
DR-C225 | USB | 0x1083/0x1658 | Untested |
DR-F120 | USB | 0x1083/0x1654 | Basic | Flatbed not working. ADF working. Simplex+duplex, all resolutions <= 600, gray/color, calibration poor.
DR-G1100 | USB | 0x1083/0x1650 | Good |
DR-G1130 | USB | 0x1083/0x164f | Untested |
DR-M140 | USB | 0x1083/0x163f | Good |
DR-M160 | USB | 0x1083/0x163e | Good |
DR-M160II | USB |  | Untested |
DR-M1060 | USB | 0x1083/0x1657 | Untested |
P-150 | USB |  | Untested | Same as P-150M?
P-150M | USB | 0x1083/0x162c | Good |
P-201 | USB | 0x1083/0x1652 | Untested |
DR-P208 | USB | 0x1083/0x164b | Untested | Same as P-208?
P-208 | USB | 0x1083/0x164c | Basic | All modes and resolutions working, but calibration is poor.
P-208 | USB | 0x1083/0x164e | Basic | This is the same device as the 0x164c P-208, but the mode switch on the scanner is in the wrong position, you must move the switch.
DR-P208II | USB | 0x1083/0x165d | Untested |
P-208II | USB | 0x1083/0x165f | Untested |
DR-P215 | USB | 0x1083/0x1641 | Untested | Same as P-215?
P-215 | USB | 0x1083/0x1646 | Basic | All modes and resolutions working, but calibration is poor. Card reader slot not working.
P-215 | USB | 0x1083/0x1647 | Basic | This is the same device as the 0x1646 P-215, but the mode switch on the scanner is in the wrong position, you must move the switch.
DR-P215II | USB | 0x1083/0x1659 | Untested |
P-215II | USB | 0x1083/0x165b | Untested |
FSU-201 | USB | 0x1083/0x1648 | Untested |

### Backend: canon_pp (0.33 (unmaintained))

Link(s): http://canon-fb330p.sourceforge.net
Manual page: sane-canon_pp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Canon | CanoScan FB310P | Parport (ECP) |  | Unsupported | Rebadged Avision, different command set
CanoScan FB610P | Parport (ECP) |  | Unsupported | Rebadged Avision, different command set
CanoScan FB320P | Parport (ECP) |  | Basic | Newly added support
CanoScan FB620P | Parport (ECP) |  | Basic | Newly added support
CanoScan FB330P | Parport (ECP) |  | Good |
CanoScan FB630P | Parport (ECP) |  | Good |
CanoScan N340P | Parport (ECP) |  | Good |
CanoScan N640P | Parport (ECP) |  | Good |
CanoScan N640P ex | Parport (ECP) |  | Good | Just an N640P in a different box?

### Backend: cardscan (3)

Link(s): http://www.thebility.com/cardscan/
Manual page: sane-cardscan
Comment: Backend updated for SANE release 1.0.21, see sane-cardscan manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Corex/Dymo | 800c | USB | 0x08f0/0x0005 | Good | 4 inch wide 8bit Gray or 24bit Color simplex card/receipt scanner
600c | USB | 0x08f0/0x0002 | Basic | 4 inch wide 8bit Gray or 24bit Color simplex card/receipt scanner
Sanford | 800c | USB | 0x0451/0x6250 | Good | 4 inch wide 8bit Gray or 24bit Color simplex card/receipt scanner

### Backend: coolscan (0.4.3 (unmaintained))

Link(s): http://andreas.rick.free.fr/sane/
Manual page: sane-coolscan

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Nikon | LS-20 | SCSI |  | Basic | The LS-20 has been replaced by the LS-30
LS-30 | SCSI |  | Basic | alpha: only 24/30 bit RGB + 32/40 bit RGBI
LS-2000 | SCSI |  | Basic | alpha: only 24/36 bit + RGB 32/48 bit RGBI
LS-1000 | SCSI |  | Basic | Doesn't support gamma correction

### Backend: coolscan2 (0.1.8 (unmaintained))

Link(s): http://coolscan2.sourceforge.net/
Manual page: sane-coolscan2

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Nikon | LS 30 | SCSI |  | Complete | working -- model available to developer
LS 2000 | SCSI |  | Good |
LS 40 ED | USB | 0x04b0/0x4000 | Complete |
LS 4000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later
LS 50 ED | USB | 0x04b0/0x4001 | Minimal |
Coolscan V ED | USB | 0x04b0/0x4001 | Minimal |
Super Coolscan LS-5000 ED | USB | 0x04b0/0x4002 | Untested | May work, similar to LS 50 ED, but untested. Please tell us if it works.
LS 8000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later

### Backend: coolscan3 (1.0.0 (unmaintained))

Manual page: sane-coolscan3

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Nikon | LS 30 | SCSI |  | Complete |
Coolscan III | SCSI |  | Complete | Rebadged LS 30?
LS 40 ED | USB | 0x04b0/0x4000 | Complete |
Coolspan IV | USB | 0x04b0/0x4000 | Complete | Rebadged LS 40?
LS 50 ED | USB | 0x04b0/0x4001 | Minimal |
Coolscan V ED | USB | 0x04b0/0x4001 | Minimal | Rebadged LS 50?
LS 2000 | SCSI |  | Good |
LS 4000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later
Super Coolscan LS-5000 ED | USB | 0x04b0/0x4002 | Untested | May work, similar to LS 50 ED, but untested. Please tell us if it works.
LS 8000 ED | IEEE-1394 |  | Good | needs linux kernel 2.4.19 or later

### Backend: dell1600n_net (unmaintained)

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Dell | 1600n | Ethernet USB | 0x413c/0x5250 | Basic | Supports colour and monochrome scans over ethernet (USB not supported)

### Backend: epjitsu (31)

Manual page: sane-epjitsu
Comment: Backend updated for SANE release 1.0.26, see sane-epjitsu manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Fujitsu | fi-60F | USB | 0x04c5/0x10c7 | Good | A6-size flatbed. Hardware provides 150/200/300/400/600 dpi in color. Software creates other resolutions, plus grayscale and binary modes. Hardware grayscale mode is not used due to poor calibration.
ScanSnap S300 | USB | 0x04c5/0x1156 | Good | Letter-size ADF. Hardware provides duplex, 150/225/300/600 dpi in color on AC or USB power. Software creates other resolutions, plus grayscale and binary modes. All buttons and sensors are exposed. Scanner always scans in _triplex_ color, fast USB required.
ScanSnap S300M | USB | 0x04c5/0x117f | Good | Same as S300, with different usb id
fi-65F | USB | 0x04c5/0x11bd | Good | Same as fi-60f, with different usb id. Button support untested.
ScanSnap S1300 | USB | 0x04c5/0x11ed | Good | Same as S300, with different usb id
ScanSnap S1100 | USB | 0x04c5/0x1200 | Good | Letter-size ADF. Hardware provides simplex, 300/600 dpi in color on USB power. Software creates other resolutions, plus grayscale and binary modes. All buttons and sensors are exposed. Scanner always scans in _triplex_ color, fast USB required.
ScanSnap S1300i | USB | 0x04c5/0x128d | Good | Same as S300, with different usb id
ScanSnap S1100i | USB | 0x04c5/0x1447 | Good | Same as S1100, with different usb id

### Backend: epson (0.2.42 (unmaintained))

Link(s): http://www.khk.net/sane
Manual page: sane-epson

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Epson | GT-5000 | SCSI Parport |  | Good |
Actionscanner II | SCSI Parport |  | Good | US version of GT-5000
GT-6000 | SCSI Parport |  | Good |
ES-300C | SCSI Parport |  | Good | US version of GT-6000
ES-300GS | SCSI |  | Good |
GT-5500 | SCSI |  | Good |
GT-6500 | Parport |  | Good |
ES-600C | Parport |  | Good | US version of GT-6500
ES-1200C | Parport |  | Good | US version of GT-9000
GT-7000 | SCSI |  | Good |
GT-8000 | SCSI |  | Good |
ES-8500 | SCSI |  | Good |
Perfection 636S | SCSI |  | Complete | US version of GT-7000
Perfection 636 | SCSI |  | Complete |
Perfection 636U | USB | 0x04b8/0x0101 | Complete |
Perfection 610 | USB | 0x04b8/0x0103 | Complete |
Perfection 640 | USB | 0x04b8/0x010c | Complete |
Perfection 1200S | SCSI |  | Complete |
Perfection 1200U | USB | 0x04b8/0x0104 | Complete |
Perfection 1200Photo | USB | 0x04b8/0x0104 | Complete | with TPU
Perfection 1240 | SCSI USB | 0x04b8/0x010b | Complete |
Perfection 1640 | SCSI USB | 0x04b8/0x010a | Complete |
Perfection 1650 | USB | 0x04b8/0x0110 | Complete |
Perfection 1660 | USB | 0x04b8/0x011e | Complete |
Perfection 2400 | USB | 0x04b8/0x011b | Complete |
Perfection 2450 | USB IEEE-1394 | 0x04b8/0x0112 | Complete |
Perfection 3200 | USB IEEE-1394 | 0x04b8/0x011c | Complete | US version of the GT-9800
Perfection 4870 | USB | 0x04b8/0x0128 | Complete | US version of the GT-X700
Perfection 4990 | USB | 0x04b8/0x012a | Complete | US version of the GT-X800
Expression 636 | SCSI |  | Complete | US version of GT-9500
Expression 800 | SCSI |  | Complete |
Expression 1600 | SCSI USB IEEE-1394 | 0x04b8/0x0107 | Complete |
Expression 1680 | SCSI USB IEEE-1394 | 0x04b8/0x010e | Complete |
FilmScan 200 | SCSI |  | Unsupported |
CX-3200 | USB | 0x04b8/0x0802 | Good |
CX-3600 | USB | 0x04b8/0x080e | Good |
CX-3650 | USB | 0x04b8/0x080e | Good |
CX-4600 | USB | 0x04b8/0x080d | Good |
CX-4800 | USB | 0x04b8/0x0819 | Good |
CX-5000 | USB | 0x04b8/0x082b | Good |
CX-5200 | USB | 0x04b8/0x0801 | Good |
CX-5400 | USB | 0x04b8/0x0801 | Good |
CX-5400 | USB | 0x04b8/0x0808 | Good |
CX-6300 | USB | 0x04b8/0x0805 | Good |
CX-6400 | USB | 0x04b8/0x0805 | Good |
CX-6500 | USB | 0x04b8/0x0813 | Good |
CX-6600 | USB | 0x04b8/0x0813 | Good |
RX-500 | USB | 0x04b8/0x0807 | Good |
RX-600 | USB | 0x04b8/0x0806 | Good |
RX-425 | USB | 0x04b8/0x080f | Good |
RX-700 | USB | 0x04b8/0x0810 | Good |
RX-620 | USB | 0x04b8/0x0811 | Good |
DX-3850 | USB | 0x04b8/0x0818 | Good |
CX-3700 | USB | 0x04b8/0x0818 | Good |
CX-3800 | USB | 0x04b8/0x0818 | Good |
CX-4200 | USB | 0x04b8/0x0820 | Good |
DX-3800 | USB | 0x04b8/0x0818 | Good |
DX-5000 | USB | 0x04b8/0x082b | Good |
DX-5050 | USB | 0x04b8/0x082b | Good |
DX-6000 | USB | 0x04b8/0x082e | Good |
DX-7400 | USB | 0x04b8/0x0838 | Good |
DX-4050 | USB | 0x04b8/0x082f | Good |
AcuLaser CX11 | USB | 0x04b8/0x0815 | Good |
AcuLaser CX11NF | USB | 0x04b8/0x0815 | Good |
V700 | USB IEEE-1394 | 0x04b8/0x012c | Good |
V750 | USB IEEE-1394 | 0x04b8/0x012c | Good |

### Backend: epson2 (1.0.124 (unmaintained))

Manual page: sane-epson2

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Epson | AL-MX300DN Series | USB | 0x04b8/0x08ac | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
AL-MX300DNF Series | USB | 0x04b8/0x08ac | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Actionscanner II | parallel SCSI |  | Good | overseas version of the GT-5000
AcuLaser CX11 | USB | 0x04b8/0x0815 | Good | overseas version of the LP-A500
AcuLaser CX11NF | USB Network | 0x04b8/0x0815 | Good | network interface supported AcuLaser CX11 with network interface and fax
AcuLaser CX21 | USB Network | 0x04b8/0x0835 | Good | network interface supported
AcuLaser MX20DN | USB | 0x04b8/0x0866 | Complete | network interface probably supported business all-in-one
AcuLaser MX20DNF | USB | 0x04b8/0x0866 | Complete | network interface probably supported business all-in-one
AcuLaser MX21DNF | USB | 0x04b8/0x0866 | Complete | network interface probably supported business all-in-one
Artisan 635 | USB | 0x04b8/0x0878 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-704A
Artisan 700 | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one overseas version of the EP-801A
Artisan 710 Series | USB | 0x04b8/0x0852 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-802A
Artisan 725 | USB | 0x04b8/0x0861 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-803A
Artisan 730 Series | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-804A
Artisan 800 | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A
Artisan 810 Series | USB | 0x04b8/0x0853 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-902A
Artisan 835 | USB | 0x04b8/0x0860 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-903A
Artisan 837 | USB | 0x04b8/0x0879 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-904F
CC-500L | USB | 0x04b8/0x010d | Unsupported | all-in-one
CC-550L | USB | 0x04b8/0x011a | Unsupported | all-in-one
CC-570L | USB | 0x04b8/0x0802 | Good | all-in-one
CC-600PX | USB | 0x04b8/0x0801 | Good | all-in-one
CC-700 | USB | 0x04b8/0x0108 | Unsupported | all-in-one
DS-30 | USB | 0x04b8/0x0147 | Unsupported | supported by the epkowa backend plus non-free interpreter
EP-702A | USB | 0x04b8/0x0850 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-703A | USB | 0x04b8/0x0862 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-704A | USB | 0x04b8/0x0878 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-705A | USB | 0x04b8/0x089f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-706A | USB | 0x04b8/0x08b7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-707A | USB | 0x04b8/0x08c9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-774A | USB | 0x04b8/0x0893 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-775A | USB | 0x04b8/0x089e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-775AW | USB | 0x04b8/0x089e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-776AB | USB | 0x04b8/0x08b6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-776AW | USB | 0x04b8/0x08b6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-777A | USB | 0x04b8/0x08c8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-801A | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one
EP-802A | USB | 0x04b8/0x0852 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-803A | USB | 0x04b8/0x0861 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-803AW | USB | 0x04b8/0x0861 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-804A | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-804AR | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-804AW | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-805A | USB | 0x04b8/0x089c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-805AR | USB | 0x04b8/0x089c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-805AW | USB | 0x04b8/0x089c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-806AB | USB | 0x04b8/0x08b5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-806AR | USB | 0x04b8/0x08b5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-806AW | USB | 0x04b8/0x08b5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-807AB | USB | 0x04b8/0x08c7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-807AR | USB | 0x04b8/0x08c7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-807AW | USB | 0x04b8/0x08c7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-901A | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one
EP-901F | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one
EP-902A | USB | 0x04b8/0x0853 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-903A | USB | 0x04b8/0x0860 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-903F | USB | 0x04b8/0x0860 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-904A | USB | 0x04b8/0x0879 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-904F | USB | 0x04b8/0x0879 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-905A | USB | 0x04b8/0x089b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-905F | USB | 0x04b8/0x089a | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-906F | USB | 0x04b8/0x08b4 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-907F | USB | 0x04b8/0x08c6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-976A3 | USB | 0x04b8/0x08b3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
EP-977A3 | USB | 0x04b8/0x08c5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ES-300C | SCSI parallel |  | Good | overseas version of the GT-6000
ES-300GS | SCSI |  | Good |
ES-600C | parallel |  | Good | overseas version of the GT-5400
ES-800C | SCSI |  | Good | overseas version of the GT-8000
ES-1000C | ? |  | Unsupported | overseas version of the GT-8500
ES-1200C | parallel |  | Good | overseas version of the GT-9000
ES-2000 | SCSI USB | 0x04b8/0x0107 | Complete | IEEE1394 untested
ES-2200 | SCSI USB | 0x04b8/0x010e | Complete | IEEE1394 untested
ES-6000 | SCSI |  | Good |
ES-6000H | SCSI |  | Good | IEEE1394 untested
ES-6000HS | SCSI |  | Good | IEEE1394 untested
ES-7000H | SCSI USB | 0x04b8/0x0126 | Good | network interface probably supported IEEE1394 untested
ES-8000 | SCSI |  | Untested |
ES-8500 | SCSI USB | 0x04b8/0x0109 | Good | IEEE1394 untested
ES-9000H | SCSI |  | Good | IEEE1394 untested
ES-10000G | USB | 0x04b8/0x0129 | Good | network interface probably supported IEEE1394 untested
ES-D200 | USB | 0x04b8/0x0137 | Unsupported | supported by the epkowa backend plus non-free interpreter
ES-D350 | USB | 0x04b8/0x0144 | Unsupported | supported by the epkowa backend plus non-free interpreter
ES-D400 | USB | 0x04b8/0x0136 | Unsupported | supported by the epkowa backend plus non-free interpreter
ES-G11000 | USB | 0x04b8/0x014b | Good |
ES-H300 | USB | 0x04b8/0x012b | Good | network interface probably supported
ES-H7200 | USB Ethernet | 0x04b8/0x0138 | Good | network interface supported via DFSG non-free iscan-network-nt package
Expression 636 | SCSI |  | Complete | overseas version of the GT-9500
Expression 800 | SCSI |  | Complete | overseas version of the GT-9600
Expression 836XL | SCSI |  | Untested | overseas version of the ES-8000
Expression 1600 | SCSI USB | 0x04b8/0x0107 | Complete | IEEE1394 untested overseas version of the ES-2000
Expression 1640XL | SCSI USB | 0x04b8/0x0109 | Good | IEEE1394 untested overseas version of the ES-8500
Expression 1680 | SCSI USB | 0x04b8/0x010e | Complete | IEEE1394 untested overseas version of the ES-2200
Expression 1680 Pro | SCSI USB |  | Untested | IEEE1394 option
Expression 1680XL Pro | SCSI USB |  | Untested |
Expression 10000XL | USB | 0x04b8/0x0129 | Good | network interface probably supported IEEE1394 untested overseas version of the ES-10000G
Expression 10000XL Graphic Arts | USB IEEE1394 |  | Untested | network interface probably supported
Expression 10000XL Photo | USB IEEE1394 |  | Untested | network interface probably supported
Expression 11000XL | USB | 0x04b8/0x014b | Good | overseas version of the ES-G11000
F-3200 | USB IEEE1394 | 0x04b8/0x080a | Unsupported | Film scanner
F-3200 Photo | USB IEEE1394 |  | Unsupported |
FilmScan 200 | SCSI |  | Minimal | missing documentation
GT-1500 | USB | 0x04b8/0x0133 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-2200 | USB | 0x04b8/0x0102 | Unsupported |
GT-2500 | USB | 0x04b8/0x012b | Good | network interface probably supported overseas version of the ES-H300
GT-4000 | ? |  | Untested |
GT-5000 | parallel SCSI |  | Good |
GT-5400 | parallel |  | Good |
GT-5500 | SCSI |  | Good |
GT-6000 | SCSI Parport |  | Good |
GT-6500 | parallel |  | Good | overseas version of the GT-5400
GT-6600U | USB | 0x04b8/0x0103 | Complete |
GT-6700U | USB | 0x04b8/0x010c | Complete |
GT-7000S | SCSI |  | Complete |
GT-7000U | USB | 0x04b8/0x0101 | Complete |
GT-7200U | USB | 0x04b8/0x010f | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-7300U | USB | 0x04b8/0x011d | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-7400U | USB | 0x04b8/0x0120 | Unsupported | supported by the snapscan backend
GT-7600S | SCSI |  | Complete | SCSI version of the GT-7600U
GT-7600U | USB | 0x04b8/0x0104 | Complete | USB version of the GT-7600S
GT-7600UF | USB | 0x04b8/0x0104 | Complete | GT-7600U with TPU option bundled
GT-7700U | USB | 0x04b8/0x010b | Complete |
GT-8000 | SCSI |  | Good |
GT-8200U | USB | 0x04b8/0x0110 | Complete |
GT-8200UF | USB | 0x04b8/0x0110 | Good |
GT-8300UF | USB | 0x04b8/0x011e | Complete |
GT-8400UF | USB | 0x04b8/0x011f | Unsupported |
GT-8500 | ? |  | Untested |
GT-8700 | SCSI USB | 0x04b8/0x010a | Complete |
GT-8700F | SCSI USB | 0x04b8/0x010a | Good | GT-8700U with TPU option bundled
GT-9000 | parallel |  | Good |
GT-9300UF | USB | 0x04b8/0x011b | Complete |
GT-9400UF | USB | 0x04b8/0x0116 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-9500 | SCSI |  | Complete |
GT-9600 | SCSI |  | Complete |
GT-9700F | USB IEEE1394 | 0x04b8/0x0112 | Complete |
GT-9800F | USB IEEE1394 | 0x04b8/0x011c | Complete |
GT-10000 | SCSI |  | Good | overseas version of the ES-6000
GT-10000+ | SCSI |  | Good | IEEE1394 untested overseas version of the ES-6000H
GT-12000 | SCSI |  | Untested | overseas version of the ES-8000
GT-15000 | SCSI USB | 0x04b8/0x0126 | Good | IEEE1394 untested overseas version of the ES-7000H
GT-20000 | USB Ethernet | 0x04b8/0x0138 | Good | network interface supported via DFSG non-free iscan-network-nt package overseas version of the ES-H7200
GT-30000 | SCSI |  | Good | IEEE1394 untested overseas version of the ES-9000H
GT-D1000 | USB | 0x04b8/0x0133 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F500 | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F520 | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F550 | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F570 | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F600 | USB | 0x04b8/0x0118 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F650 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F670 | USB | 0x04b8/0x012e | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F700 | USB | 0x04b8/0x012f | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F720 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F730 | USB | 0x04b8/0x0142 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-F740 | USB | 0x04b8/0x014a | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S50 | USB | 0x04b8/0x0137 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S55 | USB | 0x04b8/0x0143 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S80 | USB | 0x04b8/0x0136 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S85 | USB | 0x04b8/0x0144 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S600 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S620 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S630 | USB | 0x04b8/0x0142 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S640 | USB | 0x04b8/0x014a | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-S650 | USB | 0x04b8/0x013d | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-X700 | USB | 0x04b8/0x0128 | Complete | IEEE1394 untested
GT-X750 | USB | 0x04b8/0x0119 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-X770 | USB | 0x04b8/0x0130 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-X800 | USB | 0x04b8/0x012a | Complete | film area guide mode not supported IEEE1394 untested
GT-X820 | USB | 0x04b8/0x013a | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-X830 | USB | 0x04b8/0x0153 | Unsupported | supported by the epkowa backend plus non-free interpreter
GT-X900 | USB | 0x04b8/0x012c | Good | IEEE1394 untested
GT-X970 | USB | 0x04b8/0x0135 | Good | IEEE1394 untested
GT-X980 | USB | 0x04b8/0x0151 | Good |
K200 Series | USB | 0x04b8/0x0871 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
K300 Series | USB | 0x04b8/0x0872 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
L200 Series | USB | 0x04b8/0x0873 | Complete | all-in-one
L210 Series | USB | 0x04b8/0x08a1 | Complete | all-in-one
L350 | USB | 0x04b8/0x08a1 | Complete | all-in-one
L351 | USB | 0x04b8/0x08a1 | Complete | all-in-one
L355 | USB | 0x04b8/0x08a8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
L358 | USB | 0x04b8/0x08a8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
L550 Series | USB | 0x04b8/0x08a9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
L850 Series | USB | 0x04b8/0x08ca | Complete | all-in-one
LP-7900CS | ? |  | Untested | business all-in-one; scanner is a ES-7000H
LP-9000CCH | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-9000CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H
LP-9000CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-9500CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H
LP-9500CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-9500CH2 | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-9800CCH | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-9800CCS | ? |  | Untested | business all-in-one; scanner is a ES-7000H
LP-9800CFH | ? |  | Untested | business all-in-one; scanner is a ES-9000H
LP-A500 | USB Network | 0x04b8/0x0815 | Good | network interface supported business all-in-one
LP-M5000 | USB | 0x04b8/0x0843 | Good | network interface probably supported business all-in-one
LP-M5300 Series | USB | 0x04b8/0x0894 | Good | network interface probably supported business all-in-one
LP-M5500 | USB | 0x04b8/0x0817 | Good | network interface probably supported business all-in-one
LP-M5500F | USB | 0x04b8/0x0817 | Good | network interface probably supported business all-in-one LP-M5500 with the fax option bundled
LP-M5600 | USB | 0x04b8/0x0833 | Good | network interface probably supported business all-in-one
LP-M6000 | USB | 0x04b8/0x0834 | Good | network interface probably supported business all-in-one
LP-M8040 | USB | 0x04b8/0x08ad | Good | network interface probably supported business all-in-one
LP-M8040A | USB | 0x04b8/0x08ad | Good | network interface probably supported business all-in-one
LP-M8040F | USB | 0x04b8/0x08ad | Good | network interface probably supported business all-in-one
M200 Series | USB | 0x04b8/0x08aa | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME 200 | USB | 0x04b8/0x0830 | Good | all-in-one
ME 300 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A
ME 320 Series | USB | 0x04b8/0x085c | Complete | all-in-one
ME 330 Series | USB | 0x04b8/0x085c | Complete | all-in-one
ME 340 Series | USB | 0x04b8/0x0883 | Complete | all-in-one
ME OFFICE 510 | USB | 0x04b8/0x084f | Good | all-in-one
ME OFFICE 520 Series | USB | 0x04b8/0x0865 | Complete | all-in-one
ME OFFICE 535 | USB | 0x04b8/0x0881 | Complete | all-in-one overseas version of the PX-404A
ME OFFICE 560W Series | USB | 0x04b8/0x0864 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME OFFICE 570W Series | USB | 0x04b8/0x0880 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-434A
ME Office 600F | USB | 0x04b8/0x0848 | Good | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME OFFICE 620F Series | USB | 0x04b8/0x0863 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME OFFICE 650FN Series | USB | 0x04b8/0x0854 | Good | all-in-one
ME Office 700FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F
ME OFFICE 900WD Series | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
ME OFFICE 940FW Series | USB | 0x04b8/0x0890 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME OFFICE 960FWD Series | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME-101 | USB | 0x04b8/0x08a0 | Complete | all-in-one
ME-301 | USB | 0x04b8/0x0896 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
ME-303 | USB | 0x04b8/0x0897 | Complete | all-in-one overseas version of the PX-405A
ME-401 | USB | 0x04b8/0x0898 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-435A
PM-A700 | USB | 0x04b8/0x0814 | Good | all-in-one
PM-A750 | USB | 0x04b8/0x081a | Good | all-in-one
PM-A820 | USB | 0x04b8/0x0827 | Good | all-in-one
PM-A840 | USB | 0x04b8/0x083c | Good | all-in-one
PM-A840S | USB | 0x04b8/0x083c | Good | network interface probably supported all-in-one
PM-A850 | USB | 0x04b8/0x0806 | Good | all-in-one
PM-A870 | USB | 0x04b8/0x0811 | Good | all-in-one
PM-A890 | USB | 0x04b8/0x081c | Good | all-in-one
PM-A900 | USB | 0x04b8/0x0810 | Good | all-in-one
PM-A920 | USB | 0x04b8/0x082a | Good | all-in-one
PM-A940 | USB | 0x04b8/0x0837 | Good | all-in-one
PM-A950 | USB | 0x04b8/0x081d | Good | all-in-one
PM-A970 | USB | 0x04b8/0x0828 | Good | all-in-one
PM-T960 | USB | 0x04b8/0x0836 | Good | all-in-one
PM-T990 | USB | 0x04b8/0x0829 | Good | all-in-one PM-A970 with network interface
PX-045A | USB | 0x04b8/0x0895 | Complete | all-in-one
PX-046A | USB | 0x04b8/0x08ae | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-047A | USB | 0x04b8/0x08c0 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-1600F | USB | 0x04b8/0x0869 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-1700F | USB | 0x04b8/0x087c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-401A | USB | 0x04b8/0x0841 | Good | all-in-one
PX-402A | USB | 0x04b8/0x084d | Good | all-in-one
PX-403A | USB | 0x04b8/0x087f | Complete | all-in-one
PX-404A | USB | 0x04b8/0x0881 | Complete | all-in-one
PX-405A | USB | 0x04b8/0x0897 | Complete | all-in-one
PX-434A | USB | 0x04b8/0x0880 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-435A | USB | 0x04b8/0x0898 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-436A | USB | 0x04b8/0x08af | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-437A | USB | 0x04b8/0x08bf | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-501A | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one
PX-502A | USB | 0x04b8/0x0856 | Good | all-in-one
PX-503A | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-504A | USB | 0x04b8/0x0891 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-505F | USB | 0x04b8/0x08a5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-535F | USB | 0x04b8/0x08a6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-601F | USB | 0x04b8/0x0847 | Good | network interface probably supported
PX-602F | USB | 0x04b8/0x0855 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-603F | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-605F | USB | 0x04b8/0x0899 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-673F | USB | 0x04b8/0x086a | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-675F | USB | 0x04b8/0x0899 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-A550 | USB | 0x04b8/0x080e | Good | all-in-one
PX-A620 | USB | 0x04b8/0x082f | Good | all-in-one
PX-A640 | USB | 0x04b8/0x0838 | Good | all-in-one
PX-A650 | USB | 0x04b8/0x0819 | Good | all-in-one
PX-A720 | USB | 0x04b8/0x082e | Good | all-in-one
PX-A740 | USB | 0x04b8/0x0839 | Good | all-in-one
PX-B750F | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-FA700 | USB | 0x04b8/0x083a | Good | all-in-one
PX-M350F | USB | 0x04b8/0x08d0 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M5040F | USB | 0x04b8/0x08b9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M5041F | USB | 0x04b8/0x08b9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M650A | USB | 0x04b8/0x08c3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M650F | USB | 0x04b8/0x08c3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M740F | USB | 0x04b8/0x08b8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M741F | USB | 0x04b8/0x08b8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
PX-M840F | USB | 0x04b8/0x08bd | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Perfection 600 | SCSI |  | Unsupported | supported by the umax backend rebadged UMAX Astra 1200S
Perfection 610 | USB | 0x04b8/0x0103 | Basic | overseas version of the GT-6600U
Perfection 636S | SCSI |  | Complete | overseas version of the GT-7000S
Perfection 636U | USB | 0x04b8/0x0101 | Complete | overseas version of the GT-7000U
Perfection 640U | USB | 0x04b8/0x010c | Complete | overseas version of the GT-6700U
Perfection 660 | USB | 0x04b8/0x0114 | Unsupported | supported by the snapscan backend
Perfection 1200S | SCSI |  | Complete | overseas version of the GT-7600S
Perfection 1200U | USB | 0x04b8/0x0104 | Complete | overseas version of the GT-7600U
Perfection 1200U PHOTO | USB | 0x04b8/0x0104 | Complete | Perfection 1200U with TPU option bundled overseas version of the GT-7600UF
Perfection 1240U | USB | 0x04b8/0x010b | Complete | overseas version of the GT-7700U
Perfection 1250 | USB | 0x04b8/0x010f | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 1250 PHOTO | USB | 0x04b8/0x010f | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 1260 | USB | 0x04b8/0x011d | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 1260 PHOTO | USB | 0x04b8/0x011d | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 1270 | USB | 0x04b8/0x0120 | Unsupported | supported by the snapscan backend overseas version of the GT-7400
Perfection 1600 | SCSI |  | Unsupported |
Perfection 1640SU | SCSI USB | 0x04b8/0x010a | Complete | overseas version of the GT-8700
Perfection 1640SU PHOTO | SCSI USB | 0x04b8/0x010a | Good | overseas version of the GT-8700F
Perfection 1650 | USB | 0x04b8/0x0110 | Complete | overseas version of the GT-8200U
Perfection 1650 PHOTO | USB | 0x04b8/0x0110 | Good | overseas version of the GT-8200UF
Perfection 1660 PHOTO | USB | 0x04b8/0x011e | Complete | overseas version of the GT-8300UF
Perfection 1670 | USB | 0x04b8/0x011f | Unsupported | supported by the snapscan backend
Perfection 1670 PHOTO | USB | 0x04b8/0x011f | Unsupported | supported by the snapscan backend overseas version of the GT-8400UF
Perfection 2400 PHOTO | USB | 0x04b8/0x011b | Complete | overseas version of the GT-9300UF
Perfection 2450 PHOTO | USB IEEE1394 | 0x04b8/0x0112 | Complete | overseas version of the GT-9700F
Perfection 2480 PHOTO | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 2580 PHOTO | USB | 0x04b8/0x0121 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 3170 PHOTO | USB | 0x04b8/0x0116 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 3200 PHOTO | USB IEEE1394 | 0x04b8/0x011c | Complete | overseas version of the GT-9800F
Perfection 3490 PHOTO | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 3590 PHOTO | USB | 0x04b8/0x0122 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 4180 PHOTO | USB | 0x04b8/0x0118 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 4490 PHOTO | USB | 0x04b8/0x0119 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection 4870 PHOTO | USB | 0x04b8/0x0128 | Complete | IEEE1394 untested overseas version of the GT-X700
Perfection 4990 PHOTO | USB | 0x04b8/0x012a | Good | film area guide mode not supported IEEE1394 untested overseas version of the GT-X800
Perfection 4990 Pro | USB IEEE1394 |  | Untested | seems to be a 4990 PHOTO with additional software
Perfection V10 | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V19 | USB | 0x04b8/0x013c | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V30 | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V33 | USB | 0x04b8/0x0142 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V37 | USB | 0x04b8/0x014a | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V39 | USB | 0x04b8/0x013d | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V100 Photo | USB | 0x04b8/0x012d | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V200 Photo | USB | 0x04b8/0x012e | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V300 Photo | USB | 0x04b8/0x0131 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V330 Photo | USB | 0x04b8/0x0142 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V370 Photo | USB | 0x04b8/0x014a | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V350 Photo | USB | 0x04b8/0x012f | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V500 Photo | USB | 0x04b8/0x0130 | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V550 Photo | USB | 0x04b8/0x013b | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V600 Photo | USB | 0x04b8/0x013a | Unsupported | supported by the epkowa backend plus non-free interpreter
Perfection V700 Photo | USB | 0x04b8/0x012c | Good | IEEE1394 untested overseas version of the GT-X900
Perfection V750 Photo | USB | 0x04b8/0x012c | Good | IEEE1394 untested overseas version of the GT-X900
Perfection V800 Photo | USB | 0x04b8/0x0151 | Good |
Perfection V850 Pro | USB | 0x04b8/0x0151 | Good | overseas version of the GT-X980
Stylus CX1500 | USB | 0x04b8/0x080c | Unsupported | supported by the snapscan backend all-in-one
Stylus CX2800 | USB | 0x04b8/0x0830 | Good | all-in-one
Stylus CX2900 | USB | 0x04b8/0x0830 | Good | all-in-one
Stylus CX3100 | USB | 0x04b8/0x0802 | Good | all-in-one overseas version of the CC-570L
Stylus CX3200 | USB | 0x04b8/0x0802 | Good | all-in-one overseas version of the CC-570L
Stylus CX3500 | USB | 0x04b8/0x080e | Good | all-in-one overseas version of the PX-A550
Stylus CX3600 | USB | 0x04b8/0x080e | Good | all-in-one overseas version of the PX-A550
Stylus CX3650 | USB | 0x04b8/0x080e | Good | all-in-one
Stylus CX3700 | USB | 0x04b8/0x0818 | Good | all-in-one
Stylus CX3800 | USB | 0x04b8/0x0818 | Good | all-in-one
Stylus CX3810 | USB | 0x04b8/0x0818 | Good | all-in-one
Stylus CX3900 | USB | 0x04b8/0x082f | Good | all-in-one overseas version of the PX-A620
Stylus CX4100 | USB | 0x04b8/0x0820 | Good | all-in-one
Stylus CX4200 | USB | 0x04b8/0x0820 | Good | all-in-one
Stylus CX4300 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter
Stylus CX4400 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter
Stylus CX4500 | USB | 0x04b8/0x080d | Good | all-in-one
Stylus CX4600 | USB | 0x04b8/0x080d | Good | all-in-one
Stylus CX4700 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650
Stylus CX4800 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650
Stylus CX4900 | USB | 0x04b8/0x082b | Good | all-in-one
Stylus CX5000 | USB | 0x04b8/0x082b | Good | all-in-one
Stylus CX5100 | USB | 0x04b8/0x0801 | Good | all-in-one overseas version of the CC-600PX
Stylus CX5200 | USB | 0x04b8/0x0801 | Good | all-in-one overseas version of the CC-600PX
Stylus CX5300 | USB | 0x04b8/0x0808 | Good | all-in-one
Stylus CX5400 | USB | 0x04b8/0x0808 | Good | all-in-one
Stylus CX5500 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter
Stylus CX5600 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter
Stylus CX5700F | USB | 0x04b8/0x0821 | Unsupported | may work with the snapscan backend all-in-one with FAX
Stylus CX5800F | USB | 0x04b8/0x0821 | Unsupported | may work with the snapscan backend all-in-one with FAX
Stylus CX5900 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720
Stylus CX6000 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720
Stylus CX6300 | USB | 0x04b8/0x0805 | Good | all-in-one mistakenly thinks its a PX-A650
Stylus CX6400 | USB | 0x04b8/0x0805 | Good | all-in-one mistakenly thinks its a PX-A650
Stylus CX6500 | USB | 0x04b8/0x0813 | Good | all-in-one
Stylus CX6600 | USB | 0x04b8/0x0813 | Good | all-in-one
Stylus CX6900F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX
Stylus CX7000F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX
Stylus CX7300 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640
Stylus CX7400 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640
Stylus CX7700 | USB | 0x04b8/0x081f | Good | all-in-one
Stylus CX7800 | USB | 0x04b8/0x081f | Good | all-in-one
Stylus CX8300 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740
Stylus CX8400 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740
Stylus CX9300F | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700
Stylus CX9400Fax | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700
Stylus DX3800 | USB | 0x04b8/0x0818 | Good | all-in-one
Stylus DX3850 | USB |  | Good | all-in-one
Stylus DX4000 | USB | 0x04b8/0x082f | Good | all-in-one overseas version of the PX-A620
Stylus DX4200 | USB | 0x04b8/0x0820 | Good | all-in-one
Stylus DX4400 | USB | 0x04b8/0x083f | Unsupported | supported by the epkowa backend plus non-free interpreter
Stylus DX4800 | USB | 0x04b8/0x0819 | Good | all-in-one overseas version of the PX-A650
Stylus DX4850 | USB | 0x04b8/0x0819 | Good | all-in-one DX4800 + card reader
Stylus DX5000 | USB | 0x04b8/0x082b | Good | all-in-one
Stylus DX6000 | USB | 0x04b8/0x082e | Good | all-in-one overseas version of the PX-A720
Stylus DX7000F | USB | 0x04b8/0x0831 | Unsupported | may work with the snapscan backend all-in-one with FAX
Stylus DX7400 | USB | 0x04b8/0x0838 | Good | all-in-one overseas version of the PX-A640
Stylus DX8400 | USB | 0x04b8/0x0839 | Good | all-in-one overseas version of the PX-A740
Stylus DX9400F | USB | 0x04b8/0x083a | Good | all-in-one overseas version of the PX-FA700
Stylus Office BX300F | USB | 0x04b8/0x0848 | Good | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX305F | USB | 0x04b8/0x0863 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX305FW | USB | 0x04b8/0x0863 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX305FW Plus | USB | 0x04b8/0x0870 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX310FN Series | USB | 0x04b8/0x0854 | Good | all-in-one
Stylus Office BX320FW Series | USB | 0x04b8/0x085f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX535WD | USB | 0x04b8/0x0891 | Complete | network interface supported via DFSG non-free iscan-network-nt package overseas version of the PX-504A
Stylus Office BX630FW Series | USB | 0x04b8/0x0890 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX525WD | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
Stylus Office BX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F
Stylus Office BX610FW Series | USB | 0x04b8/0x0855 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-602F
Stylus Office BX625FWD | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX635FWD | USB | 0x04b8/0x088f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office BX925FWD | USB | 0x04b8/0x086a | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-673F
Stylus Office BX935FWD | USB | 0x04b8/0x0892 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office TX300F | USB | 0x04b8/0x0848 | Good | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office TX320F Series | USB | 0x04b8/0x0863 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office TX510FN Series | USB | 0x04b8/0x0854 | Good | all-in-one
Stylus Office TX525FW | USB | 0x04b8/0x085f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Office TX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F
Stylus Office TX610FW Series | USB | 0x04b8/0x0855 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-602F
Stylus Office TX620FWD Series | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Photo PX650 Series | USB | 0x04b8/0x0850 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-702A
Stylus Photo PX660 Series | USB | 0x04b8/0x0862 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-703A
Stylus Photo PX700W | USB Network | 0x04b8/0x0846 | Good | network interface supported all-in-one overseas version of the EP-801A
Stylus Photo PX710W Series | USB | 0x04b8/0x0852 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-802A
Stylus Photo PX720WD Series | USB | 0x04b8/0x0861 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-803A
Stylus Photo PX730WD Series | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-804A
Stylus Photo PX800FW | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A
Stylus Photo PX810FW Series | USB | 0x04b8/0x0853 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-902A
Stylus Photo PX820FWD Series | USB | 0x04b8/0x0860 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-903A
Stylus Photo PX830FWD Series | USB | 0x04b8/0x0879 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-904F
Stylus Photo RX420 | USB | 0x04b8/0x080f | Good | all-in-one
Stylus Photo RX425 | USB | 0x04b8/0x080f | Good | all-in-one
Stylus Photo RX430 | USB | 0x04b8/0x080f | Good | all-in-one
Stylus Photo RX500 | USB | 0x04b8/0x0807 | Good | all-in-one
Stylus Photo RX510 | USB | 0x04b8/0x0807 | Good | all-in-one
Stylus Photo RX520 | USB | 0x04b8/0x081a | Good | all-in-one overseas version of the PM-A750
Stylus Photo RX530 | USB | 0x04b8/0x081a | Good | all-in-one overseas version of the PM-A750
Stylus Photo RX560 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820
Stylus Photo RX585 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840
Stylus Photo RX580 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820
Stylus Photo RX595 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840
Stylus Photo RX590 | USB | 0x04b8/0x0827 | Good | all-in-one overseas version of the PM-A820
Stylus Photo RX600 | USB | 0x04b8/0x0806 | Good | all-in-one overseas version of the PM-A850
Stylus Photo RX610 | USB | 0x04b8/0x083c | Good | all-in-one overseas version of the PM-A840
Stylus Photo RX620 | USB | 0x04b8/0x0811 | Good | all-in-one overseas version of the PM-A870
Stylus Photo RX630 | USB | 0x04b8/0x0811 | Good | all-in-one overseas version of the PM-A870
Stylus Photo RX640 | USB | 0x04b8/0x081c | Good | all-in-one overseas version of the PM-A890
Stylus Photo RX650 | USB | 0x04b8/0x081c | Good | all-in-one overseas version of the PM-A890
Stylus Photo RX680 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940
Stylus Photo RX685 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940
Stylus Photo RX690 | USB | 0x04b8/0x0837 | Good | all-in-one overseas version of the PM-A940
Stylus Photo RX700 | USB | 0x04b8/0x0810 | Good | all-in-one overseas version of the PM-A900
Stylus Photo TX650 Series | USB | 0x04b8/0x0850 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-702A
Stylus Photo TX700W | USB | 0x04b8/0x0846 | Good | network interface probably supported all-in-one overseas version of the EP-801A
Stylus Photo TX710W Series | USB | 0x04b8/0x0852 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-802A
Stylus Photo TX720WD Series | USB | 0x04b8/0x0861 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-803A
Stylus Photo TX730WD Series | USB | 0x04b8/0x087b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-804A
Stylus Photo TX800FW | USB | 0x04b8/0x0844 | Good | network interface probably supported all-in-one overseas version of the EP-901A
Stylus Photo TX820FWD Series | USB | 0x04b8/0x0860 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-903A
Stylus NX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A
Stylus NX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A
Stylus NX125 | USB | 0x04b8/0x085c | Complete | all-in-one
Stylus NX127 | USB | 0x04b8/0x085c | Complete | all-in-one
Stylus NX130 Series | USB | 0x04b8/0x0883 | Complete | all-in-one
Stylus NX200 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus NX210 Series | USB | 0x04b8/0x084f | Good | all-in-one
Stylus NX220 Series | USB | 0x04b8/0x0865 | Complete | all-in-one
Stylus NX230 Series | USB | 0x04b8/0x0885 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus NX300 Series | USB | 0x04b8/0x0848 | Good | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus NX330 Series | USB | 0x04b8/0x0880 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus NX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A
Stylus NX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one
Stylus NX420 Series | USB | 0x04b8/0x0864 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus NX430W Series | USB | 0x04b8/0x0884 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus NX510 Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A
Stylus NX530 Series | USB | 0x04b8/0x0891 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-504A
Stylus NX625 | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
Stylus NX635 | USB | 0x04b8/0x0891 | Complete | network interface supported via DFSG non-free iscan-network-nt package overseas version of the PX-504A
Stylus SX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A
Stylus SX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A
Stylus SX125 | USB | 0x04b8/0x085c | Complete | all-in-one
Stylus SX130 Series | USB | 0x04b8/0x0883 | Complete | all-in-one
Stylus SX200 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus SX205 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus SX210 Series | USB | 0x04b8/0x084f | Good | all-in-one
Stylus SX218 | USB | 0x04b8/0x0865 | Complete | all-in-one
Stylus SX230 Series | USB | 0x04b8/0x0881 | Complete | all-in-one overseas version of the PX-404A
Stylus SX235W | USB | 0x04b8/0x0885 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus SX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A
Stylus SX405 | USB | 0x04b8/0x084a | Good | all-in-one
Stylus SX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one
Stylus SX420W Series | USB | 0x04b8/0x0864 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus SX430W Series | USB | 0x04b8/0x0880 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus SX440W Series | USB | 0x04b8/0x0884 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus SX510W Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A
Stylus SX525WD | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
Stylus SX535WD | USB | 0x04b8/0x0891 | Complete | network interface supported via DFSG non-free iscan-network-nt package overseas version of the PX-504A
Stylus SX600FW | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F
Stylus SX610FW Series | USB | 0x04b8/0x0855 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-602F
Stylus SX620FW Series | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus Scan 2000 | USB | 0x04b8/0x0105 | Untested | apparently mostly the same as the Stylus Scan 2500
Stylus Scan 2500 | USB | 0x04b8/0x0106 | Untested | scanner is apparently a GT-7000
Stylus TX100 | USB | 0x04b8/0x0841 | Good | all-in-one overseas version of the PX-401A
Stylus TX110 Series | USB | 0x04b8/0x084d | Good | all-in-one overseas version of the PX-402A
Stylus TX120 Series | USB | 0x04b8/0x085c | Complete | all-in-one
Stylus TX130 Series | USB | 0x04b8/0x0883 | Complete | all-in-one
Stylus TX200 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus TX203 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus TX209 | USB | 0x04b8/0x0849 | Good | all-in-one
Stylus TX210 Series | USB | 0x04b8/0x084f | Good | all-in-one
Stylus TX220 Series | USB | 0x04b8/0x0865 | Complete | all-in-one
Stylus TX230W Series | USB | 0x04b8/0x0885 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus TX235 | USB | 0x04b8/0x0881 | Complete | all-in-one overseas version of the PX-404A
Stylus TX400 | USB | 0x04b8/0x084a | Good | network interface probably supported all-in-one overseas version of the PX-501A
Stylus TX410 Series | USB | 0x04b8/0x0851 | Good | network interface probably supported all-in-one
Stylus TX420W Series | USB | 0x04b8/0x0864 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus TX430W Series | USB | 0x04b8/0x0880 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus TX435W | USB | 0x04b8/0x0884 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
Stylus TX550W Series | USB | 0x04b8/0x0856 | Good | all-in-one overseas version of the PX-502A
Stylus TX560WD Series | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
WF-2510 Series | USB | 0x04b8/0x08a5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-505F
WF-2520 Series | USB | 0x04b8/0x08a6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-535F
WF-2530 Series | USB | 0x04b8/0x08a6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-535F
WF-2540 Series | USB | 0x04b8/0x08a6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-535F
WF-2630 Series | USB | 0x04b8/0x08c4 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-2650 Series | USB | 0x04b8/0x08c3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-2660 Series | USB | 0x04b8/0x08c3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-3520 Series | USB | 0x04b8/0x0899 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-605F
WF-3530 Series | USB | 0x04b8/0x0899 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-675F
WF-3540 Series | USB | 0x04b8/0x0899 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-3620 Series | USB | 0x04b8/0x08b8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M740F
WF-3640 Series | USB | 0x04b8/0x08b8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M741F
WF-4630 Series | USB | 0x04b8/0x08be | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-4640 Series | USB | 0x04b8/0x08be | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-5620 Series | USB | 0x04b8/0x08bd | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M840F
WF-5690 Series | USB | 0x04b8/0x08bd | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-7510 Series | USB | 0x04b8/0x0869 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-1600F
WF-7520 Series | USB | 0x04b8/0x087c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-1700F
WF-7610 Series | USB | 0x04b8/0x08b9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M5040F
WF-7620 Series | USB | 0x04b8/0x08b9 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M5041F
WF-M1560 Series | USB | 0x04b8/0x08ab | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-M5690 Series | USB | 0x04b8/0x08d0 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-M350F
WF-R4640 Series | USB | 0x04b8/0x08cd | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WF-R5690 Series | USB | 0x04b8/0x08cd | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WP-4511 | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-B750F
WP-4515 | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WP-4521 | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-B750F
WP-4525 | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-B750F
WP-4530 Series | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-B750F
WP-4540 Series | USB | 0x04b8/0x087d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-B750F
WP-4590 Series | USB | 0x04b8/0x087e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 310 Series | USB | 0x04b8/0x0854 | Good | all-in-one
WorkForce 320 Series | USB | 0x04b8/0x0863 | Complete | network interface supported via DFSG non-free iscan-network-nt package some models in the series have a built-in network interface all-in-one
WorkForce 435 | USB | 0x04b8/0x0870 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 500 | USB | 0x04b8/0x084c | Good | all-in-one
WorkForce 520 Series | USB | 0x04b8/0x085f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 545 | USB | 0x04b8/0x0890 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 600 | USB | 0x04b8/0x0847 | Good | network interface probably supported all-in-one overseas version of the PX-601F
WorkForce 610 Series | USB | 0x04b8/0x0855 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-602F
WorkForce 625 | USB | 0x04b8/0x085e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-503A
WorkForce 630 Series | USB | 0x04b8/0x085d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 645 | USB | 0x04b8/0x088f | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce 840 Series | USB | 0x04b8/0x086a | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-673F
WorkForce 845 | USB | 0x04b8/0x0892 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
WorkForce K301 | USB | 0x04b8/0x0872 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
XP-100 Series | USB | 0x04b8/0x0895 | Complete | all-in-one overseas version of the PX-045A
XP-200 Series | USB | 0x04b8/0x0896 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
XP-211 | USB | 0x04b8/0x08ae | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-046A
XP-212 | USB | 0x04b8/0x08ae | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-046A
XP-215 | USB | 0x04b8/0x08ae | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-046A
XP-225 | USB | 0x04b8/0x08c0 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-047A
XP-300 Series | USB | 0x04b8/0x0898 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-435A
XP-310 Series | USB | 0x04b8/0x08af | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-436A
XP-320 Series | USB | 0x04b8/0x08bf | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-437A
XP-400 Series | USB | 0x04b8/0x0898 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the PX-435A
XP-410 Series | USB | 0x04b8/0x08b0 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
XP-420 Series | USB | 0x04b8/0x08c1 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
XP-600 Series | USB | 0x04b8/0x089e | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-775A
XP-510 Series | USB | 0x04b8/0x08b7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-706A
XP-520 Series | USB | 0x04b8/0x08c8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-777A
XP-610 Series | USB | 0x04b8/0x08b6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-776AB/EP-776AW
XP-620 Series | USB | 0x04b8/0x08c8 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-777A
XP-700 Series | USB | 0x04b8/0x089d | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one
XP-710 Series | USB | 0x04b8/0x08b5 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-806AB/EP-806AR/EP-806AW
XP-720 Series | USB | 0x04b8/0x08c7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-807AB/EP-807AR/EP-807AW
XP-750 Series | USB | 0x04b8/0x089c | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-805A/EP-805AR/EP-805AW
XP-760 Series | USB | 0x04b8/0x08c7 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-807AB/EP-807AR/EP-807AW
XP-800 Series | USB | 0x04b8/0x089b | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-905A
XP-810 Series | USB | 0x04b8/0x08b4 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-906F
XP-820 Series | USB | 0x04b8/0x08c6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-907F
XP-850 Series | USB | 0x04b8/0x089a | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-905F
XP-860 Series | USB | 0x04b8/0x08c6 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-907F
XP-950 Series | USB | 0x04b8/0x08b3 | Complete | network interface supported via DFSG non-free iscan-network-nt package all-in-one overseas version of the EP-976A3
Epson ME 350 | USB | 0x04b8/0x088d | Good |
WP-M4525, WP-M4521, PX-K751F, WP-M4595 | USB | 0x04b8/0x08a7 | Good |

### Backend: epsonds (1.0.18 (unmaintained))

Manual page: sane-epsonds

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Epson | DS-5500 | USB | 0x04b8/0x0145 | Untested |
DS-6500 | USB | 0x04b8/0x0145 | Untested |
DS-7500 | USB | 0x04b8/0x0145 | Untested |
DS-50000 | USB | 0x04b8/0x0146 | Untested |
DS-60000 | USB | 0x04b8/0x0146 | Good |
DS-70000 | USB | 0x04b8/0x0146 | Untested |
DS-510 | USB | 0x04b8/0x014c | Good |
DS-560 | USB | 0x04b8/0x014d | Untested |
DS-40 | USB | 0x04b8/0x0150 | Untested |
DS-760 | USB | 0x04b8/0x0152 | Untested |
DS-860 | USB | 0x04b8/0x0152 | Untested |
DS-520 | USB | 0x04b8/0x0154 | Untested |
PX-M7050 Series | USB | 0x04b8/0x08bc | Untested |
WF-8510/8590 Series | USB | 0x04b8/0x08bc | Untested |
PX-M7050FX Series | USB | 0x04b8/0x08cc | Untested |
WF-R8590 Series | USB | 0x04b8/0x08cc | Untested |

### Backend: fujitsu (133)

Link(s): http://www.thebility.com/fujitsu/
Manual page: sane-fujitsu
Comment: Backend updated for SANE release 1.0.26, see sane-fujitsu manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Fujitsu | M3091DC | SCSI |  | Complete | small, old, discontinued
M3092DC | SCSI |  | Complete | small, old, discontinued
fi-4120C | SCSI USB | 0x04c5/0x1041 | Complete | small, recent, discontinued, usb 1.1
fi-4120C2 | SCSI USB | 0x04c5/0x10ae | Complete | small, recent, discontinued, usb 2.0
fi-4220C | SCSI USB | 0x04c5/0x1042 | Complete | small, recent, discontinued, usb 1.1
fi-4220C2 | SCSI USB | 0x04c5/0x10af | Complete | small, recent, discontinued, usb 2.0
fi-5110C | USB | 0x04c5/0x1097 | Complete | small, recent, discontinued
fi-5110EOX/2 | USB | 0x04c5/0x1096 | Complete | small, recent, discontinued
fi-5110EOX3 | USB | 0x04c5/0x10e6 | Complete | small, recent, discontinued
fi-5110EOXM | USB | 0x04c5/0x10f2 | Complete | small, recent, discontinued
fi-5120C | SCSI USB | 0x04c5/0x10e0 | Complete | small, recent, discontinued
fi-5220C | SCSI USB | 0x04c5/0x10e1 | Complete | small, recent, discontinued
fi-5000N | Ethernet |  | Untested | Not a scanner, rather a scanner to ethernet interface
fi-6000NS | Ethernet |  | Untested | small, recent, discontinued, integrated touchscreen and keyboard
ScanSnap S500 | USB | 0x04c5/0x10fe | Complete | small, recent, discontinued
ScanSnap S500M | USB | 0x04c5/0x1135 | Complete | small, recent, discontinued
ScanSnap S510 | USB | 0x04c5/0x1155 | Complete | small, recent, discontinued
ScanSnap S510M | USB | 0x04c5/0x116f | Complete | small, recent, discontinued
fi-6125 | USB | 0x04c5/0x11ee | Complete | small, recent, discontinued
fi-6130 | USB | 0x04c5/0x114f | Complete | small, recent, discontinued
fi-6230 | USB | 0x04c5/0x1150 | Complete | small, recent, discontinued
fi-6130Z | USB | 0x04c5/0x11f3 | Complete | small, recent, discontinued
fi-6230Z | USB | 0x04c5/0x11f4 | Complete | small, recent, discontinued
fi-6120ZLA | SCSI USB | 0x04c5/0x146d | Untested | small, recent, discontinued, expected to work
fi-6220ZLA | SCSI USB | 0x04c5/0x146e | Untested | small, recent, discontinued, expected to work
fi-6125ZLA | SCSI USB | 0x04c5/0x1463 | Untested | small, recent, discontinued, expected to work
fi-6225ZLA | SCSI USB | 0x04c5/0x1464 | Untested | small, recent, discontinued, expected to work
fi-6130ZLA | SCSI USB | 0x04c5/0x1461 | Complete | small, recent, discontinued
fi-6230ZLA | SCSI USB | 0x04c5/0x1462 | Untested | small, recent, discontinued, expected to work
ScanSnap S1500 | USB | 0x04c5/0x11a2 | Complete | small, discontinued
ScanSnap S1500M | USB | 0x04c5/0x11a2 | Complete | small, discontinued, same as S1500
ScanSnap N1800 | Ethernet |  | Untested | small, discontinued, integrated touchscreen and keyboard
ScanSnap N7100 | Ethernet |  | Untested | small, current, integrated touchscreen and keyboard
ScanSnap fi-6010N | Ethernet |  | Untested | small, current, integrated touchscreen and keyboard
fi-6110 | USB | 0x04c5/0x11fc | Complete | small, current
fi-7160 | USB | 0x04c5/0x132e | Complete | small, current
fi-7260 | USB | 0x04c5/0x132f | Complete | small, current
ScanSnap iX500 | USB WiFi | 0x04c5/0x132b | Good | small, current, WiFi not supported. Hardware only scans in color. Backend generates binary and grayscale modes.
ScanSnap iX100 | USB WiFi | 0x04c5/0x13f4 | Good | small, current, WiFi not supported.
ScanSnap SV600 | USB | 0x04c5/0x128e | Untested | Also has a second USB VID 0x13ba. Will require some gymnastics to support.
M3093E | RS232C/Video |  | Unsupported | medium, old, discontinued
M3093DE | RS232C/Video |  | Unsupported | medium, old, discontinued
M3093DG | SCSI |  | Complete | medium, old, discontinued
M3093EX | RS232C/Video |  | Unsupported | medium, old, discontinued
M3093GX | SCSI |  | Complete | medium, old, discontinued
M3096EX | RS232C/Video |  | Unsupported | medium, old, discontinued
M3096GX | SCSI |  | Complete | medium, old, discontinued
M3097E+ | RS232C/Video |  | Unsupported | medium, old, discontinued
M3097G+ | SCSI |  | Complete | medium, old, discontinued
M3097DE | RS232C/Video |  | Unsupported | medium, old, discontinued
M3097DG | SCSI |  | Complete | medium, old, discontinued
fi-4340C | SCSI USB | 0x04c5/0x10cf | Complete | medium, current
fi-4530C | SCSI USB | 0x04c5/0x1078 | Complete | medium, recent, discontinued
fi-4640S | SCSI |  | Complete | medium, recent, discontinued
fi-4750C | SCSI |  | Complete | medium, recent, discontinued
fi-5530C | SCSI USB | 0x04c5/0x10e2 | Complete | medium, recent, discontinued
fi-6140 | SCSI USB | 0x04c5/0x114d | Complete | medium, recent, discontinued
fi-6240 | SCSI USB | 0x04c5/0x114e | Complete | medium, recent, discontinued
fi-6140Z/fi-6140ZLA | SCSI USB | 0x04c5/0x11f1 | Complete | medium, recent, discontinued
fi-6240Z | SCSI USB | 0x04c5/0x11f2 | Complete | medium, recent, discontinued
fi-6135ZLA | SCSI USB | 0x04c5/0x146b | Untested | medium, recent, discontinued, expected to work
fi-6235ZLA | SCSI USB | 0x04c5/0x146c | Untested | medium, recent, discontinued, expected to work
fi-6140ZLA | SCSI USB | 0x04c5/0x145f | Untested | medium, recent, discontinued, expected to work
fi-6240ZLA | SCSI USB | 0x04c5/0x1460 | Untested | medium, recent, discontinued, expected to work
fi-5530C2 | SCSI USB | 0x04c5/0x114a | Complete | medium, current
fi-7180 | USB | 0x04c5/0x132c | Complete | medium, current
fi-7280 | USB | 0x04c5/0x132d | Complete | medium, current
M3099A | RS232C/Video |  | Unsupported | big, old, discontinued
M3099G | SCSI |  | Complete | big, old, discontinued
M3099EH | RS232C/Video |  | Unsupported | big, old, discontinued
M3099GH | SCSI |  | Complete | big, old, discontinued
M3099EX | RS232C/Video |  | Unsupported | big, old, discontinued
M3099GX | SCSI |  | Complete | big, old, discontinued
M4097D | SCSI |  | Complete | big, old, discontinued
M4099D | SCSI |  | Complete | big, old, discontinued
fi-4750L | SCSI |  | Complete | big, recent, discontinued
fi-4860C | SCSI |  | Complete | big, recent, discontinued
fi-4860C2 | SCSI |  | Complete | big, recent, discontinued
fi-4990C | SCSI |  | Complete | big, recent, discontinued
fi-5650C | SCSI USB | 0x04c5/0x10ad | Complete | big, recent, discontinued
fi-5750C | SCSI USB | 0x04c5/0x1095 | Complete | big, recent, discontinued
fi-5900C | SCSI USB | 0x04c5/0x10e7 | Good | big, recent, discontinued. Independent ultrasonic control and multistream unsupported
fi-6750S | USB | 0x04c5/0x1178 | Untested | Simplex, USB only version of fi-6770, won't wakeup via software, discontinued
fi-5950 | SCSI USB | 0x04c5/0x1213 | Untested | big, current. Faster version of fi-5900?
fi-6670 | SCSI USB | 0x04c5/0x1176 | Good | big, current, won't wakeup via software
fi-6670A | SCSI USB | 0x04c5/0x1177 | Good | big, current, VRS CGA board unsupported, won't wakeup via software
fi-6770 | SCSI USB | 0x04c5/0x1174 | Good | big, current, won't wakeup via software
fi-6770A | SCSI USB | 0x04c5/0x1175 | Good | big, current, VRS CGA board unsupported, won't wakeup via software
fi-6800 | SCSI USB | 0x04c5/0x119d | Untested | big, current. Independent ultrasonic control and multistream unsupported
fi-6800-CGA | SCSI USB | 0x04c5/0x119e | Untested | big, current. VRS CGA board unsupported, Independent ultrasonic control and multistream unsupported
fi-6400 | SCSI USB | 0x04c5/0x14ac | Good |
fi-6420 | SCSI USB | 0x04c5/0x14bd | Untested |
fi-6225 | USB | 0x04c5/0x11ef | Untested |
ScanSnap iX500EE | USB | 0x04c5/0x13f3 | Untested |
ScanPartner SP25 | USB | 0x04c5/0x1409 | Unsupported | Possibly Genesys protocol?
ScanPartner SP30 | USB | 0x04c5/0x140a | Unsupported | Possibly Genesys protocol?
ScanPartner SP30F | USB | 0x04c5/0x140c | Unsupported | Possibly Genesys protocol?
N7100 | USB Ethernet | 0x04c5/0x146f | Untested |
fi-7480 | USB | 0x04c5/0x14b8 | Good |
fi-7460 | USB | 0x04c5/0x14be | Good |
fi-7140 | USB | 0x04c5/0x14df | Untested |
fi-7240 | USB | 0x04c5/0x14e0 | Untested |
fi-7135 | USB | 0x04c5/0x14e1 | Untested |
fi-7235 | USB | 0x04c5/0x14e2 | Untested |
fi-7130 | USB | 0x04c5/0x14e3 | Untested |
fi-7230 | USB | 0x04c5/0x14e4 | Untested |
fi-7125 | USB | 0x04c5/0x14e5 | Untested |
fi-7225 | USB | 0x04c5/0x14e6 | Untested |
fi-7120 | USB | 0x04c5/0x14e7 | Untested |
fi-7220 | USB | 0x04c5/0x14e8 | Untested |
fi-400F | USB | 0x04c5/0x151e | Untested |
fi-7030 | USB | 0x04c5/0x151f | Good |
fi-7700 | USB | 0x04c5/0x1520 | Good |
fi-7600 | USB | 0x04c5/0x1521 | Good |
fi-7700S | USB | 0x04c5/0x1522 | Untested |

### Backend: genesys (1.0-63)

Link(s): http://www.meier-geinitz.de/sane/genesys-backend/
Manual page: sane-genesys
Comment: Only the USB scanners mentioned below are currently supported.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Plustek | OpticBook 3600 | USB | 0x07b3/0x0900 | Basic | Has a Primax USB ID
Medion/Lifetec/Tevion/Cytron | MD5345 | USB | 0x0461/0x0377 | Good | Has a Primax USB ID
MD6228 | USB | 0x0461/0x0377 | Good | Has a Primax USB ID. Same as MD5345
MD6471 | USB | 0x0461/0x0377 | Complete | Has a Primax USB ID. Same as MD5345
Hewlett-Packard | ScanJet 2300C | USB | 0x03f0/0x0901 | Complete | 600x1200 dpi max
ScanJet 2400C | USB | 0x03f0/0x0a01 | Complete | 1200x1200 dpi max
ScanJet G2410 | USB | 0x03f0/0x0a01 | Basic | clone of the HP 2400C
ScanJet 3670C | USB | 0x03f0/0x1405 | Complete | 1200x1200 dpi max, complete transparency adaptor support
ScanJet 3690C | USB | 0x03f0/0x1405 | Complete | 1200x1200 dpi max, same as HP 3670C
ScanJet 4850C | USB | 0x03f0/0x1b05 | Good | resolution from 100 to 2400 supported, UTA not supported yet
ScanJet G4010 | USB | 0x03f0/0x4505 | Good | resolution from 100 to 2400 supported, UTA not supported yet
ScanJet G4050 | USB | 0x03f0/0x4605 | Good | resolution from 100 to 2400 supported, UTA not supported yet
ScanJet N6310 | USB | 0x03f0/0x4705 | Untested | Not supported yet
Canon | CanoScan LiDE 35 | USB | 0x04a9/0x2213 | Good | Same ids as LiDE 50.
CanoScan LiDE 40 | USB | 0x04a9/0x2213 | Good | Same ids as LiDE 50.
CanoScan LiDE 50 | USB | 0x04a9/0x2213 | Good |
CanoScan LiDE 60 | USB | 0x04a9/0x221c | Good |
CanoScan LiDE 80 | USB | 0x04a9/0x2214 | Basic | No 2400 dpi support, slow speed at lower resolution
CanoScan LiDE 100 | USB | 0x04a9/0x1904 | Complete | GL847 based, resolution from 75 to 2400 dpi
CanoScan LiDE 110 | USB | 0x04a9/0x1909 | Complete | GL124 based, resolution from 75 to 2400 dpi
CanoScan LiDE 120 | USB | 0x04a9/0x190e | Complete | GL124+ based, resolution from 75 to 2400 dpi
CanoScan LiDE 200 | USB | 0x04a9/0x1905 | Complete | GL847 based, resolution from 75 to 4800 dpi
CanoScan LiDE 210 | USB | 0x04a9/0x190a | Complete | GL124 based, resolution from 75 to 4800 dpi
CanoScan LiDE 220 | USB | 0x04a9/0x190f | Complete | GL124+ based, resolution from 75 to 4800 dpi
CanoScan 4400f | USB | 0x04a9/0x2228 | Unsupported | GL843 based, to be added to the genesys backend
CanoScan 5600F | USB | 0x04a9/0x1906 | Unsupported | GL847 based, to be added to the genesys backend
CanoScan 700F | USB | 0x04a9/0x1907 | Good | GL847 based, resolution from 75 to 4800 dpi
Canon Image Formula 101 | USB | 0x1083/0x162e | Unsupported | GL846 based, work in progress
Visioneer | Strobe XP 100,r3 | USB | 0x04a7/0x049b | Good | All resolution and mode supported, calibration is available
Strobe XP 200 | USB | 0x04a7/0x0426 | Good | All resolution and mode supported, calibration is available
Strobe XP 300 | USB | 0x04a7/0x0474 | Good | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally.
Roadwarrior | USB | 0x04a7/0x0494 | Basic | All resolution and mode supported, calibration is available
Visioneer OneTouch 7100 | USB | 0x04a7/0x0229 | Complete | Same as MD5345
Pentax | DSmobile 600 | USB | 0x0a17/0x3210 | Good | All resolution and mode supported, calibration is available
DSmobile 600 | USB | 0x04f9/0x2038 | Good | All resolution and mode supported, calibration is available
DCT | DocketPort 487 | USB | 0x1dcc/0x4810 | Basic | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally.
Syscan | DocketPort 485 | USB | 0x0a82/0x4810 | Basic | All resolution and mode supported, front- and backside side-by-side, with backside mirrored horizontally.
DocketPort 465 | USB | 0x0a82/0x4802 | Untested | All resolution and mode should be supported, but uncorrected scans
DocketPort 665 | USB | 0x0a82/0x4803 | Basic | All resolution and mode supported, calibration is available
DocketPort 685/ Ambir DS685 | USB | 0x0a82/0x480c | Good | All resolution and mode supported, calibration is available, front- and backside side-by-side, with backside mirrored horizontally.
Xerox | Travel Scanner 100 | USB | 0x04a7/0x04ac | Good | All resolution and mode supported, calibration is available
2400 Onetouch | USB | 0x0461/0x038b | Complete | GL646 based, resolution from 75 to 2400 dpi
Panasonic | KV-SS080 | USB | 0x04da/0x100f | Complete | All resolution and mode supported, calibration is available. Support sponsored by cncsolutions (http://www.cncsolutions.com.br)

### Backend: gt68xx (1.0-84 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/gt68xx-backend/
Manual page: sane-gt68xx
Comment: Only the USB scanners mentioned below are supported. For other Mustek BearPaws, look at the Plustek and the MA-1509 backend.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Artec/Ultima | Ultima 2000 | USB | 0x05d8/0x4002 | Good | Works, only product id 0x4002 is supported
Ultima 2000 e+ | USB | 0x05d8/0x4002 | Good | Works, however 12 bit mode doesn't seem to be supported
Boeder | Sm@rtScan Slim Edition | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000
Fujitsu | 1200CUS | USB | 0x05d8/0x4002 | Basic | Works, but is slow. Probably a Mustek BearPaw 2400 CU clone.
Genius | ColorPage Slim 1200 | USB | 0x0458/0x201e | Untested | Untested but should work.
Colorpage SF600 | USB | 0x0458/0x2021 | Basic |
Colorpage Vivid3x | USB | 0x0458/0x2011 | Good |
Colorpage Vivid3 V2 | USB | 0x0458/0x2011 | Good | Same as Colorpage Vivid3x
Colorpage Vivid3xe | USB | 0x0458/0x2017 | Good |
Colorpage Vivid4 | USB | 0x0458/0x2014 | Good |
Colorpage Vivid4x | USB | 0x0458/0x201b | Good |
Colorpage Vivid4xe | USB | 0x0458/0x201a | Good |
Colorpage Vivid 1200 X | USB | 0x0458/0x201d | Good |
Colorpage Vivid 1200 XE | USB | 0x0458/0x201f | Good |
Googlegear | 2000 | USB | 0x05d8/0x4002 | Good | Same as Artec Ultima 2000.
Lexmark | X70 | USB | 0x043d/0x002d | Good | Works, some resolutions fail at 16 bit
X73 | USB | 0x043d/0x002d | Good | Works, some resolutions fail at 16 bit, same as X70
Medion/Lifetec/Tevion/Cytron | MD 4394 | USB | 0x05d8/0x4002 | Good | Product id 0x4002. If you have 0x4003, use artec_eplus48u backend.
MD/LT 9375 | USB | 0x05d8/0x4002 | Untested | Untested, but is reported to have the same ids as the Artec Ultima 2000. Please test.
MD/LT 9385 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000
LT 9452 | USB | 0x05d8/0x4002 | Good | Similar to Mustek ScanExpress 1200 UB Plus
MD 9458 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000 (e+?)
Mustek | BearPaw 1200 CS | USB | 0x055f/0x021e | Good |
BearPaw 1200 CU | USB | 0x05d8/0x4002 | Good |
BearPaw 1200 CU Plus | USB | 0x055f/0x021b | Good |
BearPaw 1200 CU Plus | USB | 0x055f/0x021c | Good |
BearPaw 1200 TA | USB | 0x055f/0x021e | Good | Transparency adapter supported
BearPaw 1248 CU | USB | 0x055f/0x021c | Good | Seems to use the same ids as BearPaw 1200 CU Plus.
BearPaw 2400 CS | USB | 0x055f/0x0218 | Untested | Probably works, reports are welcome
BearPaw 2400 CS Plus | USB | 0x055f/0x0219 | Good | Works, problems with 12/16 bit modes?
BearPaw 2400 CU | USB | 0x05d8/0x4002 | Basic | Works, but is slow
BearPaw 2400 CU Plus | USB | 0x055f/0x021d | Good |
BearPaw 2400 TA | USB | 0x055f/0x0218 | Good | Transparency adapter supported
BearPaw 2400 TA Plus | USB | 0x055f/0x0219 | Good | Transparency adapter supported
BearPaw 2448 CS Plus | USB | 0x055f/0x021a | Basic | Slow. Same as 2448 TA Plus, but without TA.
BearPaw 2448 TA Plus | USB | 0x055f/0x021a | Basic | Slow. Transparency adapter supported. Slow. Brightness depends on resolution?
Plug-n-Scan 2400 MT | USB | 0x055f/0x0219 | Good | Works but is slow in high resolutions. Same as BearPaw 2400 TA Plus.
Plug-n-Scan 2400 M | USB | 0x055f/0x0219 | Good | Works but is slow in high resolutions. Same as BearPaw 2400 CS Plus.
ScanExpress 1200 UB Plus | USB | 0x05d8/0x4002 | Good |
ScanExpress 1248 UB | USB | 0x055f/0x021f | Complete |
ScanExpress 2400 USB | USB | 0x05d8/0x4002 | Minimal | Should be detected but may need some more work in the code. Testers welcome. Please contact me if you own this scanner.
ScanExpress A3 USB | USB | 0x055f/0x0210 | Basic | Still some vertical stripes.
ScanMagic 1200 UB Plus | USB | 0x05d8/0x4002 | Good | Same as ScanExpress 1200 UB Plus
NeatReceipts | Scanalizer Professional 2.5 | USB | 0x07b3/0x0412 | Untested | Similar to Plustek OpticSlim M12. Please tell us if this scanner works.
Mobile Scanner | USB | 0x07b3/0x0462 | Basic | Similar to Plustek OpticSlim M12.
Nortek | MyScan 1200 | USB | 0x07b3/0x040b | Untested | Untested. Please test. Similar to Plustek OpticPro S12?
Packard Bell | Diamond 1200 | USB | 0x05d8/0x4002 | Good | Similar to Mustek BearPaw 1200 (Plus)
Diamond 1200 Plus | USB | 0x055f/0x021c | Good | Similar to Mustek BearPaw 1200 Plus
Diamond 1200 Plus | USB | 0x055f/0x021b | Good | Similar to Mustek BearPaw 1200 Plus
Diamond 2450 | USB | 0x055f/0x0219 | Good |
Plustek | OpticPro 1248U | USB | 0x07b3/0x0400 | Good |
OpticPro 1248U | USB | 0x07b3/0x0401 | Good |
OpticPro U16B | USB | 0x07b3/0x0402 | Good |
OpticPro U16B+ | USB | 0x07b3/0x0403 | Good |
OpticPro UT16B | USB | 0x07b3/0x0403 | Untested | Probably works. Transparency adapter not supported yet. Please contact me if you own such a device.
OpticPro S12 | USB | 0x07b3/0x040b | Good | Product ID 0x040b only.
OpticPro S24 | USB | 0x07b3/0x040e | Good | Product ID 0x040e only. Is reported to work.
OpticPro ST12 | USB | 0x07b3/0x040b | Untested | Product ID 0x040b only. Needs testing. Transparency adapter completely untested. Please contact me if you own such a scanner.
OpticSlim 1200 | USB | 0x07b3/0x0413 | Good |
OpticSlim 2400 | USB | 0x07b3/0x0422 | Good | Works up to 1200 dpi.
OpticSlim 2400 plus | USB | 0x07b3/0x0454 | Good | Same as OpticSlim 2400.
Iriscan Express 2 | USB | 0x07b3/0x045f | Complete | Works up to 1200 dpi. Calibration with external calibration sheet supported
OpticSlim M12 | USB | 0x07b3/0x0412 | Complete | Works up to 1200 dpi. Calibration with external calibration sheet supported
RevScan | 19200i | USB | 0x07b3/0x0400 | Good | Similar to Plustek OpticPro 1248U
Trust | 240TH Easy Webscan Gold | USB | 0x055f/0x0218 | Good | Same as Mustek Bearpaw 2400 TA plus.
Compact Scan USB 19200 | USB | 0x05d8/0x4002 | Good | Works, if you have vendor id 0x055f and product id 0x0006, use the mustek_usb backend instead, similar to Mustek ScanExpress 1200 UB (Plus)
Direct WebScan 19200 | USB | 0x055f/0x021c | Good | Same as Mustek BearPaw 1200 CU Plus (0x021c).
Flat Scan USB 19200 | USB | 0x05d8/0x4002 | Good | Similar to Artec Ultima 2000
Visioneer | OneTouch 7300 | USB | 0x04a7/0x0444 | Good | Works upto 1200 dpi and 12 bits/color.

### Backend: hp (unmaintained)

Manual page: sane-hp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet Plus | Propietary |  | Complete | Driver for HP parallel interface card required
ScanJet IIc | SCSI |  | Complete |
ScanJet IIp | SCSI |  | Complete |
ScanJet IIcx | SCSI |  | Complete |
ScanJet 3c | SCSI |  | Complete |
ScanJet 3p | SCSI |  | Complete |
ScanJet 4c | SCSI |  | Complete |
ScanJet 4p | SCSI |  | Complete | Buttons may not work on some scanners
ScanJet 4100C | USB | 0x03f0/0x0101 | Complete | Buttons may not work on some scanners
ScanJet 5p | SCSI |  | Complete | Buttons may not work on some scanners
ScanJet 5100C | Parport |  | Complete | Requires ppscsi driver and epst module. Buttons may not work on some scanners
ScanJet 5200C | Parport USB | 0x03f0/0x0401 | Complete | Parallel interface requires ppscsi driver and epst module. Buttons may not work on some scanners
ScanJet 6100C | SCSI |  | Complete |
ScanJet 6200C | SCSI USB | 0x03f0/0x0201 | Complete | Buttons may not work on some scanners
ScanJet 6250C | SCSI USB | 0x03f0/0x0201 | Complete | Buttons may not work on some scanners
ScanJet 6300C | SCSI USB | 0x03f0/0x0601 | Complete | Buttons may not work on some scanners
ScanJet 6350C | SCSI USB | 0x03f0/0x0601 | Complete | Buttons may not work on some scanners
ScanJet 6390C | SCSI USB | 0x03f0/0x0601 | Complete | Buttons may not work on some scanners
PhotoSmart PhotoScanner | SCSI |  | Complete |

### Backend: hp3500 (1.1)

Link(s): http://projects.troy.rollo.name/rt-scanners/
Manual page: sane-hp3500
Comment: HP3500 series scanners.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 3500C | USB | 0x03f0/0x2205 | Good |
ScanJet 3530C | USB | 0x03f0/0x2005 | Good |
ScanJet 3570C | USB | 0x03f0/0x2005 | Good |

### Backend: hp3900 (0.12 (unmaintained))

Link(s): http://sourceforge.net/projects/hp3900-series/
Manual page: sane-hp3900
Comment: Still Beta

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 3800 | USB | 0x03f0/0x2605 | Basic | Works with resolutions equal and less than 600dpi
ScanJet 3970c | USB | 0x03f0/0x2305 | Good |
ScanJet 4070 Photosmart | USB | 0x03f0/0x2405 | Good |
ScanJet 4370 | USB | 0x03f0/0x4105 | Basic | Works with resolutions lower than 1200dpi
ScanJet G2710 | USB | 0x03f0/0x2805 | Basic | Similar to hp scanjet 3800
ScanJet G3010 | USB | 0x03f0/0x4205 | Basic | Similar to hp scanjet 4370
ScanJet G3110 | USB | 0x03f0/0x4305 | Basic | Similar to hp scanjet 4370
UMAX | Astra 4900 | USB | 0x06dc/0x0020 | Minimal | developing yet
BenQ | 5550 | USB | 0x04a5/0x2211 | Minimal | developing yet

### Backend: hp4200 (1.0-2 (unmaintained))

Link(s): http://hp4200-backend.sourceforge.net
Manual page: sane-hp4200

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 4200C | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only
ScanJet 4200Cxi | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only
ScanJet 4200Cse | USB | 0x03f0/0x0105 | Basic | 8bpp color, 75/150/300/600 dpi only

### Backend: hp5400 (1.0-2 (unmaintained))

Link(s): http://sourceforge.net/projects/hp5400backend
Manual page: sane-hp5400
Comment: HP5400 and HP5470 scanners. Prototype backend available

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5400c | USB | 0x03f0/0x1005 | Basic |
ScanJet 5470c | USB | 0x03f0/0x1105 | Basic |
ScanJet 5490c | USB | 0x03f0/0x1105 | Basic |

### Backend: hp5590 (1.0.5)

Manual page: sane-hp5590

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 4500C | USB | 0x03f0/0x1205 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives
ScanJet 4570C | USB | 0x03f0/0x1305 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/TMA slides/TMA negatives
ScanJet 5500C | USB | 0x03f0/0x1305 | Untested | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/TMA slides/TMA negatives
ScanJet 5550C | USB | 0x03f0/0x1205 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives
ScanJet 5590 | USB | 0x03f0/0x1705 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives
ScanJet 7650 | USB | 0x03f0/0x1805 | Complete | Lineart/grayscale/color (24 bit), 100/200/300/600/1200/2400 DPI, flatbed/ADF/ADF duplex/TMA slides/TMA negatives

### Backend: hpljm1005 (0 (unmaintained))

Manual page: sane-hpljm1005

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | LaserJet M1005 MFP | USB | 0x03f0/0x3b17 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI
LaserJet M1120 MFP | USB | 0x03f0/0x5617 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI
LaserJet M1120n MFP | USB | 0x03f0/0x5717 | Good | grayscale/color (24 bit), 75/100/150/200/300/600/1200 DPI

### Backend: hpsj5s (0.03 (unmaintained))

Link(s): http://hpsj5s.sourceforge.net/
Manual page: sane-hpsj5s

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5s | Parport (EPP) |  | Minimal | Requires libieee1284 library. Only gray mode.

### Backend: hs2p (1.00)

Link(s): http://www.acjlaw.net:8080/~jeremy/Ricoh/
Manual page: sane-hs2p
Comment: This backend has been tested with the IS450DE (Duplex/Endorser). All major functions necessary for scanning are supported. This backend should work with all Ricoh scanners in the IS450 family as well as the IS420 series, but the IS420 has not yet been tested. Features provided by the optional Image Processing Unit (IPU) are not yet integrated into the backend, as my scanner lacks the IPU.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Ricoh | IS450 | SCSI |  | Complete | All major scanning-related features are supported (except for IPU). Certain non-scanning features, such as those related to scanner maintenance, are not supported. Such features would be better implemented in a separate stand-alone tool. For instance, if you replace the ADF Unit, you must recalibrate the scanner optics using a Ricoh Test Sheet and reset the E^2PROM registers. Reports are welcome.
IS-410 | SCSI |  | Untested | Untested, please report!
IS-420 | SCSI |  | Untested | Untested, please report!
IS-430 | SCSI |  | Untested | Untested, please report!

### Backend: ibm (1.0-4 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/ibm-backend/
Manual page: sane-ibm
Comment: This backend has had only limited testing. It needs more work especially for the Ricoh scanners. Patches are welcome.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
IBM | 2456 | SCSI |  | Basic | Was reported to work long time ago. Reports are welcome.
Ricoh | IS-410 | SCSI |  | Untested | Untested, please report!
IS-420 | SCSI |  | Basic | Works at least in flatbed mode.
IS-430 | SCSI |  | Untested | Untested, please report!

### Backend: kodak (7)

Link(s): http://www.thebility.com/kodak/
Manual page: sane-kodak
Comment: New backend for SANE release 1.0.21, see sane-kodak manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Kodak | Scanner 1500 | SCSI |  | Untested | Please test!
Scanner 2500 | SCSI |  | Untested | Please test!
Scanner 3500 | SCSI |  | Untested | Please test!
Scanner 3510 | SCSI |  | Untested | Please test!
Scanner 3520 | SCSI |  | Untested | Please test!
Color Scanner 3590C | SCSI |  | Untested | Please test!
Color Scanner 4500 | SCSI |  | Untested | Please test!
i150 Scanner | IEEE-1394 |  | Untested | Please test!
i160 Scanner | IEEE-1394 |  | Untested | Please test!
i250 Scanner | IEEE-1394 |  | Untested | Please test!
i260 Scanner | IEEE-1394 |  | Untested | Please test!
i280 Scanner | IEEE-1394 |  | Untested | Please test!
Scanner 900 | SCSI |  | Untested | Please test!
Scanner 923 | SCSI |  | Untested | Please test!
Scanner 5500 | SCSI |  | Untested | Please test!
Scanner 7500 | SCSI |  | Untested | Please test!
Scanner 7520 | SCSI |  | Untested | Please test!
Scanner 9500 | SCSI |  | Untested | Please test!
Scanner 9520 | SCSI |  | Untested | Please test!
i610 Scanner | IEEE-1394 |  | Untested | Please test!
i620 Scanner | IEEE-1394 |  | Untested | Please test!
i640 Scanner | IEEE-1394 |  | Untested | Please test!
i660 Scanner | IEEE-1394 |  | Untested | Please test!
i730 Scanner | IEEE-1394 |  | Untested | Please test!
i750 Scanner | IEEE-1394 |  | Untested | Please test!
i780 Scanner | IEEE-1394 |  | Untested | Please test!
i810 Scanner | SCSI |  | Untested | Please test!
i820 Scanner | SCSI |  | Untested | Please test!
i830 Scanner | SCSI |  | Untested | Please test!
i840 Scanner | SCSI |  | Untested | Please test!
i1840 Scanner | IEEE-1394 |  | Untested | Please test!
i1860 Scanner | IEEE-1394 |  | Basic | Uncompressed B&W, Gray and Color, some automatic features supported
s1740 | SCSI |  | Untested | Please test!

### Backend: kodakaio (2.7.2)

Link(s): http://sourceforge.net/projects/cupsdriverkodak/
Manual page: sane-kodakaio
Comment: Backend for Kodak AiO ESP and Hero printers. Also possibly Advent AWL10

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Kodak | ESP 2150 | USB | 0x040a/0x4059 | Untested | Please test!
ESP 2170 | USB | 0x040a/0x4066 | Basic | Tested with network
ESP 3200 | USB | 0x040a/0x4043 | Untested | Please test!
ESP 3300 | USB | 0x040a/0x4031 | Untested | Please test!
ESP 4100 | USB | 0x040a/0x4053 | Untested | Please test!
ESP 5000 | USB | 0x040a/0x4028 | Untested | Please test!
ESP 5100 | USB | 0x040a/0x4025 | Untested | Please test!
ESP 5200 | USB Ethernet | 0x040a/0x4041 | Complete | USB good, Network good
ESP 5300 | USB | 0x040a/0x4026 | Untested | Please test!
ESP 5500 | USB | 0x040a/0x4027 | Untested | Please test!
ESP 6100 | USB | 0x040a/0x4054 | Untested | Please test!
ESP 7200 | USB | 0x040a/0x4056 | Untested | Please test!
ESP 9200 | USB | 0x040a/0x4065 | Untested | Please test!
ESP 5 | USB | 0x040a/0x4032 | Untested | Please test!
ESP 7 | USB | 0x040a/0x403e | Untested | Please test!
ESP 9 | USB | 0x040a/0x403f | Untested | Please test!
ESP C110 | USB | 0x040a/0x4057 | Untested | Please test!
ESP C115 | USB | 0x040a/0x4058 | Untested | Please test!
ESP C310 | USB | 0x040a/0x405d | Untested | Please test!
ESP C315 | USB | 0x040a/0x405e | Untested | Please test!
Hero 3.1 | USB | 0x040a/0x406d | Untested | Please test!
Hero 4.1 | USB | 0x040a/0x4069 | Untested | Please test!
Hero 5.1 | USB | 0x040a/0x4064 | Untested | Please test!
Hero Office 6.1 | USB | 0x040a/0x4062 | Basic | Does the adf work?
Hero 7.1 | USB | 0x040a/0x4063 | Untested | Please test!
Hero 9.1 | USB Ethernet | 0x040a/0x4067 | Complete | USB good, Network good
Advent | AW10 | USB | 0x040a/0x4060 | Untested | Please test!

### Backend: kvs20xx (unmaintained)

Manual page: sane-kvs20xx
Comment: New backend for SANE release 1.0.22, see sane-kvs20xx manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Panasonic | KV-S2025C | SCSI |  | Untested |
KV-S2026C | USB SCSI | 0x04da/0x1000 | Untested |
KV-S2028C | USB | 0x04da/0x100a | Untested |
KV-S2045C | SCSI |  | Untested |
KV-S2046C | USB SCSI | 0x04da/0x1001 | Untested |
KV-S2048C | USB | 0x04da/0x1009 | Untested |

### Backend: kvs40xx (unmaintained)

Manual page: sane-kvs40xx
Comment: New backend for SANE release 1.0.23, see sane-kvs40xx manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Panasonic | KV-S4065C | USB | 0x04da/0x100d | Untested |
KV-S4085C | USB | 0x04da/0x100c | Untested |
KV-S7075C | USB | 0x04da/0x100e | Untested |

### Backend: kvs1025 (unmaintained)

Manual page: sane-kvs1025
Comment: New backend for SANE release 1.0.21, see sane-kvs1025 manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Panasonic | KV-S1020C | USB | 0x04da/0x1007 | Good |
KV-S1025C | USB | 0x04da/0x1006 | Good |
KV-S1045C | USB | 0x04da/0x1010 | Good |

### Backend: leo (1.0-10 (unmaintained))

Link(s): http://www.zago.net/sane/#leo
Manual page: sane-leo

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
LEO | LEOScan S3 | SCSI |  | Good | FCC ID LUZFS1130
Across Technologies | FS-1130 | SCSI |  | Good | FCC ID LUZFS1130
Genius | FS-1130 Colorpage Scanner | SCSI |  | Good |

### Backend: lexmark (1.0-0 (unmaintained))

Link(s): http://stef.dev.free.fr/sane/lexmark
Manual page: sane-lexmark
Comment: This backend supports lexmark x1100 series scanners.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Lexmark | X1110 | USB | 0x043d/0x007c | Untested |
X1130 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi
X1140 | USB | 0x043d/0x007c | Untested |
X1150 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi
X1170 | USB | 0x043d/0x007c | Good | Supports 75, 150, 300, 600 dpi
X1180 | USB | 0x043d/0x007c | Good |
X1185 | USB | 0x043d/0x007c | Good | Tested with xscanimage. Supports 75, 150, 300, 600, 1200(600x1200) dpi resolutions. Does grayscale or colour scans in the following sizes: wallet, 3x5, 4x6, 5x7, 8x10, letter.
X1195 | USB | 0x043d/0x007c | Untested |
X74 | USB | 0x043d/0x0060 | Good | Supports 75, 150, 300, 600 dpi
X12xx | USB | 0x043d/0x007d | Good | USB1.1 is OK, USB2.0 needs testing
Dell | A920 | USB | 0x413c/0x5105 | Good | Relabelled X11xx model

### Backend: ma1509 (1.0-3 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/ma1509-backend/
Manual page: sane-ma1509

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Mustek | BearPaw 1200 F | USB | 0x055f/0x0010 | Good | Works upto 600 dpi. No support for TA and ADF yet.
Fujitsu | fi-4110EOX/2/3 | USB | 0x04c5/0x1040 | Unsupported | Uses ma1509 chip, but very different from other scanners supported by the ma1509 backend

### Backend: magicolor (1.0.0 (unmaintained))

Link(s): http://wiki.kainhofer.com/hardware/magicolor_scan
Manual page: sane-magicolor

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
KONICA MINOLTA | magicolor 1690MF | USB Network | 0x132b/0x2089 | Good | Multi-function color laser printer with fax, scanner and network interface
magicolor 4690MF | USB Network | 0x132b/0x2079 | Good | Multi-function color laser printer with fax, scanner and network interface
BizHub 162/132 | USB Network |  | Unsupported | Uses a similar protocol as the magicolor 1690MF, according to Ilia Sotnikov.
DiMage 1611 | USB Network |  | Unsupported | Uses a similar protocol as the magicolor 1690MF, according to Ilia Sotnikov.

### Backend: matsushita (1.0-7 (unmaintained))

Link(s): http://www.zago.net/sane
Manual page: sane-matsushita

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Panasonic | KV-SS25 | SCSI |  | Complete |
KV-SS25D | SCSI |  | Complete |
KV-SS50 | SCSI |  | Untested |
KV-SS55 | SCSI |  | Untested |
KV-SS50EX | SCSI |  | Untested |
KV-SS55EX | SCSI |  | Minimal | no color, no high resolution, no automatic cropping
KV-SS850 | SCSI |  | Untested |
KV-SS855 | SCSI |  | Untested |
KV-S2025C | SCSI |  | Minimal | no color, no high resolution, no automatic cropping
KV-S2045C | SCSI |  | Minimal | no color, no high resolution, no automatic cropping
KV-S2065L | SCSI |  | Minimal | no color, no high resolution, no automatic cropping

### Backend: microtek (0.13.1 (unmaintained))

Link(s): http://www.mir.com/mtek/
Manual page: sane-microtek

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Microtek | Scanmaker E6 | SCSI |  | Good |
Scanmaker E3 | SCSI |  | Good |
Scanmaker E2 | SCSI |  | Good | 3-pass
Scanmaker 35t+ | SCSI |  | Good | slide-scanner
Scanmaker 45t | SCSI |  | Good | slide-scanner
Scanmaker 35 | SCSI |  | Good | slide-scanner
Scanmaker III | SCSI |  | Good |
Scanmaker IISP | SCSI |  | Good |
Scanmaker IIHR | SCSI |  | Good | 3-pass
Scanmaker IIG | SCSI |  | Good | gray only
Scanmaker II | SCSI |  | Good | 3-pass
Scanmaker 600Z(S) | SCSI |  | Untested |
Scanmaker 600G(S) | SCSI |  | Basic | gray only (see manpage)
Color PageWiz | SCSI (Parport) |  | Basic | sheet-fed (preliminary, see mapage)
Agfa | Arcus II | SCSI |  | Good | Arcus *II*, not Arcus!
StudioScan | SCSI |  | Good |
StudioScan II | SCSI |  | Good |
StudioScan IIsi | SCSI |  | Good |
Studiostar | SCSI |  | Minimal | Is detected but scans are very dark
DuoScan | SCSI |  | Basic |
Vobis | Highscreen Realscan | SCSI |  | Good |
Genius | Colorpage-SP2 | SCSI |  | Good | Same as Microtek Scanmaker E3

### Backend: microtek2 (unmaintained)

Link(s): http://karstenfestag.gmxhome.de/linux.html
Manual page: sane-microtek2

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Microtek | ScanMaker E3plus | Parport |  | Complete |
ScanMaker E3plus | SCSI |  | Complete |
ScanMaker X6 | SCSI |  | Complete |
ScanMaker X6EL | SCSI |  | Basic |
ScanMaker X6USB | USB | 0x05da/0x0099 | Good |
ScanMaker V300 | SCSI |  | Good |
ScanMaker V300 | Parport |  | Good |
ScanMaker V310 | SCSI |  | Basic |
ScanMaker V310 | Parport |  | Basic |
ScanMaker V600 | SCSI |  | Basic |
ScanMaker V600 | Parport |  | Basic |
ScanMaker 330 | SCSI |  | Basic |
ScanMaker 630 | SCSI |  | Basic |
ScanMaker 636 | SCSI |  | Complete |
ScanMaker 6400XL | SCSI |  | Complete |
ScanMaker 9600XL | SCSI |  | Good | only flatbed mode ?
ScanMaker 9800XL | IEEE-1394 |  | Minimal | IEEE-1394 seems to work. See link. More reports welcome.
Phantom 330CX | Parport |  | Complete |
SlimScan C3 | Parport |  | Complete |
Phantom 636 | SCSI |  | Complete |
Phantom 636CX | Parport |  | Complete |
SlimScan C6 | USB | 0x05da/0x009a | Complete |
ScanMaker V6UPL | USB | 0x05da/0x00b6 | Basic | Sometimes scan speed goes to fast and results look badly smudged.
ScanMaker V6USL | SCSI |  | Complete |
ScanMaker V6USL | USB | 0x05da/0x00a3 | Complete |
ScanMaker V6USL | USB | 0x05da/0x80a3 | Complete |
ScanMaker X12USL | SCSI |  | Good | only Flatbed mode ?
Vobis | HighScan | SCSI |  | Complete | only E3plus based models
Scanport | SQ300 | Parport? |  | Basic |
SQ2030 | Parport |  | Basic |
SQ4836 | SCSI |  | Basic |
Genius | ColorPage-EP | Parport |  | Good |

### Backend: mustek (1.0-138 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/mustek-backend/
Manual page: sane-mustek
Comment: Most Mustek SCSI scanners are supported by this backend. For USB scanners, look at the mustek_usb backend.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Mustek | Paragon MFS-6000CX | SCSI |  | Good | 3-pass
Paragon MFS-12000CX | SCSI |  | Good | 3-pass
Paragon MFC-600S | SCSI |  | Complete |
Paragon 600 II CD | SCSI |  | Complete |
Paragon 600 II ED | Parport |  | Untested | Completely untested. If it's the same as the 600 II EP, it may work. Please contact me if you own such a device.
Paragon 600 II EP | Parport |  | Minimal | Works, however only low resolutions and quality in color mode is bad.
ScanMagic 600 II SP | SCSI |  | Complete |
TwainScan II SP | SCSI |  | Complete |
Paragon MFC-800S | SCSI |  | Complete |
Paragon 800 II SP | SCSI |  | Complete |
Paragon MFS-6000SP | SCSI |  | Complete |
Paragon MFS-8000SP | SCSI |  | Complete |
Paragon MFS-1200SP | SCSI |  | Complete |
Paragon MFS-12000SP | SCSI |  | Complete |
ScanExpress 6000SP | SCSI |  | Complete |
ScanExpress 12000SP | SCSI |  | Complete |
ScanExpress 1200 FS | SCSI |  | Untested | One report that it crashes the computer. SCSI driver issue? Please contact me if you own such a device.
ScanExpress 12000SP Plus | SCSI |  | Complete |
Paragon 1200 III SP | SCSI |  | Complete |
Paragon 1200 LS | SCSI |  | Complete |
ScanMagic 9636S | SCSI |  | Complete |
ScanMagic 9636S Plus | SCSI |  | Complete |
ScanExpress A3 SP | SCSI |  | Basic | Please test!
Paragon 1200 SP Pro | SCSI |  | Good |
Paragon 1200 A3 Pro | SCSI |  | Complete | ADF and TA untested. Please contact me if you own such equipment.
Paragon 600 II N | Proprietary |  | Basic | Resolutions above 300 dpi may cause trouble.
Trust | Imagery 1200 | SCSI |  | Good | 3-pass, Mustek Paragon MFS-6000CX compatible
Imagery 1200 SP | SCSI |  | Complete | Mustek Paragon MFS-6000SP compatible
Imagery 4800 SP | SCSI |  | Complete | Mustek Paragon 600 II CD compatible
SCSI Connect 19200 | SCSI |  | Complete | Mustek ScanExpress 12000SP compatible
SCSI excellence series 19200 | SCSI |  | Complete | Mustek ScanExpress 12000SP compatible
Primax | Compact 4800 SCSI | SCSI |  | Complete | Mustek 600 II CD compatible

### Backend: mustek_pp (13 (unmaintained))

Link(s): http://penguin-breeder.org/sane/mustek_pp/
Manual page: sane-mustek_pp
Comment: Supports CIS and CCD type parallel port scanners from Mustek.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Mustek | ScanExpress 6000 P | Parport (EPP) |  | Good | 300 dpi CCD scanner
ScanExpress 600 SEP | Parport (EPP) |  | Good | 300 dpi CCD scanner
ScanMagic 4800 P | Parport (EPP) |  | Good | 300 dpi CCD scanner
600 III EP Plus | Parport (EPP) |  | Good | 300 dpi CCD scanner
96 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
ScanExpress 600 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
ScanMagic 600 CP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
ScanExpress 1200 CP | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
ScanExpress 1200 CP+ | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
Medion/Lifetec/Tevion/Cytron | MD 9848 | Parport (EPP) |  | Good | 300 dpi CCD scanner
MD 9806 | Parport (EPP) |  | Good | 300 dpi CCD scanner
MD/LT 935x | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
MD/LT 985x | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
MD/LT 9890 | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
Targa | Funline TS12 EP | Parport (EPP) |  | Good | 600x1200 dpi CIS scanner
Funline TS6 EP | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
Trust | Easy Connect 9600+ | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
Easy Connect 19200+ | Parport (EPP) |  | Good | 300x600 dpi CIS scanner
Viviscan | Compact II | Parport (EPP) |  | Good | 300 dpi CCD scanner
Cybercom | 9352 | Parport (EPP) |  | Good | CIS scanner
Gallery | 4800 | Parport (EPP) |  | Good | 300 dpi CCD scanner
Network | Easy Plus 30 Bit | Parport (EPP) |  | Good | 300 dpi CCD scanner
Micromaxx | MM-9851 | Parport (EPP) |  | Good | 300x600 dpi CIS scanner

### Backend: mustek_usb (1.0-18 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/mustek_usb-backend/
Manual page: sane-mustek_usb
Comment: Only the USB scanners mentioned below are supported. For BearPaws, look at the Plustek, MA-1509, and gt68xx backends.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Mustek | ScanExpress 600 CU | USB | 0x055f/0x0002 | Complete |
ScanExpress 1200 CU | USB | 0x055f/0x0001 | Complete |
ScanExpress 1200 CU Plus | USB | 0x055f/0x0008 | Complete |
ScanExpress 1200 UB | USB | 0x055f/0x0006 | Complete | For the UB Plus, see gt68xx backend
Trust | Compact Scan USB 19200 | USB | 0x055f/0x0006 | Complete | Mustek 1200 UB compatible

### Backend: mustek_usb2 (1.0-10 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/mustek_usb2-backend/
Manual page: sane-mustek_usb2
Comment: Only BearPaw 2448TA Pro is supported at the moment

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Mustek | BearPaw 2448TA Pro | USB | 0x055f/0x0409 | Good |

### Backend: nec (0.12 (unmaintained))

Link(s): http://www5a.biglobe.ne.jp/~saetaka/
Manual page: sane-nec

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
NEC | PC-IN500/4C | SCSI |  | Good | PC-IN500/4C was sold only in JAPAN

### Backend: niash (0.3 (unmaintained))

Link(s): http://sourceforge.net/projects/hp3300backend
Manual page: sane-niash

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 3300c | USB | 0x03f0/0x0205 | Complete |
ScanJet 3400c | USB | 0x03f0/0x0405 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary.
ScanJet 4300c | USB | 0x03f0/0x0305 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary.
ScanJet 4300c/Silitek | USB | 0x047b/0x1002 | Complete | If you use Linux 2.6, version 2.6.8 or newer is necessary.
Agfa | Snapscan Touch | USB | 0x06bd/0x0100 | Complete |
Trust | Office Scan USB 19200 | USB | 0x047b/0x1000 | Complete |

### Backend: p5 (1 (unmaintained))

Link(s): http://www.sane-project.org/
Manual page: sane-p5
Comment: New backend for SANE release 1.0.21, see sane-p5 manpage

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
PRIMAX | PagePartner | Parport (EPP/ECP) |  | Basic | Sheetfed scanner, work in gray and color, but uncalibrated scans

### Backend: pie (1.0 (unmaintained))

Link(s): http://www.munton.demon.co.uk/sane
Manual page: sane-pie

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Devcom | 9636PRO | SCSI |  | Good |
9636S | SCSI |  | Untested |
9630S | SCSI |  | Untested |
PIE | ScanAce 1236S | SCSI |  | Good |
ScanAce 1230S | SCSI |  | Good |
ScanAce II | SCSI |  | Untested |
ScanAce III | SCSI |  | Good |
ScanAce Plus | SCSI |  | Untested |
ScanAce II Plus | SCSI |  | Untested |
ScanAce III Plus | SCSI |  | Untested |
ScanAce V | SCSI |  | Untested |
ScanAce ScanMedia | SCSI |  | Untested |
ScanAce ScanMedia II | SCSI |  | Untested |
ScanAce 630S | SCSI |  | Untested |
ScanAce 636S | SCSI |  | Untested |
Adlib | JetScan630 | SCSI |  | Good |
JetScan636PRO | SCSI |  | Untested |

### Backend: pieusb (1.0 (unmaintained))

Link(s): https://github.com/kkaempf/sane-backends
Manual page: sane-pieusb

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
PIE | PowerSlide 3600 | USB | 0x05e3/0x0142 | Untested | Identical to Reflecta DigitDia 3600
PowerSlide 3650 | USB | 0x05e3/0x0142 | Basic | Identical to Reflecta DigitDia 4000
PowerSlide 4000 | USB | 0x05e3/0x0142 | Basic | Identical to Reflecta DigitDia 5000
PowerSlide 5000 | USB | 0x05e3/0x0142 | Basic | Identical to Reflecta DigitDia 6000
Reflecta | Reflecta ProScan 10T | USB | 0x05e3/0x0145 | Basic |
Reflecta ProScan 7200 | USB | 0x05e3/0x0145 | Good | Similar to PrimeFilm 7250 scanner from Pacific Image Electronics
CrystalScan 3600 | USB | 0x05e3/0x0145 | Basic |
CrystalScan 7200 | USB |  | Untested |
Reflecta CrystalScan 7250 | USB | 0x05e3/0x0145 | Basic | Similar to PrimeFilm 7250 scanner from Pacific Image Electronics
DigitDia 3600 | USB | 0x05e3/0x0142 | Untested | Identical to Pacific Image Electronics PowerSlide 3600 scanner
DigitDia 4000 | USB | 0x05e3/0x0142 | Basic | Identical to Pacific Image Electronics PowerSlide 3650 scanner
DigitDia 5000 | USB | 0x05e3/0x0142 | Untested | Identical to Pacific Image Electronics PowerSlide 4000 scanner
Reflecta DigitDia 6000 Multiple Slide Scanner | USB | 0x05e3/0x0142 | Good | Identical to Pacific Image Electronics PowerSlide 5000 scanner

### Backend: pixma (0.17.37)

Manual page: sane-pixma

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Canon | PIXMA E400 | USB | 0x04a9/0x177a | Untested | Testers needed!
PIXMA E460 Series | USB | 0x04a9/0x1788 | Untested | Testers needed!
PIXMA E470 Series | USB | 0x04a9/0x180c | Untested | Testers needed!
PIXMA E480 Series | USB WiFi | 0x04a9/0x1789 | Untested | Testers needed!
PIXMA E500 | USB | 0x04a9/0x1758 | Untested | Testers needed!
PIXMA E510 | USB | 0x04a9/0x1761 | Untested | Testers needed!
PIXMA E560 | USB | 0x04a9/0x177b | Untested | Testers needed!
PIXMA E600 | USB | 0x04a9/0x175a | Untested | Testers needed!
PIXMA E610 | USB | 0x04a9/0x1767 | Untested | Testers needed!
PIXMA G3000 | USB WIFI | 0x04a9/0x181d | Untested | Testers needed!
PIXMA MG2100 Series | USB | 0x04a9/0x1751 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG2200 Series | USB | 0x04a9/0x1760 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG2400 Series | USB | 0x04a9/0x176c | Complete | All resolutions supported (up to 600DPI).
PIXMA MG2500 Series | USB | 0x04a9/0x176d | Complete | All resolutions supported (up to 600DPI).
PIXMA MG2900 Series | USB WiFi | 0x04a9/0x1780 | Complete | All resolutions supported (up to 600DPI).
PIXMA MG3000 Series | USB WiFi | 0x04a9/0x180b | Untested | Testers needed!
PIXMA MG3100 Series | USB WiFi | 0x04a9/0x1752 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG3200 Series | USB WiFi | 0x04a9/0x1762 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG3500 Series | USB WiFi | 0x04a9/0x176e | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG3600 Series | USB Ethernet WiFi | 0x04a9/0x178a | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG4100 Series | USB | 0x04a9/0x1753 | Untested | Testers needed!
PIXMA MG4200 Series | USB | 0x04a9/0x1763 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG5100 Series | USB | 0x04a9/0x1748 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG5200 Series | USB | 0x04a9/0x1749 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG5300 Series | USB | 0x04a9/0x1754 | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG5400 Series | USB WiFi | 0x04a9/0x1764 | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG5500 Series | USB WiFi | 0x04a9/0x1771 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG5600 Series | USB WiFi | 0x04a9/0x177f | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG5700 Series | USB WiFi | 0x04a9/0x178e | Complete | All resolutions supported (up to 1200 DPI).
PIXMA MG6100 Series | USB | 0x04a9/0x174a | Complete | All resolutions supported (up to 2400 DPI)
PIXMA MG6200 Series | USB | 0x04a9/0x1755 | Complete | All resolutions supported (up to 4800 DPI)
PIXMA MG6300 Series | USB Ethernet | 0x04a9/0x1765 | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG6400 Series | USB WiFi | 0x04a9/0x1770 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MG6500 Series | USB | 0x04a9/0x176f | Untested | Testers needed!
PIXMA MG6600 Series | USB | 0x04a9/0x177e | Untested | Testers needed!
PIXMA MG6800 Series | USB WiFi | 0x04a9/0x178d | Untested | Testers needed!
PIXMA MG6900 Series | USB WiFi | 0x04a9/0x178c | Untested | Testers needed!
PIXMA MG7100 Series | USB | 0x04a9/0x1772 | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG7500 Series | USB Ethernet WiFi | 0x04a9/0x177c | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG7700 Series | USB WiFi | 0x04a9/0x178b | Complete | All resolutions supported (up to 2400DPI).
PIXMA MG8100 Series | USB | 0x04a9/0x174b | Untested | Testers needed!
PIXMA MG8200 Series | USB Ethernet | 0x04a9/0x1756 | Complete | All resolutions supported (up to 4800DPI).
PIXUS MP5 | USB | 0x04a9/0x2635 | Untested | Testers needed! Identical with imageCLASS MPC190.
PIXUS MP10 | USB | 0x04a9/0x261f | Complete | All resolutions supported (up to 600DPI). Identical with imageCLASS MPC200.
PIXMA MP140 | USB | 0x04a9/0x172b | Complete | All resolutions supported (up to 600 DPI)
PIXMA MP150 | USB | 0x04a9/0x1709 | Good |
PIXMA MP160 | USB | 0x04a9/0x1714 | Basic |
PIXMA MP170 | USB | 0x04a9/0x170a | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP180 | USB | 0x04a9/0x1715 | Basic |
PIXMA MP190 | USB | 0x04a9/0x1734 | Complete | All resolutions supported (up to 600DPI)
PIXMA MP210 | USB | 0x04a9/0x1721 | Complete | All resolutions supported (up to 600DPI)
PIXMA MP220 | USB | 0x04a9/0x1722 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP230 | USB | 0x04a9/0x175f | Complete | All resolutions supported (up to 600DPI).
PIXMA MP240 | USB | 0x04a9/0x1732 | Complete | All resolutions supported (up to 1200DPI)
PIXMA MP250 | USB | 0x04a9/0x173a | Complete | All resolutions supported (up to 600DPI)
PIXMA MP260 | USB | 0x04a9/0x1733 | Complete | All resolutions supported (up to 1200DPI)
PIXMA MP270 | USB | 0x04a9/0x173b | Complete | All resolutions supported (up to 1200DPI)
PIXMA MP280 | USB | 0x04a9/0x1746 | Good | All resolutions supported (up to 600DPI).
PIXMA MP360 | USB | 0x04a9/0x263c | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP370 | USB | 0x04a9/0x263d | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP375R | USB | 0x04a9/0x263f | Untested | Same protocol as Pixma MP360/370/390? Testers needed!
PIXMA MP390 | USB | 0x04a9/0x263e | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP450 | USB | 0x04a9/0x170b | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP460 | USB | 0x04a9/0x1716 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP470 | USB | 0x04a9/0x1723 | Complete | All resolutions supported (up to 2400DPI).
PIXMA MP480 | USB | 0x04a9/0x1731 | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP490 | USB | 0x04a9/0x173c | Complete | All resolutions supported (up to 1200DPI)
PIXMA MP493 | USB | 0x04a9/0x1757 | Untested | Testers needed!
PIXMA MP495 | USB | 0x04a9/0x1747 | Untested | Same protocol as Pixma MP280? Testers needed!
PIXMA MP500 | USB | 0x04a9/0x170c | Good |
PIXMA MP510 | USB | 0x04a9/0x1717 | Complete | All resolutions supported (up to 1200DPI).
PIXMA MP520 | USB | 0x04a9/0x1724 | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP530 | USB | 0x04a9/0x1712 | Good |
PIXMA MP540 | USB | 0x04a9/0x1730 | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP550 | USB | 0x04a9/0x173d | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP560 | USB | 0x04a9/0x173e | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP600 | USB | 0x04a9/0x1718 | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP600R | USB Ethernet | 0x04a9/0x1719 | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP610 | USB | 0x04a9/0x1725 | Complete | All resolutions supported (up to 4800DPI)
PIXMA MP620 | USB Ethernet | 0x04a9/0x172f | Complete | All resolutions supported (up to 2400DPI)
PIXMA MP630 | USB | 0x04a9/0x172e | Complete | All resolutions supported (up to 4800DPI)
PIXMA MP640 | USB Ethernet | 0x04a9/0x173f | Complete | All resolutions supported (up to 4800DPI)
PIXMA MP700 | USB | 0x04a9/0x2630 | Complete | All resolutions supported (flatbed color up to 1200DPI, grayscale up to 600DPI).
PIXMA MP710 | USB | 0x04a9/0x264d | Complete | All resolutions supported (up to 1200DPI)
PIXMA MP730 | USB | 0x04a9/0x262f | Good | Flatbed color up to 1200DPI, grayscale up to 600DPI. ADF scan to be confirmed.
PIXMA MP740 | USB | 0x04a9/0x264c | Untested | Same protocol as Pixma MP710? Testers needed!
PIXMA MP750 | USB | 0x04a9/0x1706 | Minimal | No grayscale. Canceling scan in ADF mode doesn't eject the paper!
PIXMA MP760 | USB | 0x04a9/0x1708 | Minimal | No grayscale. The scanner sometimes hangs!
PIXMA MP770 | USB | 0x04a9/0x1708 | Minimal | No grayscale. The scanner sometimes hangs!
PIXMA MP780 | USB | 0x04a9/0x1707 | Minimal | No grayscale. The scanner sometimes hangs!
PIXMA MP790 | USB | 0x04a9/0x1707 | Minimal | No grayscale. The scanner sometimes hangs!
PIXMA MP800 | USB | 0x04a9/0x170d | Complete | All resolutions supported up to 2400DPI. Full TPU support up to 2400DPI.
PIXMA MP800R | USB | 0x04a9/0x170e | Complete | All resolutions supported up to 2400DPI. Full TPU support up to 2400DPI.
PIXMA MP810 | USB | 0x04a9/0x171a | Complete | All resolutions supported up to 4800DPI. Full TPU support (negative and slides) up to 4800DPI.
PIXMA MP830 | USB | 0x04a9/0x1713 | Complete | All resolutions supported up to 2400DPI. Flatbed, ADF simplex and Duplex supported.
PIXMA MP960 | USB | 0x04a9/0x171b | Complete | All resolutions supported up to 4800DPI. Full TPU support (negative and slides) up to 4800DPI.
PIXMA MP970 | USB Ethernet | 0x04a9/0x1726 | Complete | All resolutions supported (up to 4800DPI). Full TPU support (negative and slides) at 24 or 48 bits.
PIXMA MP980 | USB Ethernet | 0x04a9/0x172d | Complete | Working fine at all resolutions.
PIXMA MP990 | USB Ethernet | 0x04a9/0x1740 | Complete | Working fine at all resolutions.
PIXMA MX300 | USB | 0x04a9/0x1727 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
PIXMA MX310 | USB | 0x04a9/0x1728 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI)
PIXMA MX320 | USB | 0x04a9/0x1736 | Untested | Same protocol as Pixma Generation 3? Testers needed!
PIXMA MX330 | USB | 0x04a9/0x1737 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI)
PIXMA MX340 | USB | 0x04a9/0x1741 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI)
PIXMA MX350 | USB Ethernet | 0x04a9/0x1742 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI)
PIXMA MX360 | USB | 0x04a9/0x174d | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX370 Series | USB | 0x04a9/0x1759 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX390 Series | USB | 0x04a9/0x1766 | Untested | Testers needed!
PIXMA MX410 | USB Ethernet WiFi | 0x04a9/0x174e | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX420 | USB Ethernet | 0x04a9/0x174f | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX430 Series | USB Ethernet | 0x04a9/0x175b | Untested | Testers needed!
PIXMA MX450 Series | USB | 0x04a9/0x1768 | Untested | Testers needed!
PIXMA MX470 Series | USB Ethernet | 0x04a9/0x1774 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX490 Series | USB WiFi | 0x04a9/0x1787 | Untested | Testers needed!
PIXMA MX510 Series | USB Ethernet | 0x04a9/0x175c | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX520 Series | USB Ethernet WiFi | 0x04a9/0x1769 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX530 Series | USB WiFi | 0x04a9/0x1775 | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
PIXMA MX700 | USB Ethernet | 0x04a9/0x1729 | Complete | Flatbed and ADF scan. All resolutions supported (up to 2400DPI)
PIXMA MX710 Series | USB Ethernet | 0x04a9/0x175d | Untested | Testers needed!
PIXMA MX720 Series | USB Ethernet WiFi | 0x04a9/0x176a | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX850 | USB Ethernet | 0x04a9/0x172c | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX860 | USB Ethernet | 0x04a9/0x1735 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX870 | USB Ethernet | 0x04a9/0x1743 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX880 Series | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX882 | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX885 | USB Ethernet | 0x04a9/0x1750 | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX890 Series | USB Ethernet | 0x04a9/0x175e | Complete | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX920 Series | USB Ethernet WiFi | 0x04a9/0x176b | Good | All resolutions supported (up to 2400DPI). Flatbed, ADF simplex and Duplex supported.
PIXMA MX7600 | USB Ethernet | 0x04a9/0x171c | Complete | Flatbed and ADF scan. All resolutions supported (up to 4800DPI)
PIXMA TS9000 Series | USB WiFi | 0x04a9/0x179f | Untested | Testers needed!
PIXMA TS8000 Series | USB WiFi | 0x04a9/0x1800 | Untested | Testers needed!
PIXMA TS6000 Series | USB WiFi | 0x04a9/0x1801 | Untested | Testers needed!
PIXMA TS5000 Series | USB WiFi | 0x04a9/0x1802 | Untested | Testers needed!
imageCLASS D420 | USB | 0x04a9/0x26ef | Complete | All resolutions supported (up to 600DPI). Flatbed, ADF simplex and Duplex supported.
imageCLASS D480 | USB | 0x04a9/0x26ed | Complete | All resolutions supported (up to 600DPI). Flatbed, ADF simplex and Duplex supported.
imageCLASS D530 | USB | 0x04a9/0x2775 | Complete | All resolutions supported (up to 600DPI)
i-SENSYS MF210 Series | USB Ethernet WiFi | 0x04a9/0x27a9 | Untested | Testers needed!
i-SENSYS MF220 Series | USB Ethernet WiFi | 0x04a9/0x27a8 | Untested | Testers needed!
i-SENSYS MF230 Series | USB WiFi | 0x04a9/0x27d1 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). WiFi only for w Types.
i-SENSYS MF240 Series | USB Ethernet WiFi | 0x04a9/0x27d2 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). ADF only 300DPI.
i-SENSYS MF810/820 | USB Ethernet | 0x04a9/0x27a6 | Untested | Testers needed!
i-SENSYS MF3010 | USB Ethernet | 0x04a9/0x2759 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF3110 | USB | 0x04a9/0x2660 | Complete | All resolutions supported (up to 600DPI).
imageCLASS MF3240 | USB | 0x04a9/0x2684 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4010 | USB | 0x04a9/0x26b4 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4018 | USB | 0x04a9/0x26b4 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4120 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4122 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4140 | USB | 0x04a9/0x26a3 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4150 | USB | 0x04a9/0x26a3 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageCLASS MF4270 | USB | 0x04a9/0x26b5 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
I-SENSYS MF4320d | USB | 0x04a9/0x26ee | Complete | All resolutions supported (up to 600DPI)
I-SENSYS MF4330d | USB | 0x04a9/0x26ee | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageCLASS MF4350d | USB | 0x04a9/0x26ee | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageCLASS MF4370dn | USB | 0x04a9/0x26ec | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Network not supported
imageCLASS MF4380dn | USB | 0x04a9/0x26ec | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Network not supported
imageCLASS MF4410 | USB | 0x04a9/0x2737 | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4430 | USB | 0x04a9/0x2737 | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI). ADF empty buggy.
i-SENSYS MF4500 Series | USB | 0x04a9/0x2736 | Good | Flatbed and ADF scan. All resolutions supported (up to 600DPI).
imageCLASS MF4570dw | USB | 0x04a9/0x275a | Complete | All resolutions supported (up to 600DPI)
imageCLASS MF4660 | USB | 0x04a9/0x26b0 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageCLASS MF4690 | USB | 0x04a9/0x26b0 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
i-SENSYS MF4700 Series | USB Ethernet | 0x04a9/0x2774 | Good | Flatbed scan. All resolutions supported (up to 600DPI). ADF buggy.
i-SENSYS MF4800 Series | USB Ethernet | 0x04a9/0x2773 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Ethernet buggy.
imageCLASS MF5630 | USB | 0x04a9/0x264e | Untested | Testers needed!
laserBase MF5650 | USB | 0x04a9/0x264f | Untested | Testers needed!
imageCLASS MF5730 | USB | 0x04a9/0x265d | Complete | Flatbed and ADF scan. All resolutions supported (up to 1200DPI).
imageCLASS MF5750 | USB | 0x04a9/0x265e | Untested | Testers needed!
imageCLASS MF5770 | USB | 0x04a9/0x265f | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI).
i-SENSYS MF5880dn | USB | 0x04a9/0x26f9 | Untested | Testers needed!
i-SENSYS MF5900 Series | USB Ethernet | 0x04a9/0x2743 | Untested | Testers needed!
i-SENSYS MF6100 Series | USB Ethernet | 0x04a9/0x278e | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Note: document feeder does not have 600DPI capability.
imageCLASS MF6500 Series | USB | 0x04a9/0x2686 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageCLASS MF6550 | USB | 0x04a9/0x2686 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
i-SENSYS MF6680dn | USB | 0x04a9/0x26fa | Untested | Testers needed!
imageCLASS MF8030 | USB | 0x04a9/0x2707 | Untested | Testers needed!
imageCLASS MF8170c | USB | 0x04a9/0x2659 | Untested | Testers needed!
i-SENSYS MF8200C Series | USB Ethernet | 0x04a9/0x2779 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI). Note: document feeder does not have 600DPI capability.
i-SENSYS MF8300 Series | USB Ethernet | 0x04a9/0x2708 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI).
i-SENSYS MF8500C Series | USB Ethernet | 0x04a9/0x277a | Untested | Same protocol as MF8200C Series? Testers needed!
imageCLASS MPC190 | USB | 0x04a9/0x2635 | Untested | Testers needed! Identical with SmartBase MPC190 and PIXUS MP5.
imageCLASS MPC200 | USB | 0x04a9/0x261f | Complete | All resolutions supported (up to 600DPI). Identical with SmartBase MPC200 and PIXUS MP10.
imageRUNNER 1020/1024/1025 | USB | 0x04a9/0x26e6 | Complete | Flatbed and ADF scan. All resolutions supported (up to 600DPI)
imageRUNNER 1133 | USB | 0x04a9/0x2742 | Untested | Testers needed!
MAXIFY MB2000 Series | USB | 0x04a9/0x1778 | Untested | Testers needed!
MAXIFY MB2300 Series | USB | 0x04a9/0x1779 | Untested | Testers needed!
MAXIFY MB5000 Series | USB | 0x04a9/0x1776 | Complete | Flatbed works, All resolutions supported (up to 1200DPI), ADF does not work
MAXIFY MB5300 Series | USB | 0x04a9/0x1777 | Untested | Testers needed!
CanoScan 8800F | USB | 0x04a9/0x1901 | Complete | Flatbed scan. TPU for negatives and slides. All resolutions supported (up to 4800DPI).
CanoScan 9000F | USB | 0x04a9/0x1908 | Complete | Full flatbed support up to 4800DPI (Note: flatbed does not have 9600DPI capability). Full TPU support (negatives, slides and infrared) up to 9600DPI.
CanoScan 9000F Mark II | USB | 0x04a9/0x190d | Complete | Full flatbed support up to 4800DPI (Note: flatbed does not have 9600DPI capability). Full TPU support (negatives, slides and infrared) up to 9600DPI.

### Backend: plustek (0.52)

Link(s): http://www.gjaeger.de/scanner/plustek/
Manual page: sane-plustek

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Plustek | OpticPro U12 | USB | 0x07b3/0x0010 | Complete | NOTE: Devices with product ID 0x0001 are not supported!
OpticPro UT12 | USB | 0x07b3/0x0013 | Complete |
OpticPro UT12 | USB | 0x07b3/0x0017 | Complete | Note: Devices with product ID 0x0001 are not supported!
OpticPro UT16 | USB | 0x07b3/0x0017 | Complete |
OpticPro U24 | USB | 0x07b3/0x0011 | Complete |
OpticPro U24 | USB | 0x07b3/0x0015 | Complete |
OpticPro UT24 | USB | 0x07b3/0x0017 | Complete |
Genius | Colorpage HR6 V2 | USB | 0x0458/0x2007 | Complete |
Colorpage HR6 V2 | USB | 0x0458/0x2008 | Complete |
Colorpage HR7 | USB | 0x0458/0x2013 | Complete |
Colorpage HR6A | USB | 0x0458/0x2009 | Untested |
Colorpage HR7LE | USB | 0x0458/0x2015 | Untested |
Colorpage HR6X | USB | 0x0458/0x2016 | Untested |
Mustek | BearPaw 1200 | USB | 0x0400/0x1000 | Complete | both product versions are supported, see backends' man-page
BearPaw 1200 | USB | 0x0400/0x1001 | Complete | both product versions are supported, see backends' man-page
BearPaw 2400 | USB | 0x0400/0x1001 | Complete |
Hewlett-Packard | ScanJet 2100C | USB | 0x03f0/0x0505 | Complete |
ScanJet 2200C | USB | 0x03f0/0x0605 | Complete |
Epson | Perfection 1250 | USB | 0x04b8/0x010f | Complete |
Perfection 1250Photo | USB | 0x04b8/0x010f | Good | TPA scans not perfect
Perfection 1260 | USB | 0x04b8/0x011d | Complete |
Perfection 1260Photo | USB | 0x04b8/0x011d | Good | TPA scans not perfect
Umax | UMAX 3400 | USB | 0x1606/0x0050 | Complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x
UMAX 3400 | USB | 0x1606/0x0060 | Complete | there are some UMAX 3400 outside the U.S. which are not supported, as they use another chipset than the LM983x
UMAX Astranet ia101 | USB | 0x1606/0x0060 | Complete | seems to be a renamed UMAX 3400
UMAX 3450 | USB | 0x1606/0x0060 | Complete |
UMAX 5400 | USB | 0x1606/0x0160 | Complete |
Compaq | S4-100 | USB | 0x049f/0x001a | Complete | Identical to UMAX 3400
Canon | CanoScan N650U/N656U | USB | 0x04a9/0x2206 | Complete |
CanoScan N1220U | USB | 0x04a9/0x2207 | Complete |
CanoScan N670U/N676U/LiDE20 | USB | 0x04a9/0x220d | Complete |
CanoScan N1240U/LiDE30 | USB | 0x04a9/0x220e | Complete |
CanoScan LiDE25 | USB | 0x04a9/0x2220 | Good |
CanoScan D660U | USB | 0x04a9/0x2208 | Good | TPA scans not perfect
Syscan | TravelScan 460/464 | USB | 0x0a82/0x4600 | Complete |
TravelScan 662 | USB | 0x0a82/0x6620 | Complete |
Ambir | Visigo A4 | USB | 0x0a82/0x4600 | Complete | Rebaged Travelscan 464
Portable Peripheral Co., Ltd. | Q-Scan USB001 (A4 portable scanner) | USB | 0x0a53/0x1000 | Complete |
Q-Scan USB201 (A6 portable scanner) | USB | 0x0a53/0x2000 | Good |
Visioneer | Strobe XP 100 | USB | 0x04a7/0x0427 | Basic |

### Backend: plustek_pp (0.43)

Link(s): http://www.gjaeger.de/scanner/plustek_pp/
Manual page: sane-plustek_pp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Plustek | OpticPro 4800P | Parport (SPP, EPP) |  | Complete |
OpticPro 4830P | Parport (SPP, EPP) |  | Complete |
OpticPro 600P/6000P | Parport (SPP, EPP) |  | Complete |
OpticPro 4831P | Parport (SPP, EPP) |  | Complete |
OpticPro 9630P | Parport (SPP, EPP) |  | Complete |
OpticPro 9630PL | Parport (SPP, EPP) |  | Complete | use driver-switch mov=1
OpticPro 9600P | Parport (SPP, EPP) |  | Complete |
OpticPro 1236P | Parport (SPP, EPP) |  | Complete | reported as OpticPro 12000P/96000P
OpticPro 12000P/96000P | Parport (SPP, EPP) |  | Complete |
OpticPro 9636P | Parport (SPP, EPP) |  | Complete | use driver-switch mov=4
OpticPro 9636P+/Turbo | Parport (SPP, EPP) |  | Complete | use driver-switch mov=3
OpticPro 9636T | Parport (SPP, EPP) |  | Complete |
OpticPro 12000T | Parport (SPP, EPP) |  | Complete |
OpticPro AI3 | Parport (SPP, EPP) |  | Basic | use driver-switch mov=5, poor picture quality
OpticPro P8 | Parport |  | Untested |
OpticPro P12 | Parport (SPP, EPP) |  | Complete |
OpticPro PT12 | Parport (SPP, EPP) |  | Complete |
Primax | Colorado 4800 | Parport (SPP, EPP) |  | Untested | same as OpticPro 4800P
Compact 4800 Direct | Parport (SPP, EPP) |  | Complete | use driver-switch mov=2
Compact 4800 Direct-30 | Parport (SPP, EPP) |  | Complete | same as OpticPro 4830P, use driver-switch mov=7
Compact 9600 Direct-30 | Parport (SPP, EPP) |  | Complete | same as OpticPro 9630P
Genius | Colorpage Vivid III V2 | Parport (SPP, EPP) |  | Complete | Reported as PT12
Colorpage Vivid Pro II Film | Parport (SPP, EPP) |  | Complete | Reported as OP9636T/12000T
Colorpage HR6X EPP | Parport (SPP, EPP) |  | Good | Negative scanning does not work correctly
Aries | Scan-It Pro 4800 | Parport (SPP, EPP) |  | Complete | use driver-switch mov=2
BrightScan | BrighScan OpticPro | Parport (SPP, EPP) |  | Complete | Reported as P12

### Backend: ricoh (unmaintained)

Manual page: sane-ricoh

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Ricoh | Ricoh IS50 | SCSI |  | Basic |
Ricoh IS60 | SCSI |  | Basic |

### Backend: rts8891 (1.0-0 (unmaintained))

Link(s): http://stef.dev.free.fr/sane/rts8891/index.html
Manual page: sane-rts8891
Comment: This backend supports Realtek RTS8891 ASIC bases scanners.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
UMAX | Astra 4400 | USB | 0x1606/0x0070 | Good | Supports 75, 150, 300, 600 and 1200 dpi
Astra 4450 | USB | 0x1606/0x0070 | Untested |
Hewlett-Packard | scanjet 4470c | USB | 0x03f0/0x0805 | Good | re-branded Astra 4400
scanjet 4400c | USB | 0x03f0/0x0705 | Good | exists with 2 different sensors of which only one works

### Backend: s9036 (unmaintained)

Manual page: sane-s9036

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Siemens | 9036 Flatbed scanner | SCSI |  | Basic |

### Backend: sceptre (1.0-10 (unmaintained))

Link(s): http://www.zago.net/sane/
Manual page: sane-sceptre

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Sceptre | Vividscan S1200 | SCSI |  | Basic |
Komodo | S1200 | SCSI |  | Untested | rebadged Sceptre S1200

### Backend: sharp (0.32 (unmaintained))

Link(s): http://www.satzbau-gmbh.de/staff/abel/sane-sharp.html
Manual page: sane-sharp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Sharp | JX-610 | SCSI |  | Good |
JX-250 | SCSI |  | Good |
JX-320 | SCSI |  | Good |
JX-325 | SCSI |  | Untested |
JX-330 | SCSI |  | Good |
JX-350 | SCSI |  | Good |

### Backend: sm3600 (0.1 (unmaintained))

Link(s): http://sm3600.sourceforge.net/
Manual page: sane-sm3600

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Microtek | ScanMaker 3600 | USB | 0x05da/0x40b3 | Basic | works
ScanMaker 3600 | USB | 0x05da/0x40ca | Basic | works
ScanMaker 3600 | USB | 0x05da/0x40ff | Basic | works
ScanMaker 3700 | USB | 0x05da/0x40b8 | Basic | works
ScanMaker 3700 | USB | 0x05da/0x40cb | Basic | works
ScanMaker 3750 | USB | 0x05da/0x40dd | Basic | works (told)

### Backend: sm3840 (1.1 (unmaintained))

Link(s): http://www.ziplabel.com/sm3840/
Manual page: sane-sm3840
Comment: This reverse-engineered backend supports the USB ScanMaker 3840 model

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Microtek | ScanMaker 3840 | USB | 0x05da/0x30d4 | Good | 8 and 16 bit, color and grayscale
ScanMaker 4800 | USB | 0x05da/0x30cf | Good | Same hardware as SM3840, different color box

### Backend: SnapScan (1.4)

Link(s): http://snapscan.sourceforge.net/
Manual page: sane-snapscan
Comment: Supported bit depths: 24 bit (color), 48 bit (color, Epson) 8 bit (gray)

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
AGFA | SnapScan | SCSI |  | Good |
SnapScan 300 | SCSI |  | Good |
SnapScan 310 | SCSI |  | Good |
SnapScan 600 | SCSI |  | Good | Optional ADF supported.
Arcus 1200 | SCSI |  | Good | Optional transparency unit supported.
SnapScan 1236s | SCSI |  | Good | Optional ADF and transparency unit supported.
SnapScan 1236u | USB | 0x06bd/0x0002 | Good | Optional ADF and transparency unit supported.
SnapScan 1212U | USB | 0x06bd/0x0001 | Good |
SnapScan 1212U_2 | USB | 0x06bd/0x2061 | Good |
SnapScan e10 | USB | 0x06bd/0x2093 | Good |
SnapScan e20 | USB | 0x06bd/0x2091 | Good |
SnapScan e25 | USB | 0x06bd/0x2095 | Good |
SnapScan e26 | USB | 0x06bd/0x2097 | Good |
SnapScan e40 | USB | 0x06bd/0x208d | Good |
SnapScan e42 | USB | 0x06bd/0x20ff | Good |
SnapScan e50 | USB | 0x06bd/0x208f | Good | Optional tranparency unit supported
SnapScan e52 | USB | 0x06bd/0x20fd | Good | Optional tranparency unit supported
SnapScan e60 | USB |  | Untested |
Benq (Acer) | 300f | SCSI |  | Good |
310s | SCSI |  | Good |
610s | SCSI |  | Good |
610plus | SCSI |  | Good |
620s | SCSI |  | Good |
ScanWit 2720s | SCSI |  | Good |
310U | USB | 0x04a5/0x1a20 | Good |
320U | USB | 0x04a5/0x2022 | Good |
340U | USB | 0x04a5/0x2022 | Good |
620U | USB | 0x04a5/0x1a2a | Good | Optional tranparency unit supported
620UT | USB | 0x04a5/0x2040 | Good | Optional tranparency unit supported
640U | USB | 0x04a5/0x2060 | Good | Optional tranparency unit supported
640bu | USB | 0x04a5/0x207e | Good |
640BT | USB | 0x04a5/0x20be | Good | Optional tranparency unit supported
1240 | USB | 0x04a5/0x20c0 | Good | Optional tranparency unit supported
3300 | USB | 0x04a5/0x20b0 | Good |
3300 | USB | 0x04a5/0x20de | Good |
4300 | USB | 0x04a5/0x20b0 | Good |
4300 | USB | 0x04a5/0x20de | Good |
5000E | USB | 0x04a5/0x20fc | Basic | Same as 5000U, working up to 600 DPI
5000U | USB | 0x04a5/0x20fc | Basic | Same as 5000E, working up to 600 DPI
5000 | USB | 0x04a5/0x20f8 | Good | USB ID 0x04a5,0x20f8: Color / grayscale scans working up to 1200 DPI
5150 | USB | 0x04a5/0x2137 | Basic | Calibration algorithm unknown
5250 | USB | 0x04a5/0x2137 | Basic | Same hardware as 5150 (?), Calibration algorithm unknown
5300 | USB | 0x04a5/0x20fe | Basic | Problems with firmware upload reported
Guillemot / Hercules | Maxi Scan A4 Deluxe (SCSI) | SCSI |  | Good | Rebadged SnapScan 310s.
Scan@home Touch 1248 (USB) | USB | 0x04a5/0x20de | Good | Rebadged Benq 3300.
Maxi Scan A4 USB 640U | USB | 0x04a5/0x2060 | Good | Rebadged Benq 640U.
Maxi A4 36 bit | USB | 0x04a5/0x2060 | Good | Rebadged Benq 620U, needs Benq firmware file u96v???.bin
Mitsubishi | Diamondview 648UT | USB | 0x04a5/0x2022 | Good | Rebadged Benq 320u.
Diamondview 650U | USB | 0x04a5/0x20b0 | Good | Rebadged Benq 4300.
Epson | Perfection 660 | USB | 0x04b8/0x0114 | Good |
Perfection 1270 | USB | 0x04b8/0x0120 | Good |
Perfection 1670 | USB | 0x04b8/0x011f | Good |
Perfection 2480 | USB | 0x04b8/0x0121 | Good |
Perfection 2580 | USB | 0x04b8/0x0121 | Basic | Film scanning unit unsupported
Perfection 3490 | USB | 0x04b8/0x0122 | Good |
Perfection 3590 | USB | 0x04b8/0x0122 | Basic | Film scanning unit unsupported
Stylus CX-1500 | USB | 0x04b8/0x080c | Good |

### Backend: sp15c (unmaintained)

Manual page: sane-sp15c

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Fujitsu | ScanPartner 15C | SCSI |  | Good |
ScanPartner 600C | SCSI |  | Good |

### Backend: st400 (1.6 (unmaintained))

Link(s): http://www.informatik.uni-oldenburg.de/~ingo/sane/
Manual page: sane-st400

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Siemens | ST400 | SCSI |  | Basic | 6 bit gray
ST800 | SCSI |  | Basic | 6 bit gray

### Backend: tamarack (unmaintained)

Manual page: sane-tamarack

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Tamarack | Artiscan 6000C | SCSI |  | Good | 3 pass, 300 DPI
Artiscan 8000C | SCSI |  | Good | 3 pass, 400 DPI
Artiscan 12000C | SCSI |  | Good | 3 pass, 600 DPI

### Backend: teco1 (1.0-10 (unmaintained))

Link(s): http://www.zago.net/sane/#teco
Manual page: sane-teco1

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Relisys | RELI 2412 | SCSI |  | Complete | sub model VM3530+
AVEC 2400 | SCSI |  | Complete | sub model VM3520
RELI 4830 | SCSI |  | Good | sub model VM4542
AVEC 2412 | SCSI |  | Complete | sub model VM3520+
AVEC 4800 | SCSI |  | Untested | sub model VM4530
AVEC 4816 | SCSI |  | Untested | sub model VM4530+
RELI DS6 | SCSI |  | Untested | sub model VM3420
RELI DS15 | SCSI |  | Untested | sub model VM3440
RELI 2400 | SCSI |  | Untested | sub model VM3530
RELI 4816 | SCSI |  | Complete | sub model VM4540
RELI 9600 | SCSI |  | Untested | sub model VM6530
RELI 9612 | SCSI |  | Untested | sub model VM6530*
RELI 9624 | SCSI |  | Untested | sub model VM6530+
RELI 9630 | SCSI |  | Untested | sub model VM6540
Actown | ACT Scan I 30 | SCSI |  | Untested | sub model VM3520A
Dextra | DF-600P | SCSI |  | Good | sub model VM3510
DF-1200T+ | SCSI |  | Untested | sub model VM3530+
DF-4830T | SCSI |  | Untested | sub model VM4542
DF-9624 | SCSI |  | Untested | sub model VM6530+

### Backend: teco2 (1.0-9 (unmaintained))

Link(s): http://gkall.hobby.nl/teco2.html
Manual page: sane-teco2

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Relisys | AVEC Super 3 | SCSI |  | Untested | sub model VM3575
AVEC II S3 | SCSI |  | Good | sub model VM3564
SCORPIO Super 3 | SCSI |  | Good | sub model VM3575
APOLLO Express 3 | SCSI |  | Basic | sub model VM356A
APOLLO Express 6 | SCSI |  | Good | sub model VM6565
SCORPIO Pro | SCSI |  | Good | sub model VM6575
SCORPIO Pro-S | SCSI |  | Untested | sub model VM6586
Primax | Jewel 4800 | SCSI |  | Good | sub model VM356A
Profi 9600 | SCSI |  | Basic | sub model VM6575
Profi 19200 | SCSI |  | Good | sub model VM6586
Mustek | ScanMagic 4830S | SCSI |  | Untested | sub model VM3575

### Backend: teco3 (1.0-1 (unmaintained))

Link(s): http://www.zago.net/sane/#teco3
Manual page: sane-teco3

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Relisys | Infinity Scorpio | SCSI |  | Good | sub model VM3552
Plustek | OpticPro 2400SP | SCSI |  | Untested | sub model VM3552
PIOTECH | Splendeur 3024 | SCSI |  | Good | sub model VM3552
Trust | Imagery 2400 SP | SCSI |  | Good | sub model VM3552
Imagery 4800 SP+ | SCSI |  | Good | sub model VM3552
Imagery 9600 SP | SCSI |  | Untested | sub model VM3552

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
TemPlate | Templ Z | SCSI | 0x1234/0x4321 | Untested | With Z-Axis scrolling
Templ ZS | USB | 0x1234/0x4322 | Unsupported | No support yet, but we have docs.
Templ ZQ | USB | 0x1234/0x4323 | Minimal |
Templ ZY | SCSI |  | Basic |
Templ ZZ | SCSI |  | Good |
ArmorPlate | AmplScan II | SCSI |  | Complete | AmplScan *II*, not AmplScan!

### Backend: u12 (0.02)

Link(s): http://www.gjaeger.de/scanner/u12/
Manual page: sane-u12

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Plustek | OpticPro U12 | USB | 0x07b3/0x0001 | Basic | Note: Only devices with product ID 0x0001 are supported!
OpticPro UT12 | USB | 0x07b3/0x0001 | Basic | Note: Only devices with product ID 0x0001 are supported!
OpticPro 1212U | USB | 0x07b3/0x0001 | Basic |
RevScan | RevScan Orange R48Ti | USB | 0x07b3/0x0001 | Basic | Rebadged Plustek OpticPro UT12
Genius | ColorPage HR6 V1 | USB | 0x0458/0x2004 | Basic |
ColorPage Vivid III USB | USB | 0x07b3/0x0001 | Untested | Note: Device has Plustek vendor and product ID (0x07b3/0x0001)

### Backend: umax (1.0-41 (unmaintained))

Link(s): http://www.rauch-domain.de/sane-umax/index.html
Manual page: sane-umax

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
UMAX | Vista S6 | SCSI |  | Good | OK
Vista S6E | SCSI |  | Good | OK
UMAX S-6E | SCSI |  | Good | OK
UMAX S-6EG | SCSI |  | Good | OK
Vista-S8 | SCSI |  | Good | OK
Supervista S-12 | SCSI |  | Good | OK
UMAX S-12 | SCSI |  | Good | OK
UMAX S-12G | SCSI |  | Good | OK
Astra 600S | SCSI |  | Good | OK
Astra 610S | SCSI |  | Good | OK
Astra 1200S | SCSI |  | Good | OK
Astra 1220S | SCSI |  | Good | OK
Astra 2100S | SCSI |  | Good | OK
Astra 2200 (SU) | SCSI |  | Good | OK
Astra 2200 (SU) | USB | 0x1606/0x0230 | Good | OK, needs USB control messages
Astra 2400S | SCSI |  | Good | OK
Astra 6400 | IEEE-1394 |  | Unsupported | will probably work one day
Astra 6450 | IEEE-1394 |  | Unsupported | will probably work one day
Astra MX3 | SCSI |  | Good | OK
Astra MX3 | USB |  | Good | OK, needs USB control messages
Mirage D-16L | SCSI |  | Good | OK
Mirage II | SCSI |  | Good | OK
Mirage IIse | SCSI |  | Good | OK
PSD | SCSI |  | Good | OK
PowerLook | SCSI |  | Good | OK, SCSI-ID=PS-2400X
PL-II | SCSI |  | Good | OK
PowerLook III | SCSI |  | Good | OK
PowerLook 270 | SCSI |  | Unsupported | incompatible
PowerLook 270plus | SCSI |  | Unsupported | incompatible
PowerLook 1100 | IEEE-1394 |  | Unsupported | will probably work one day
PowerLook 2000 | SCSI |  | Good | OK
PowerLook 2100XL | SCSI |  | Good | OK
PowerLook 3000 | SCSI |  | Good | OK
Gemini D-16 | SCSI |  | Good | OK
UMAX VT600 | SCSI |  | Untested | may work, please test and give feedback
Vista-T630 | SCSI |  | Good | OK for some firmwareversions, on others only lineart OK
UC 630 | SCSI |  | Good | Version 2.8 OK, others only lineart OK
UG 630 | SCSI |  | Good | OK
UG 80 | SCSI |  | Good | OK
UC 840 | SCSI |  | Good | Version 1.6 OK, others only lineart OK
UC 1200S | SCSI |  | Untested | may work, please test and give feedback
UC 1200SE | SCSI |  | Good | Version 3.0 OK, others unknown
UC 1260 | SCSI |  | Good | Version 1.6 OK, others unknown
Linotype Hell | Jade | SCSI |  | Good | OK, SCSI-ID=LinoHell Office
Jade | SCSI |  | Good | OK, SCSI-ID=LinoHell JADE
Jade2 | SCSI |  | Good | OK, SCSI-ID=LinoHell Office2
Saphir | SCSI |  | Untested | support disabled until tested - please contact author
Saphir2 | SCSI |  | Good | OK, SCSI-ID=LinoHell SAPHIR2
Saphir3 | SCSI |  | Good | OK, SCSI-ID=LinoHell SAPHIR3
Saphir Ultra | SCSI |  | Untested | support disabled until tested - please contact author
Saphir Ultra II | SCSI |  | Good | OK, SCSI-ID=Linotype SAPHIR4
Saphir HiRes | SCSI |  | Untested | support disabled until tested - please contact author
Opal | SCSI |  | Untested | support disabled until tested - please contact author
Opal2 | SCSI |  | Good | OK; SCSI-ID=LinoHell OPAL2
Opal Ultra | SCSI |  | Untested | support disabled until tested - please contact author
Linoscan 1400 | SCSI |  | Good | OK, SCSI-ID=HDM LS4H1S
Vobis | Highscreen Scanboostar Premium | SCSI |  | Good | OK, SCSI-ID=LinoHell Office2
EDGE | KTX-9600US | SCSI |  | Untested | no feedback
Epson | Perfection 600 | SCSI |  | Good | OK, SCSI-ID=EPSON Perfection600
Escom | Image Scanner 256 | SCSI |  | Good | OK, SCSI-ID=UMAX UG 80
Escort | Galleria 600 | SCSI |  | Untested | untested, SCSI-ID=ESCORT Galleria 600S
Genius | ColorPage-HR5 (Pro) | SCSI |  | Good | OK, SCSI-ID=KYE ColorPage-HR5
Nikon | AX-110 / Scantouch 110 | SCSI |  | Untested | may work, please test and give feedback
AX-210 | SCSI |  | Good | OK
TriGem | PowerScanII | SCSI |  | Good | OK

### Backend: umax1220u (unmaintained)

Link(s): http://sourceforge.net/projects/umax1220u-sane
Manual page: sane-umax1220u

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
UMAX | Astra 1220U | USB | 0x1606/0x0010 | Good |
Astra 1600U | USB | 0x1606/0x0030 | Good |
Astra 2000U | USB | 0x1606/0x0030 | Good |
Astra 2100U | USB | 0x1606/0x0130 | Good |

### Backend: umax_pp (1 (unmaintained))

Link(s): http://umax1220p.sourceforge.net/
Manual page: sane-umax_pp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
UMAX | Astra 1220P | Parport (EPP/ECP) |  | Good |
Astra 2000P | Parport (EPP/ECP) |  | Good |
Astra 1600P | Parport (EPP/ECP) |  | Good |
Astra 600P | Parport (SPP/ECP) |  | Unsupported | untested, but should be close to 610P
Astra 610P | Parport (SPP/ECP) |  | Good |
Hewlett-Packard | Scanjet 3200C | Parport (EPP/ECP) |  | Good | works (relabelled 1220P and 2000P)
Genius | ColorPage-Life Pro | Parport (EPP/ECP) |  | Good | works (relabelled 1220P and 2000P)

### Backend: unsupported (2010-06-09)

Link(s): /contrib.html
Comment: The devices mentioned here are not supported by any SANE backend. However, there may be links to information about them or stand-alone programs.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Agfa | DuoScan f40 | USB IEEE-1394 | 0x06bd/0x02bf | Unsupported | Unsupported. See link for details.
DuoScan T2000XL | SCSI |  | Unsupported | Unsupported. Same as Microtek ArtixScan 2020?
DuoScan T2500 | SCSI IEEE-1384 |  | Unsupported | Unsupported. Same as Microtek Artixscan 2500f
SnapScan 310P | Parport |  | Unsupported | Unsupported, see link for details.
SnapScan EZ | Parport |  | Unsupported | Unsupported, see link for details.
SnapScan 1200P | Parport |  | Unsupported | Unsupported, see link for details.
SnapScan 1212P | Parport |  | Unsupported | Unsupported, see link for details.
Artec/Ultima | 1236 USB | USB | 0x05d8/0x4001 | Unsupported | Unsupported. See link for details.
AM12e+ | Parport |  | Unsupported | Unsupported. Chips found inside: AT015, AD9816JS. Maybe similar to SCSI version or as6e?
Ultima 2000 (0x4001) | USB | 0x05d8/0x4001 | Unsupported | Same name, but different ids: This scanner is not supported. The scanner with product id 0x4002 is supported by the gt68xx backend, however.
Avigramm | Minidoc | USB Parport | 0x05cb/0x1483 | Unsupported | Not supported. See link for details.
Avision | DS310F | Parport |  | Unsupported | Probably not supported. Scanner/printer/copier combination.
iVina FB2400 | USB |  | Unsupported | Not supported. No chipset information available. Same as UMAX Astra 6700.
iVina 1600 | USB | 0x0638/0x0a10 | Unsupported | GL646 based, to be added to genesys backend. Same as UMAX Astra 4500.
iVina FB1800 | USB | 0x0638/0x0a20 | Unsupported | GL646/GL660 based. Same as UMAX Astra 4700.
Benq (Acer) | 310P | Parport |  | Unsupported | Unsupported, see link for details.
320P | Parport |  | Unsupported | Unsupported, see link for details.
340P | Parport |  | Unsupported | Unsupported, see link for details.
610P | Parport |  | Unsupported | Unsupported, see link for details.
610PT | Parport |  | Unsupported | Unsupported, see link for details.
620P | Parport |  | Unsupported | Unsupported, see link for details.
620PT | Parport |  | Unsupported | Unsupported, see link for details.
640P | Parport |  | Unsupported | Unsupported, see link for details.
5450 | USB | 0x04a5/0x211e | Unsupported | Unsupported.
5550 | USB | 0x04a5/0x2211 | Unsupported | Unsupported, see link for details.
5560 | USB | 0x04a5/0x2311 | Unsupported |
7400UT | USB | 0x04a5/0x2202 | Unsupported |
Boeder | Sm@rtScan Office | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details.
Brother | MFC 2500 | USB | 0x04f9/0x000a | Unsupported | Not supported. See link for details.
MFC 4600 | Parport |  | Unsupported | The parport 200x400dpi grayscale version of this scanner is unsupported. Dmitri Katchalov did some investigations on this scanner. If you want to write a backend, contact him (see link).
MFC 7300c | Parport USB | 0x04f9/0x0106 | Unsupported |
MFC 9600 | USB | 0x04f9/0x0101 | Unsupported |
C-Channel | MyPen Pro | USB |  | Unsupported | Probably unsupported. See link for details.
MyPen Light | USB | 0x0a93/0x0005 | Unsupported | See bug #306792 for details.
MoneyPen II | USB |  | Unsupported | Probably unsupported.
Canon | CanoScan 3000 | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based.
CanoScan 3000ex | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based.
CanoScan 3000F | USB | 0x04a9/0x2215 | Unsupported | GL660+GL646 based, to be added to genesys backend
CanoScan 4200F | USB | 0x04a9/0x221b | Unsupported | Probably unsupported. See link.
CanoScan 4400F | USB | 0x04a9/0x2228 | Unsupported | GL843 based, to be added to genesys backend
CanoScan 5000F | USB | 0x04a9/0x2212 | Unsupported | Unsupported. See link for details.
CanoScan 5200F | USB | 0x04a9/0x2217 | Unsupported | Probably unsupported. See link for details.
CanoScan 8000F | USB | 0x04a9/0x220f | Unsupported | Not supported. See link for more information. With transparency adapter.
CanoScan 8400F | USB | 0x04a9/0x221e | Unsupported | GL841 based, to be added to genesys backend
CanoScan 8600F | USB | 0x04a9/0x2229 | Unsupported | GL841 based, to be added to genesys backend
CanoScan 9900F | USB | 0x04a9/0x2210 | Unsupported | Probably unsupported, similar to 8000F. 3200x6400 dpi USB2. With transparency adapter.
CanoScan 9950F | USB | 0x04a9/0x2219 | Unsupported | Probably unsupported.
CanoScan D646U | USB | 0x04a9/0x220b | Unsupported | Probably not supported. See link for more information and test program.
CanoScan D646U ex | USB | 0x04a9/0x220b | Unsupported | Probably not supported. See D646.
CanoScan D1230U | USB | 0x04a9/0x2209 | Unsupported | Probably not supported.
CanoScan D1250U2 | USB | 0x04a9/0x220c | Unsupported | Not supported. However, someone started working on this scanner and some information is available (see link).
CanoScan D2400UF | USB | 0x04a9/0x220a | Unsupported | Not supported. See link.
CanoScan FB320U | USB | 0x04a9/0x2201 | Unsupported | Probably not supported. No details known.
CanoScan FB620U | USB | 0x04a9/0x2202 | Unsupported | Probably not supported. Some information is available.
CanoScan FB1210U | USB | 0x04a9/0x2205 | Unsupported | Not supported. However, a stand-alone program for FreeBSD is available.
CanoScan LiDE 70 | USB | 0x04a9/0x2225 | Unsupported | Philips chip. Backend started, see link
CanoScan LiDE 90 | USB | 0x04a9/0x1900 | Unsupported | Unsupported. See link for details.
CanoScan LiDE 500F | USB | 0x04a9/0x221f | Unsupported | GL841 based, to be added to genesys backend
CanoScan LiDE 600 | USB | 0x04a9/0x2224 | Unsupported | Philips chip. Backend started, see link
CanoScan LiDE 600F | USB | 0x04a9/0x2224 | Unsupported | Philips chip. Backend started, see link
FS4000 | USB SCSI | 0x04a9/0x3042 | Unsupported | Not supported. See link for more details.
IS 12 | USB |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 22 | Parport |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 32 | USB | 0x04a9/0x105d | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
IS 52 | USB |  | Unsupported | Probably not supported. Scanner cardridge for Canon inkjet printers.
ImageRunner iR1018 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details.
ImageRunner iR1022 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details.
ImageRunner iR1023 | USB | 0x04a9/0x269d | Unsupported | Probably not supported. See link for details.
PIXMA MP110 | USB | 0x04a9/0x1700 | Unsupported | Probably not supported. See link for details.
PIXMA MP130 | USB | 0x04a9/0x1701 | Unsupported | Probably not supported. See link for details.
DR-2020U | USB |  | Unsupported | GL84x?
Chinon | DS-3000 | Parport Serial Port |  | Unsupported | Unsupported at the moment, but a backend is in preparation. See link.
Compaq | S200 | USB | 0x049f/0x0021 | Unsupported | Not supported. 2400x1200 dpi. One bulk-in, one bulk-out and one interrupt endpoint. Type-number: U0001-HB21, another type nr on the inside: 75100512-00
Compeye | Simplex 1236C | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details.
Corex | Cardscan 500 | USB | 0x08f0/0x0001 | Unsupported | Probably not supported. Businesscard reader.
Cardscan 700 C | USB | 0x08f0/0x0004 | Unsupported | Probably not supported.
Dell | A940 | USB | 0x413c/0x5106 | Unsupported | Probably rebadged Lexmark X5150. May work with sane-lexmark? See bug #312130
A960 | USB | 0x413c/0x5107 | Unsupported | Probably not supported. See link for details.
922 | USB | 0x413c/0x5109 | Unsupported | Probably not supported. See link for details.
Epson | GT-2200 | USB | 0x04b8/0x0102 | Unsupported | Probably unsupported. No details known.
StylusScan 2000 | USB | 0x04b8/0x0105 | Unsupported | Probably unsupported. No details known.
Stylus DX4450 | USB | 0x04b8/0x083f | Unsupported | Probably unsupported. See link for details.
Stylus CX-5800 | USB |  | Unsupported | Probably unsupported at the moment. Not compatible to snapscan backend. It's not known if it may work with epson or epkowa backend.
EDT (Electronic Document Technology) | BizCardReader 900C | USB | 0x0a53/0x5001 | Unsupported | Probably unsupported. See link for details.
E-Lux | j-6121 | Parport |  | Unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
Enhans | j-6121 | Parport |  | Unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
M-3630 A | Parport |  | Unsupported | Probably unsupported.
Fujitsu | SP1120 | USB | 0x04c5/0x1473 | Unsupported | Genesys GL310 chipset, not supported by sane-genesys backend.
SP1125 | USB | 0x04c5/0x1475 | Unsupported | Genesys GL310 chipset, not supported by sane-genesys backend.
SP1130 | USB | 0x04c5/0x1476 | Unsupported | Genesys GL310 chipset, not supported by sane-genesys backend.
Genius | ColorPage CS | SCSI |  | Unsupported | Probably unsupported, see link for details.
ColorPage-Slim 1200 USB2 | USB | 0x0458/0x2020 | Unsupported | GL841 based, to be added to genesys backend.
ColorPage HR6X Slim | USB | 0x0458/0x2019 | Unsupported | GL646 based, to be added to genesys backend
ColorPage HR7X | USB | 0x0458/0x2018 | Unsupported | GL646 based, to be added to genesys backend
ColorPage HR7XE | USB | 0x06dc/0x0012 | Unsupported | Unsuported. See link for details.
ColorPage HR8 | USB | 0x0458/0x201c | Unsupported | GL841 based, to be added to genesys backend
Guillemot | SCAN@HOME 48 USB | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details.
Maxi Scan A4 Parallel 36 bit | Parport |  | Unsupported | Probably unsupported. Identical to the Benq Prisa 620P.
Hercules | SCAN@HOME 48 USB | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details.
Hewlett-Packard | Photo Scanner 1000 | USB | 0x03f0/0x1001 | Unsupported | Not supported by SANE. However, it's detected as mass storage device so just mounting it is reported to work. See link for device data.
Photosmart 1200 Photo | USB |  | Unsupported | Probably not supported by SANE. No details known. 10x15 cm. Maybe similar to Photo Scanner 1000?
Photosmart S20 (C5101A) | USB | 0x03f0/0x0102 | Unsupported | Not supported yet by SANE. See link for details.
Photosmart S20xi (C7150A) | USB | 0x03f0/0x0102 | Unsupported | Not supported yet by SANE. See link for details.
Photosmart C5100 series | USB | 0x03f0/0x5811 | Unsupported | Not supported yet by SANE. See link for details.
Photosmart C3180 | USB | 0x03f0/0x5611 | Unsupported | Not supported yet by SANE. See link for details.
ScanJet 3770 | USB | 0x03f0/0x2505 | Unsupported | While an external binary-only backend exists, it works only on Linux i386. Therefore the scanner is unsupported on other platforms.
ScanJet 4600 | USB | 0x03f0/0x3005 | Unsupported | Not supported. See link for details, or http://www.chmil.org/hp4600linux/ for code
ScanJet 4670 | USB | 0x03f0/0x3005 | Unsupported | Not supported. See ScanJet 4600 entry.
ScanJet 4890C | USB | 0x03f0/0x1b05 | Unsupported | GL843, maybe can be added to genesys backend
ScanJet 5530C Photosmart | USB | 0x03f0/0x1605 | Unsupported | Maybe GL841_HP, but not confirmed, maybe can be added to genesys backend
ScanJet 8390 | USB | 0x03f0/0x3805 | Unsupported | Probably not supported. See link for details.
ScanJet G4000 | USB | 0x03f0/0x4505 | Unsupported | Probably not supported. See link for details.
IBM | ADF Color Scanner | Proprietary |  | Unsupported | Unsupported. Uses proprietary ISA card. Maybe the same as the Plustek Spectra ADF?
IOMagic | MobileScan USB | USB Parport | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details.
Iris | IriScan | USB | 0x0a53/0x1000 | Unsupported | Unsupported. LM9832/3. See link for details.
IRISPen Translator Executive | USB | 0x0f43/0x015a | Unsupported | Unsupported. See link for details.
IRISCard Pro (IBCR II) | USB | 0x0a38/0x0301 | Unsupported | Unsupported. See link for details.
Kodak | Snapshot Photo Scanner 1 | Parport |  | Unsupported | Unsupported. FCC ID HWF96PHS
Lexmark | P6250 | USB | 0x043d/0x0097 | Unsupported | Unsupported. See link for details.
Photo 3150 | USB | 0x043d/0x007d | Unsupported | Unsupported. See link for details.
X74 | USB | 0x043d/0x0060 | Unsupported | Unsupported. See link for details.
X75 | USB | 0x043d/0x0060 | Unsupported | Unsupported. See link for details.
X75 PrinTrio | USB | 0x043d/0x0060 | Unsupported | Unsupported. See link for details.
X83 | USB | 0x043d/0x003d | Unsupported | Unsupported. GL640.
X2330 | USB | 0x043d/0x00bb | Unsupported | Unsupported. See link for details.
X3450 | USB | 0x043d/0x00f6 | Unsupported | Unsupported. See link for details.
X5130 | USB | 0x043d/0x0065 | Unsupported | Unsupported.
X5150 | USB | 0x043d/0x0065 | Unsupported | Probably unsupported. See link for details.
X5250 | USB | 0x043d/0x0093 | Unsupported | Unsupported.
X6170 | USB | 0x043d/0x0072 | Unsupported | Unsupported. See link for details.
X7170 | USB | 0x043d/0x0098 | Unsupported | Unsupported. See bug #310889 for details.
X7350 | USB | 0x043d/0x00b8 | Unsupported | Unsupported. See link for details.
X8350 | USB | 0x043d/0x00b9 | Unsupported | Unsupported. See link for details.
Logitech | PageScan Color | Parport |  | Unsupported | Most probably unsupported.
PageScan USB | USB | 0x046d/0x040f | Unsupported | Probably unsupported. See link for details.
Medion/Lifetec/Tevion/Cytron | MD 6190 | USB | 0x0461/0x0392 | Unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details.
MD 6190 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. There seem to exist two different scanners with that name. See link for details.
MD 40420 | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details.
MD 41260 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. See link for details.
MD 41985 | USB | 0x0461/0x037b | Unsupported | Probably unsupported. See link for details.
MD 42666 | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details.
MD 85264 | USB | 0x08ff/0x2580 | Unsupported | Fingerprint sensor. See link for details.
MD 90009 | USB | 0x05da/0x30e5 | Unsupported | Probably unsupported. See link for details.
MD 90070 | USB | 0x05da/0x3022 | Unsupported | Unsupported. See link for details.
MD 90090 | USB | 0x05da/0x3022 | Unsupported | Unsupported. See link for details.
Memorex | 6136u | USB | 0x0461/0x0346 | Unsupported | Probably unsupported.
6142u | USB | 0x0461/0x0347 | Unsupported | Probably unsupported. Same as Visioneer Onetouch 4400. See link for details.
MaxxScan 6122 | USB Parport | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details.
SCF 9612P | Parport |  | Unsupported | Probably unsupported. See link for details.
Microtek | ArtixScan 2020 | SCSI |  | Unsupported | Unsupported. Same as Agfa DuoScan T2000XL?
ArtixScanDI 2020 | USB | 0x05da/0x202e | Unsupported | Unsupported. See link for details.
Artixscan 2500f | SCSI IEEE-1384 |  | Unsupported | Unsupported. Same as Agfa DuoScan T2500?
ArtixScan 4000tf | USB |  | Unsupported | Unsupported. Uses ALI M5611B.
FilmScan 35 | USB | 0x05e3/0x0120 | Unsupported | Probably unsupported. See link for details.
ScanMaker 336 CX | SCSI |  | Unsupported | Probably unsupported. Seems to be similar to the Microtek 330 CX and is detected by the microtek2 backend. Scanning doesn't seem to work however.
Scanmaker 1850S | SCSI |  | Unsupported | Unsupported. See link for details.
ScanMaker 3630 | USB | 0x0461/0x0347 | Unsupported | Unsupported. Doesn't seem to be compatible to 3600 series, see link.
ScanMaker 3800 | USB | 0x05da/0x30ce | Unsupported | Unsupported. See link for more details.
ScanMaker 3830 | USB | 0x05da/0x30ce | Unsupported | Unsupported. See link for more details.
ScanMaker 3860 | USB | 0x05da/0x3023 | Unsupported | Unsupported. See link for more details. Appears to be similar to ScanMaker 3880.
ScanMaker 3880 | USB | 0x05da/0x3021 | Unsupported | Unsupported. SQ113 chip. See link for more details.
ScanMaker 4600 | USB | 0x05da/0x40c7 | Unsupported | Unsupported. See link for more details.
ScanMaker 4700 | USB | 0x05da/0x20b4 | Unsupported | Unsupported. See link for more details.
ScanMaker 4850 | USB | 0x05da/0x30d9 | Unsupported | Probably unsupported. See link for details.
ScanMaker 4850 II | USB | 0x05da/0x3008 | Unsupported | Probably unsupported. See link for details.
ScanMaker 4900 | USB | 0x05da/0x30b9 | Unsupported | Unsupported. See link for more details.
ScanMaker 5 | SCSI |  | Unsupported | Probably unsupported. See link for more details.
ScanMaker 5600 | USB | 0x05da/0x20a7 | Unsupported | Unsupported. See link for more details.
ScanMaker 5700 | USB | 0x05da/0x20bd | Unsupported | Unsupported. Uses ALI M5615 like the ScanMaker 4700.
ScanMaker 5800 | USB | 0x05da/0x3008 | Unsupported | Unsupported. See link for details.
ScanMaker 5800 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for details.
ScanMaker 5900 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for more details.
ScanMaker 5950 | USB | 0x05da/0x30d8 | Unsupported | Unsupported. See link for more details.
ScanMaker 6000 | USB | 0x05da/0x30e5 | Unsupported | Unsupported. See link for more details.
ScanMaker 6100 | USB | 0x05da/0x30e5 | Unsupported | Unsupported. See link for more details.
ScanMaker 6700 | USB IEEE-1394 | 0x05da/0x20c9 | Unsupported | Unsupported. See link.
ScanMaker 8700 | USB IEEE-1394 | 0x05da/0x20b1 | Unsupported | Unsupported. See link for details. USB vendor and product ids to be checked.
ScanMaker 9600XL | USB IEEE-1394 | 0x05da/0x20de | Unsupported | Probably unsupported. SCSI seems to work with microtek2 backend.
ScanMaker 9800XL | USB SCSI | 0x05da/0x20de | Unsupported | Partly unsupported. IEEE-1394 works with microtek2 backend. See link.
ScanMaker i320 | USB | 0x05da/0x30e6 | Unsupported | Unsupported. See link.
ScanMaker s400 | USB | 0x05da/0x201c | Unsupported | Unsupported. See link.
ScanMaker S400 | USB | 0x05da/0x300b | Unsupported | Unsupported. See link.
ScanPort 3000 | USB | 0x04a7/0x0224 | Unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Realtek RTS8801B?. See link for details.
Konica Minolta | Dual Scan III | USB | 0x0686/0x400d | Unsupported | Unsupported. May work with vuescan. See link for details.
Dual Scan IV | USB | 0x132b/0x000a | Unsupported | Unsupported. Works with vuescan. See link for details.
DiMAGE Scan Elite 5400 | USB IEEE-1394 | 0x0686/0x400e | Unsupported | Probably unsupported. May work with vuescan. See link for details.
DiMAGE Scan Elite 5400 2 | USB | 0x132b/0x0012 | Unsupported | Probably unsupported. See link for details.
DiMAGE Scan Multi Pro | IEEE-1394 |  | Unsupported | Probably unsupported. See link for details.
magicolor 2480MF | USB Network |  | Unsupported | Uses a different scanning protocol than the magicolor 1690MF
Mustek | 1200 III EP | Parport |  | Unsupported | Probably not supported. quarlewm at jmu dot edu offers to temporarily loan such a scanner to anyone who is interested in writing a driver.
2400 M | USB |  | Unsupported | Probably unsupported. No details known.
BearPaw 2400 TA Pro | USB | 0x055f/0x0400 | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information.
BearPaw 2448 CU Pro | USB | 0x055f/0x0408 | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information.
BearPaw 4800 TA Pro | USB | 0x055f/0x1000 | Unsupported | Not supported. See link for some information.
BearPaw 4800 TA Pro II | USB | 0x055f/0x040a | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information.
BearPaw 6400 TA Pro | USB | 0x055f/0x040b | Unsupported | Not supported. May be supported by mustek_usb2 backend later. See link for some information.
Paragon 800 II EP | Parport |  | Unsupported | Not supported. Maybe similar to 600 II EP (SCSI_over-parport)? In this case it could be supported by the mustek SCSI backend.
ScanExpress 600 USB | USB | 0x055f/0x0873 | Unsupported | Unsupported. Programming information is available.
ScanExpress 1200 USB | USB | 0x055f/0x0003 | Unsupported | Unsupported. Programming information is available.
ScanExpress 1200 USB Plus | USB | 0x055f/0x0007 | Unsupported | Unsupported.
ScanExpress 12000 P | Parport |  | Unsupported | Not supported. Asic 1505/05.
ScanExpress A3 EP | Parport |  | Unsupported | Not supported. Maybe it will be supported by the mustek_pp backend in future.
ScanExpress CardSmart | USB |  | Unsupported | Probably unsupported. USB business card scanner. Maybe works as USB storage device?
ScanMagic 9636P | Parport |  | Unsupported | Probably not supported. Same as Mustek 12000 P?. ASIC 1505.
NEC | Petiscan | USB | 0x0475/0x0100 | Unsupported | Most probably unsupported. See link for details. Vendor ID is Relisys/Teco. Not known if it is similar to other Relisys/Teco USB scanners.
Nikon | LS-9000 ED | IEEE-1394 |  | Unsupported | Probably not supported. See link for details. Possibly similar to LS-8000 ED.
Olivetti | Job-Jet M400 | USB | 0x0b3c/0xa880 | Unsupported | Probably not supported. See link for details.
Olympus | ES-10P | Parport |  | Unsupported |
ES-10S | SCSI |  | Unsupported | Probably not supported. See link for details.
Optoelectronics | Barcode scanner | USB | 0x065a/0x0001 | Unsupported | Probably not supported.
Optrox | PhotoMaker 3C | Parport |  | Unsupported |
PhotoMaker 3E | Parport |  | Unsupported |
PhotoMaker 3F | Proprietary |  | Unsupported | Special ISA card
PhotoMaker 3S | Parport |  | Unsupported |
PhotoMaker 6E | Parport |  | Unsupported |
PhotoMaker 6F | Proprietary |  | Unsupported | Special ISA card
Panasonic | KV-SS905C | SCSI |  | Unsupported | might be supported by matsushita backend. See http://code.google.com/p/kvss905c/ for a standalone scanning tool.
KV-S2055W | USB SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S2055L | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S2065W | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S3065CW | USB SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S3065CL | USB SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S3085 | USB SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S3105C | USB SCSI |  | Unsupported | might be supported by matsushita backend. See http://code.google.com/p/kvss905c/ for a standalone scanning tool.
KV-S6040W | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S6045W | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S6050W | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S6055W | SCSI |  | Unsupported | might be supported by matsushita backend.
KV-S7065C | USB SCSI |  | Unsupported | might be supported by matsushita backend.
Pentax | DSmobile USB | USB | 0x0a82/0x2000 | Unsupported | Probably not supported. Some information is available.
PIE | Primefilm 1800u | USB | 0x05e3/0x0120 | Unsupported | Not supported. See link for details.
Primefilm 2700 | USB |  | Unsupported |
Primefilm 3600PRO | USB IEEE-1394 |  | Unsupported | Probably not supported.
Powerslide 3600 | USB IEEE-1394 | 0x05e3/0x0142 | Unsupported | Probably unsupported. Film scanner that can scan directly from the magazine.
PF3650 Pro3 Film Scanner | USB IEEE-1394 | 0x05e3/0x0143 | Unsupported | Not supported. See link for details.
Plustek | OpticFilm 7200 | USB | 0x07b3/0x0807 | Unsupported | GL842 based, maybe to be added to genesys backend
OpticFilm 7200i | USB | 0x07b3/0x0c04 | Unsupported | GL843 based, maybe to be added to genesys backend
OpticPro A3U | USB |  | Unsupported | Uses Plustek ASIC P99002
OpticPro S6 | USB |  | Unsupported | Uses RealTek chipset (RTL8801D)
OpticPro S12 | USB | 0x07b3/0x0600 | Unsupported | Product id 0x0600 is unsupported but may be supported by the genesys backend in future. Product id 0x040b is supported by the gt68xx backend.
OpticPro ST12 | USB | 0x07b3/0x0600 | Unsupported | Product id 0x0600 is unsupported but may be supported by the genesys backend in future. Product id 0x040b is supported by the gt68xx backend.
OpticPro ST16 | USB | 0x07b3/0x0600 | Unsupported | GL646 based, to be added to genesys backend
OpticPro UA18 | USB |  | Unsupported | Probably LM983x based.
OpticPro S24 | USB | 0x07b3/0x0601 | Unsupported | Product id 0x0601 is unsupported but may be supported by the genesys backend in future /GL646). Product id 0x040e is supported by the gt68xx backend.
OpticPro ST24 | USB | 0x07b3/0x0601 | Unsupported | GL646 based, to be added to genesys backend
OpticPro S28 | USB | 0x07b3/0x0801 | Unsupported | GL841 based, to be added to genesys backend
OpticPro ST28 | USB | 0x07b3/0x0801 | Unsupported | GL841 based, to be added to genesys backend
OpticPro ST28 | USB | 0x07b3/0x0802 | Unsupported | GL841 based, to be added to genesys backend
Umax AstraScan 4750 | USB | 0x07b3/0x0802 | Unsupported | GL841 based, to be added to genesys backend, rebadged Plustek ST28
OpticPro ST48 | USB | 0x07b3/0x0800 | Unsupported | GL841 based, to be added to genesys backend
OpticPro ST64 | USB | 0x07b3/0x0c00 | Unsupported | GL843 based, maybe to be added to genesys backend
OpticPro ST64+ | USB | 0x07b3/0x0c03 | Unsupported | GL843 based. See link for more details.
PL 806 | USB | 0x07b3/0x0c0c | Unsupported | Unsupported. See link for more details.
SmartOffice PL 812 | USB | 0x07b3/0x0c0d | Unsupported | Unsupported. See link for more details.
OpticSlim 500 | USB | 0x07b3/0x0458 | Unsupported | Unsupported. See link for more details.
OpticSlim 2420 | USB | 0x07b3/0x0806 | Unsupported | GL841 based, to be added to genesys backend
OpticSlim 2420+ | USB | 0x07b3/0x0914 | Unsupported | GL841 based, to be added to genesys backend
OpticWorks 2000 | Parport |  | Unsupported | Multifunction device. No further information available.
OptiCard 600+ | USB |  | Unsupported | Business card reader. No further information available.
ScanCopy 115 | USB | 0x07b3/0x081c | Unsupported | GL841 based, to be added to genesys backend
Spectra ADF | Proprietary |  | Unsupported | Unsupported. Uses proprietary ISA card that also provides power and is labelled GPS-1 PAGE-A from Taiwan. Other labels on the scanner include ADF Color Scanner and SF600AS. Maybe the same as the IBM ADF Color Scanner?
Unknown Plustek Device | USB | 0x07b3/0x0005 | Unsupported | Probably unsupported. Scanner name not known yet.
Unknown Plustek Device | USB | 0x07b3/0x0007 | Unsupported | Probably unsupported. Scanner name not known yet.
Unknown Plustek Device | USB | 0x07b3/0x000f | Unsupported | Probably unsupported. Scanner name not known yet.
Unknown Plustek Device | USB | 0x07b3/0x0012 | Unsupported | Probably unsupported. Scanner name not known yet.
Unknown Plustek Device | USB | 0x07b3/0x0014 | Unsupported | Probably unsupported. Scanner name not known yet.
Unknown Plustek Device | USB | 0x07b3/0x0016 | Unsupported | Probably unsupported. Scanner name not known yet.
PLANon | DocuPen RC800 | USB | 0x18dd/0x1000 | Unsupported | Probably not supported. No details known.
DocuPen R700 | USB | 0x10c4/0xea60 | Unsupported | Probably not supported. See link for details.
DocuPen (DPEN-BW) | USB |  | Unsupported | Probably not supported. No details known.
Primax | Colorado 600U | USB | 0x0461/0x0341 | Unsupported | Not supported. Some information is available.
Colorado 1200p | Parport |  | Unsupported | Unsupported by SANE. But is reported to partly work with pxscan. See link.
Colorado 1200u | USB | 0x0461/0x0361 | Unsupported | Probably unsupported. No details known.
Primascan Colorado 2600u | USB | 0x0461/0x0347 | Unsupported | Unsupported. Same as Visioneer Onetouch 4400. See link for details.
Colorado Direct 600 | Parport |  | Unsupported | Not supported. However, a stand-alone program is available.
Colorado Direct 9600 | Parport |  | Unsupported | Not supported. However, a stand-alone program is available.
Colorado USB 9600 | USB | 0x0461/0x0340 | Unsupported | Not supported. See link for details.
G2-300 | USB | 0x0461/0x0300 | Unsupported | Probably unsupported. No details known.
G2-300 #2 | USB | 0x0461/0x0302 | Unsupported | Probably unsupported. No details known.
G2E-300 | USB | 0x0461/0x0301 | Unsupported | Probably unsupported. No details known.
G2E-300 #2 | USB | 0x0461/0x0303 | Unsupported | Probably unsupported. No details known.
G2-600 | USB | 0x0461/0x0380 | Unsupported | Probably unsupported. No details known.
G2-600 #2 | USB | 0x0461/0x0382 | Unsupported | Probably unsupported. No details known.
G2E-600 | USB | 0x0461/0x0383 | Unsupported | Probably unsupported. No details known.
OneTouch 5300 | Parport |  | Unsupported | Not supported.
ReadyScan 636i | USB | 0x0461/0x0381 | Unsupported | Probably unsupported. No details known.
Slim-Line 1200 | USB |  | Unsupported | Maybe GL646. Maybe similar to Medion MD 6228?
Onetouch 8920 | USB | 0x0461/0x0371 | Unsupported | Not supported. Look similar to Visioneer Onetouch 8920 (same USB product id).
Prolink | Winscan Pro 2448U | USB | 0x06dc/0x0014 | Unsupported | Not supported. Some information is available. RealTek RTS8801.
Winscan Pro 2000 | USB Parport |  | Unsupported | Not supported. No further information available.
Quato | X-Finity | SCSI |  | Unsupported | Probably not supported. No details yet. Originally manufactured by PFU?
X-Finity Ultra | USB IEEE-1394 |  | Unsupported | Probably not supported. No details yet.
Reflecta | DigitDia 3600 | USB IEEE-1394 | 0x05e3/0x0142 | Unsupported | Film scanner that can scan directly from the magazine.
iScan 1800 | USB | 0x05e3/0x0120 | Unsupported | Probably unsupported. See link for details.
ProScan 4000 | USB IEEE-1394 | 0x05e3/0x0143 | Unsupported | Probably unsupported. See link for details.
Relisys | Eclipse 1200U | USB | 0x0475/0x0103 | Unsupported | Probably unsupported. See link for details.
Scorpio Ultra 3 | USB | 0x0475/0x0210 | Unsupported | Probably unsupported. See link for details.
Episode | USB | 0x0475/0x0103 | Unsupported | Probably unsupported. See link for details.
AVEC II E3 | Parport |  | Unsupported | Parport version of AVEC II S3?. See bug #304992 for details
Samsung | SCX-4725FN | USB | 0x04e8/0x341f | Unsupported | Not supported. See link for details.
Scanshell | 800N | USB | 0x0a82/0x6605 | Unsupported | Not supported. See link for details.
Sicos | DMS 2000 | proprietary |  | Unsupported | Not supported until now. Work on a backend has started, contact the author for details (see link)
Siemens | ID Mouse Professional | USB | 0x0681/0x0005 | Unsupported | Not supported.
Cherry FingerTIP ID Board - Sensor | USB | 0x0681/0x0010 | Unsupported | Not supported.
SmartDisk | SmartScan 3600 | USB IEEE-1394 |  | Unsupported | Probably not supported. Same as PIE Primefilm 2600 PRO.
Spot Technology | Maxiscan A4 | proprietary |  | Unsupported | Not supported until now. Work on a backend has started, see link for more information.
ScanTak 2c | proprietary |  | Unsupported | Not supported. Work on a backend has started, see link for more information.
ScanTak 3c | proprietary |  | Unsupported | Not supported. Work on a backend has started, see link for more information.
Syscan | TravelScan FS-531 | USB | 0x0a82/0x0530 | Unsupported | Not supported. May work with the Plustek backend in future. See link for details.
TravelScan Pro | USB | 0x0a82/0x2000 | Unsupported | Probably not supported. Some information is available.
Tamarack | Artiscan 9600 | Parport |  | Unsupported | Unsupported at the moment. See link for a project for that scanner taht may support it in future.
Artiscan 9600 pro 36 | Parport |  | Unsupported | Unsupported at the moment. See link for a project for that scanner.
Artiscan 2400FS | USB | 0x05e3/0x0100 | Unsupported | Unsupported. See link for more information.
TCE | MK600U | USB | 0x0461/0x0346 | Unsupported | Not supported. Some information is available.
S450 | Parport |  | Unsupported | Not supported by SANE but is reported to work with pxscan (see link).
Teco | VM6509F | USB | 0x080d/0x0102 | Unsupported | Probably unsupported. See link for details.
Tiny | FU661E | USB | 0x0461/0x0347 | Unsupported | Unsupported. See link for details.
Trust | CombiScan 19200 | Parport USB | 0x05cb/0x1483 | Unsupported | Unsupported. See link for details.
EasyScan 19200 | Parport |  | Unsupported |
SCSI Scan 19200 -Excellence Series- | SCSI |  | Unsupported | Unsupported. See link for details.
UMAX | Astra 2500 | USB | 0x0461/0x0374 | Unsupported | Probably not supported. See link for details.
Astra 2850 | USB | 0x07b3/0x0601 | Unsupported | Probably not supported. Same IDs as Plustek OpticPro ST24. See link for details.
Astra 3000 | USB | 0x0461/0x038a | Unsupported | Probably not supported. See link for details.
Astra 3600 | USB | 0x0461/0x038a | Unsupported | Probably not supported. See link for details.
Astra 4000 | USB | 0x1606/0x1030 | Unsupported | Not supported. See link for details.
Astra 4100 | USB | 0x0461/0x038c | Unsupported | Not supported, to be added to genesys backend.
Astra 4500 | USB | 0x0638/0x0a10 | Unsupported | GL646 based, to be added to genesys backend. Avision iVina FB1600 clone
Astra 4600 | USB |  | Unsupported | Probably not supported, no details known.
Astra 4700 | USB | 0x0638/0x0a20 | Unsupported | GL646/GL660 based. Avision iVina FB1800 clone.
Astra 6700 | USB | 0x0638/0x0a30 | Unsupported | Not supported. No chipset information available. Same as Avision iVina FB2400.
AstraSlim | USB | 0x080d/0x0104 | Unsupported | Probably not supported currently. See link for more details.
AstraSlim 1200 | USB | 0x080d/0x0110 | Unsupported | See link for more details.
AstraSlim 6000 | USB | 0x080d/0x0104 | Unsupported | Probably not supported currently. See link for more details.
Nete3470' | Parport |  | Unsupported | Probably not supported. No details known..
Powerlook 180 | USB |  | Unsupported | Probably not supported. See link for details.
Powerlook 1000 USB | USB |  | Unsupported | Probably not supported. No further information available.
Vantas | 3000 | USB | 0x04a7/0x0224 | Unsupported | Not supported. See link for more details.
Visioneer | 6200 | USB | 0x0461/0x0345 | Unsupported | Not supported. Is reported to use the E5 chipset. Uses a Primax ID. Looks similar to Primascan Colorado 2600u.
6200 EPP/USB | USB | 0x04a7/0x0311 | Unsupported | Not supported. Id is from Primax? Yet another scanner with the same name?
9420 | USB | 0x0461/0x03a8 | Unsupported | Unsupported. See link for details.
9450 USB | USB | 0x04a7/0x0421 | Unsupported | Unsupported. See link for details.
Onetouch 4400 | USB | 0x0461/0x0347 | Unsupported | Not supported. E5 chipset? See link for more details.
OneTouch 4800 USB | USB | 0x04a7/0x0224 | Unsupported | Unsupported. Seems to use Realtek RTS8801B. Same as Microtek Scanport 3000. See link for details.
OneTouch 5300 USB | USB | 0x04a7/0x0226 | Unsupported | Not supported. Chipset is RTS8801B(?). See link for output of /proc/bus/usb/devices.
OneTouch 5300 | USB | 0x04a7/0x0221 | Unsupported | Not supported. Yet another scanner with this name?
OneTouch 5800 USB | USB | 0x04a7/0x0226 | Unsupported | Unsupported. 48 bit scanner, doesn't work with viceo backend. RTS8801C.
OneTouch 6600 | USB | 0x04a7/0x022a | Unsupported | Unsupported. See link for details.
Onetouch 7100 | USB | 0x04a7/0x0229 | Unsupported | GL646 based, to be added to genesys backend
Onetouch 7700 | USB | 0x04a7/0x0380 | Unsupported | LM9832/3 based, to be added to plustek backend
OneTouch 8100 | USB | 0x04a7/0x0321 | Unsupported | Unsupported. See link for details.
Onetouch 8700 | USB | 0x04a7/0x0371 | Unsupported | Not supported. See link for details.
Onetouch 8900 | USB | 0x04a7/0x0371 | Unsupported | Not supported. Same as 8920 but without TA?
Onetouch 8920 | USB | 0x04a7/0x0371 | Unsupported | Not supported. Same as 8700 and 8900 but includes a TA. Uses a Primax ID. Chipset is RTS8801C. See link for output of /proc/bus/usb/devices.
Onetouch 9000 | USB | 0x04a7/0x022c | Unsupported | Not supported. See link for details.
Onetouch 9020 | USB | 0x04a7/0x022c | Unsupported | Not supported. See link for details.
Onetouch 9320 | USB | 0x04a7/0x0362 | Unsupported | Probably not supported. See link for details.
Onetouch Pro 8800 | USB | 0x04a7/0x0410 | Unsupported | Probably not supported. See link for details.
Onetouch Pro 8820 | USB | 0x04a7/0x0410 | Unsupported | Probably not supported. See link for details.
PaperPort 3100b | Parport |  | Unsupported | Most probably not supported. See link for details.
PaperPort 6100 | Parport |  | Unsupported | Most probably not supported. More details would be appreciated.
PaperPort OneTouch | Parport |  | Unsupported | Most probably not supported. See link for details.
Strobe Pro USB | USB | 0x04a7/0x0102 | Unsupported | Not supported. See link for details.
4800 One Touch | USB | 0x04a7/0x03a0 | Unsupported | Unsupported. See link for details. Different id compared to One Touch 4800?
DocuImage 620S | SCSI |  | Unsupported | Not supported. See link for more details.
DocuMate 510 | USB | 0x04a7/0x0446 | Unsupported | Not supported. See link for more details.
DocuMate 510 | USB | 0x04a7/0x047c | Unsupported | Not supported. See link for more details. Yet another USB id.
One Touch 4800 | USB | 0x04a7/0x0224 | Unsupported | Unsupported. See link for details. Different id compared to 4800 One Touch?
WorkCentre 470cx | Parport |  | Unsupported | Not supported. See link for more details.
WorkCentre M15i | USB | 0x0924/0xffef | Unsupported | Not supported. See link for more details.
WorkCentre XK35c | USB Parport | 0x043d/0x0020 | Unsupported | Not supported. See link for more details.
WorkCentre XK50cx | USB | 0x04e8/0x3903 | Unsupported | Not supported. See link for more details.
WorkCentre Pro 412 | USB Parport | 0x043d/0x4303 | Unsupported | Not supported. See link for more details.
WorkCentre PE16 | USB Parport | 0x0924/0x4220 | Unsupported | Not supported. See link for more details.
WorkCentre PE120i | USB | 0x0924/0x4237 | Unsupported | Not supported. See link for more details.

### Backend: xerox_mfp (1.0-13)

Manual page: sane-xerox_mfp

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Xerox | Phaser 6110MFP | USB | 0x0924/0x3d5d | Good |
Phaser 3200MFP | USB | 0x0924/0x3da4 | Complete |
WorkCentre 3119 Series | USB | 0x0924/0x4265 | Good |
WorkCentre 4118 Series | USB | 0x0924/0x420c | Good |
WorkCentre 3210 | USB | 0x0924/0x4293 | Good |
WorkCentre 3220 | USB | 0x0924/0x4294 | Good |
Dell | Dell MFP Laser Printer 1815dn | USB | 0x413c/0x5124 | Good |
Dell 1235cn | USB | 0x413c/0x5310 | Good |
Samsung | X4300 Series | USB | 0x04e8/0x3324 | Untested |
K4350 Series | USB | 0x04e8/0x3325 | Untested |
X7600 Series | USB | 0x04e8/0x3326 | Untested |
K7600 Series | USB | 0x04e8/0x3327 | Untested |
K703 Series | USB | 0x04e8/0x3331 | Untested |
X703 Series | USB | 0x04e8/0x3332 | Untested |
SCX-4x16 | USB | 0x04e8/0x3409 | Untested |
SCX-6x20 | USB | 0x04e8/0x340d | Untested |
MFP-560 | USB | 0x04e8/0x340e | Untested |
MFP-750 | USB | 0x04e8/0x340f | Untested |
SCX-4x20 | USB | 0x04e8/0x3412 | Untested |
SCX-4100 | USB | 0x04e8/0x3413 | Good |
SCX-4x21 | USB | 0x04e8/0x3419 | Untested |
SCX-5x30 | USB | 0x04e8/0x341a | Untested |
SCX-4200 | USB | 0x04e8/0x341b | Good |
CLX-3160 | USB | 0x04e8/0x341c | Untested |
SCX-6x22 | USB | 0x04e8/0x341d | Untested |
SCX4725 | USB | 0x04e8/0x341f | Untested |
SCX4725-FN | USB | 0x04e8/0x341f | Good |
SCX-6x45 | USB | 0x04e8/0x3420 | Untested |
CLX-8380 | USB | 0x04e8/0x3421 | Untested |
CLX-2160 | USB | 0x04e8/0x3425 | Good |
SCX-4500 | USB | 0x04e8/0x3426 | Good |
CLX-6200 | USB | 0x04e8/0x3427 | Untested |
CLX-6240 | USB | 0x04e8/0x3428 | Untested |
SCX-6x55 | USB | 0x04e8/0x3429 | Good |
CLX-3170fn (CLX-3170 Series) | USB | 0x04e8/0x342a | Good |
CLX-3175FW | USB | 0x04e8/0x342a | Good |
SCX-4500W | USB Ethernet | 0x04e8/0x342b | Basic |
SCX-4824 (SCX-4x24 Series) | USB | 0x04e8/0x342c | Good |
SCX-4828FN (SCX-4x28 Series) | USB | 0x04e8/0x342d | Good |
SCX-4300 | USB | 0x04e8/0x342e | Good |
SCX-5835_5935 | USB | 0x04e8/0x342f | Good |
SCX-5635 | USB | 0x04e8/0x3430 | Untested |
SCX-4x26 | USB | 0x04e8/0x3432 | Untested |
SCX-4600 | USB | 0x04e8/0x3433 | Good |
SCX-4623 | USB | 0x04e8/0x3434 | Good |
MFP-65x | USB | 0x04e8/0x3435 | Untested |
SCX-6545 | USB | 0x04e8/0x3437 | Good |
CLX-8385 | USB | 0x04e8/0x3439 | Untested |
CLX-6220 | USB | 0x04e8/0x343a | Good |
CLX-6250 | USB | 0x04e8/0x343b | Untested |
SCX-4825FN (SCX-4x25 Series) | USB | 0x04e8/0x343c | Good |
CLX-3185 | USB | 0x04e8/0x343d | Good |
CLX-8540 | USB | 0x04e8/0x343f | Untested |
SCX-4623FW | USB | 0x04e8/0x3440 | Good |
SCX-3205W (SCX-3200 Series) | USB Ethernet | 0x04e8/0x3441 | Good |
SCX-6545X | USB | 0x04e8/0x3442 | Good |
SCX-6x55X | USB | 0x04e8/0x3443 | Good |
CLX-8385X | USB | 0x04e8/0x3444 | Good |
SCX-5835_5935X | USB | 0x04e8/0x3446 | Good |
SCX-4833FD | USB | 0x04e8/0x344b | Good |
SCX-4835FD | Ethernet | 0x04e8/0x344b | Good |
SCX-3405W | Ethernet |  | Good |
SCX-3400 | USB | 0x04e8/0x344f | Good |
SF-760 | USB | 0x04e8/0x3450 | Untested |
SCX-4729FD | USB | 0x04e8/0x3453 | Good |
CLX-6260 | USB | 0x04e8/0x3455 | Good |
CLX-3300 Series | USB | 0x04e8/0x3456 | Good |
SCX-470x | USB | 0x04e8/0x3457 | Untested |
CLX-4190 | USB | 0x04e8/0x345a | Good |
SCX-4650 4x21S Series | USB | 0x04e8/0x345b | Untested |
M337x 387x 407x Series | USB | 0x04e8/0x3460 | Good |
M267x 287x Series | USB | 0x04e8/0x3461 | Unsupported |
SCX-681x | USB | 0x04e8/0x3466 | Untested |
C460 | USB | 0x04e8/0x3468 | Untested |
M458x Series | USB | 0x04e8/0x346f | Untested |
M4370 5370 Series | USB | 0x04e8/0x3471 | Untested |
X401 Series | USB | 0x04e8/0x3477 | Untested |
K401 Series | USB | 0x04e8/0x3478 | Untested |
K3250 Series | USB | 0x04e8/0x3481 | Untested |
X3220 Series | USB | 0x04e8/0x3482 | Untested |

## Still Cameras

Backends: dc25, dc210, dc240, dmc

### Backend: dc25 (1.2 (unmaintained))

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc25

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Kodak | DC25 | Serial port |  | Complete |
DC20 | Serial port |  | Basic | DC-20 untested by author but reported to work

### Backend: dc210 (0.0 (unmaintained))

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc210

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Kodak | DC210 | Serial port |  | Basic |

### Backend: dc240 (0.0 (unmaintained))

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc240

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Kodak | DC240 | Serial port |  | Good | Use gphoto2 backend to get USB support

### Backend: dmc (unmaintained)

Manual page: sane-dmc

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Polaroid | DMC | SCSI |  | Good |

## Video Cameras

Backends: qcam, stv680, unsupported

### Backend: qcam (unmaintained)

Manual page: sane-qcam

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Connectix | Color QuickCam | Parport |  | Good | Requires root privileges.
Greyscale QuickCam | Parport |  | Minimal | Requires root privileges. Partly working.

### Backend: stv680 (1.0-1 (unmaintained))

Link(s): http://gkall.hobby.nl/stv680-aiptek.html
Manual page: sane-stv680
Comment: This vidcam backend is for the stv0680 chipset, See the website for more info.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Aiptek | Aiptek Pencam | USB | 0x0553/0x0202 | Minimal | image is OK for CIF and QCIF, VGA and QVGA untested, streaming video is a problem
Konica | e-mini | USB | 0x04c8/0x0722 | Untested |
Digital Dream | l' espion XS | USB | 0x1183/0x0001 | Untested |
Creative | WebCam Go Mini | USB | 0x041e/0x4007 | Untested |

### Backend: unsupported (2010-06-09)

Link(s): /contrib.html
Comment: The devices mentioned here are not supported by any SANE backend. However, there may be links to information about them or stand-alone programs.

Manufacturer | Model | Interface | USB id | Status | Comment
--- | --- | --- | --- | --- | ---
Biolux | 654 (micrOcular) | USB | 0x0923/0x010f | Unsupported | Not supported yet. See link for more details.
Grandtek Scopecam | 8x30 Binocular & Digital Camera | USB | 0x0797/0x801c | Unsupported | Not Supported yet. See link for more details.

## APIs

Backends: gphoto2, pint, pnm, template, test, v4l

### Backend: gphoto2 (0.0 (unmaintained))

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-gphoto2
Description: Multiple cameras supported by the gphoto2 libraries
Comment: The long-term plan is to support all the cameras supported by the gphoto2 libraries (currently over 140 models). However, at this stage, only a handful of cameras are definitely known to work with SANE. Other cameras will probably work if the native file format is EXIF or JPEG. Testers welcome!

### Backend: pint (unmaintained)

Manual page: sane-pint
Description: Scanners with the machine-independent PINT interface
Comment: Haven't been tested for a long time. Handle with care.

### Backend: pnm (1.0.8 (unmaintained))

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-pnm
Description: Reads PNM files
Comment: Used for debugging frontends. Obsolete, use test backend instead.

### Backend: template (0.42, NEW!)

Link(s): http://www.luser.com/temp/, http://www.luser.com/b/
Manual page: sane-template
Comment: This backend supports only the USB and SCSI models
Description: Interface to FrObYz API
Comment: Only FrObYz version 2.0 is supported!

### Backend: test (1.0-28 (unmaintained))

Link(s): http://www.meier-geinitz.de/sane/test-backend/
Manual page: sane-test
Description: Frontend-tester
Comment: Backend for testing frontends. Also serves as example for SANE backend options.

### Backend: v4l (1.0-3 (unmaintained))

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-v4l
Description: Interface to Video For Linux API
Comment: Supports video cameras and other devices accessed by the v4l kernel API, e.g. bttv devices. Quite a lot of known bugs.

## Meta Backends

Backends: dll, net

### Backend: dll (1.0.13 (unmaintained))

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-dll
Description: Dynamic loading of shared-library backends.

### Backend: net (1.0.14 (unmaintained))

Link(s): http://www.penguin-breeder.org/?page=sane-net
Manual page: sane-net
Description: Network access to saned servers
Comment: Can be used to access any scanner supported by SANE over the net. Supports IPv4 and IPv6.

### Legend:

> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Link(s):
>   Link(s) to more extensive and detailed information, if it exists, or the email address of the author or maintainer.
> Manual Page:
>   A link to the man-page online, if it exists.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Model:
>   Name of the device.
> Interface:
>   How the device is connected to the computer.
> USB id:
>   The USB vendor and product ids as printed by sane-find-scanner -q (only applicable for USB devices).
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Thu Mar 21 19:21:46 2019 by sane-desc 3.5 from sane-backends 1.0.27