| # Fax mode

Index XSane mode: Viewer mode Save mode Copy mode Multipage mode Fax mode E-mail mode Gimp plugin Scan options Medium selection Color correction: Gamma correction Brightness Contrast Threshold RGB default Negative Autoenhancement Default Restore Store Histogram window Pipette functions Standard options window Advanced options window Preview: Pipette white Pipette gray Pipette black Unzoom Zoom out Zoom in Undo zoom Autoselect scanarea Autoraise scanarea Select visible area Delete preview cache Preset area Rotation Aspect ratio RGB values Select scanarea Move scanarea Batch scan: Empty batch list Open batch list Save batch list Add area to list Remove selection Rename selection Rotate image Mirror image Setup: Copy setup Display setup Enhancement setup Fax setup Filetype setup E-mail setup Saving setup | This mode is a frontend for SANE and for a faxprogram like hylafax or mgetty+sendfax. You need to have a faxprogram like hylafax(1) or mgetty+sendfax(8) installed. The faxcommand and the options must be specified in the menu Preferences/Setup:Fax Options. #### Fine mode: The faxpages are always scanned in fine mode (204 dpi * 196 lpi). If Fine mode is enabled when the project is sent all pages are sent with 196lpi (fine mode), otherwise all pages are sent with 98lpi (normal mode). #### Insert file: You can add an external created postscript file to the fax project. The file is copied to the fax project directory. #### Show page: A postscrip viewer is called to display the selected page. #### Rename page: Rename the selected page. #### Delete page: Delete the selected page. #### Send project: Send all pages that are part of the fax project. Note that you need a working fax program! #### Delete project: Delete the fax project .

> Author: Oliver Rauch