| # Copy mode

Index XSane mode: Viewer mode Save mode Copy mode Multipage mode Fax mode E-mail mode Gimp plugin Scan options Medium selection Color correction: Gamma correction Brightness Contrast Threshold RGB default Negative Autoenhancement Default Restore Store Histogram window Pipette functions Standard options window Advanced options window Preview: Pipette white Pipette gray Pipette black Unzoom Zoom out Zoom in Undo zoom Autoselect scanarea Autoraise scanarea Select visible area Delete preview cache Preset area Rotation Aspect ratio RGB values Select scanarea Move scanarea Batch scan: Empty batch list Open batch list Save batch list Add area to list Remove selection Rename selection Rotate image Mirror image Setup: Copy setup Display setup Enhancement setup Fax setup Filetype setup E-mail setup Saving setup | In Copy mode, the scanned image is sent directly to the selected printer. ADF-Pages: Select the number of pages that shall be scanned. You can use this with an automatic document feeder (ADF) or by changing the papers by hand while the scanhead moves back. Printer: Select the printer on which the scanned image shall be printed. In the box next to the printer icon you can select the number of copies that shall be created of each scanned image. Paper orientation and image position: portrait: center, top-left, top-right, bottom-left, bottom-right landscape: center, top-left, top-right, bottom-left, bottom-right Zoom factor: Select the zoom factor for the photocopy. XSane automatically selects the correct scan resolution in dependance of the zoom factor and the defined printer resolutions. The options of the printer and the printer command can be set in the menu Preferences/Setup

> Author: Oliver Rauch