Module info:
module can read YUV frames from a given dir (-i option)
it start to search the files: 
0000.yuv 
0001.yuv
... and so on.

If some frames are missing module try to find a next aviable frame 
until it counts MAXFRM (MAXFRM=10000). If You need more - redefine it in
import_yuv.c
Remeber to add the following options to transcode:
-V (only YUV mode is supported)
-g widthxheight   (e.g. -g 384x288)
If red is swapped with blue add option:
-k 

Marek Blaszkowski
mb@intercon.pl
