NEW: transcode Additions
You can reset the filter at a scene change with the do_reset option.
Scenechange thresholds can be controled through
  
  block_thres   every SAD value greater than this will be considered "bad"
                [default 1024]
  scene_thres   Percentage of blocks where motion estimation should fail
                before a scene change is considered
  do_reset      1 = reset the filter after a scene change
                0 = dont reset [default]

 eg:

 transcode -V -i ...
   -J yuvdenoise=mode=2:block_thres=1024:scene_thres=50%:do_reset=1

YUV4MPEG-Denoiser (eventually part of the mjpegtools)
-----------------------------------------------------



1. About
--------

This program can remove noise from your typical video recordings to
increase the compression-ratio to be achieved by mpeg2enc (or if a
fixed bitrate is used, it can dramatically increase the image-
quality). 

The filter mainly reduces color- and luminance-noise and flickering
due to phase errors. It however does *not* do a good job on
color-noise introduced by the common BT8x8 chip-set itself (You will
have noticed, if you ever dared to record vertically reduced sequences
with that chip-set -- say 288 (or 384, or whatever...) lines instead of
full 576 -- that "nice" interleaved color-changes from one line to the
next. This annoying artefact is introduced by BT8x8 chip-set itself, by
only saving one color information for two lines but not interpolating
on the transmitted color-information. Despite of that oddity it has a
reasonable quality for that price... So just record "Full-Pal/NTSC"
and use yuvscaler to downscale your material! The quality is far
better than recording at your destination resolution directly!!!)  




2. Usage
--------

That's really easy! Just pipe a YUV4MPEG-stream into the filter... :)
no switches, no options (NO CARRIER. erm,...) and dare to win (or
loose -- Well, there *is* material which cannot be processed
successfully. It's rare, but it exists! Material containing really
heavy noise is very difficult. So better try it, before you sit and
wait for hours without getting a better result...)

As we now have a border-detection (which is most likely to fail ;-) we
need an option to override it: Just type "yuvdenoise -b xx" being "xx"
any number between 0 (zero, nix, nil, NULL) and a reasonable value
counted from top of the image. That is, "-b 64" will turn the topmost
64 lines in pure black as well as the lowest 64 lines, too... These
black borders seem to be symmetrically ?!? ;-)

My tip: If you can, use this feature (take the value from the
auto-detection as a first guess) as pure YUV-black (16,128,128) is easy
to encode and therefor saves some bits better to be used for the real
frame... Turn this feature off by typing "-b 0"



3. Transcode Usage
------------------
When used within transcode, the filter does provide options.
Usage of the filter is 
  $ transcode ... -J yuvdenoise=help
Provide additional options (not that these are meaningful)
  $ transcode ... -J yuvdenoise=chroma_contrast=50:luma_contrast=120:sharpen=100

The help text is:
denoiser Usage:
===========================================================================

threshold <0..255> denoiser threshold
                   accept any image-error up to +/- threshold for a single
                   pixel to be accepted as valid for the image. If the
                   absolute error is greater than this, exchange the pixel
                   with the according pixel of the reference image.
                   (default=5)

delay <1...255>    Average 'n' frames for a time-lowpassed pixel. Values
                   below 2 will lead to a good response to the reference
                   frame, while larger values will cut out more noise (and
                   as a drawback will lead to noticable artefacts on high
                   motion scenes.) Values above 8 are allowed but rather
                   useless. (default=3)

radius <8...24>    Limit the search radius to that value. Usually it will
                   not make sense to go higher than 16. Esp. for VCD sizes.
                   (default=8)

border <x>,<y>,<w>,<h> Set active image area. Every pixel outside will be set
                   to <16,128,128> ("pure black"). This can save a lot of bits
                   without even touching the image itself (eg. on 16:9 movies
                   on 4:3 (VCD and SVCD) (default=0,0,0,0)

luma_contrast <0...255>    Set luminance contrast in percent. (default=100)

chroma_contrast <0...255>  Set chrominance contrast in percent. AKA "Saturation"
                           (default=100)
sharpen <0...255>  Set sharpness in percent. WARNING: do not set too high
                   as this will gain bit-noise. (default=125)

deinterlace <0..1> Force deinterlacing. By default denoise interlaced.

mode <0..2>        [2]: Fast mode. Use only Pass II (bitnoise-reduction) for
                   low to very low noise material. (default off)
                   [1]: Interlaced material
                   [0]: Progressive material (default)

pp_threshold <0...255>   Pass II threshold (same as -t).
                   WARNING: If set to values greater than 8 you *will* see
                   artefacts...(default=4)

pre <0..1>         [0]: run as a post process filter (default)
                   [1]: run as a pre process filter (not recommended)

block_thres   every SAD value greater than this will be considered "bad"
              [default 1024]

scene_thres   Percentage of blocks where motion estimation should fail
              before a scene is considered changed

do_reset      [1] = reset the filter after a scene change
              [0] = dont reset (default)

 
4. My way of using it...
------------------------

* I record at least 352x576 to 768x576 (PAL) with nuvrec (Roman
  Hochleitner's "NuppelVideo"), eg I use to record double the vertical
  resolution, I finally need! This is important for BT8x8 (it may not
  for Mjpeg based cards -- I don't know...).

* I use exportvideo to get rid of annoying borders and to generate a
  YUV4MPEG-stream which is piped ...

* ... into yuvscaler first(!) --> 352x288

* and then into the filter. (Well, the other way would work, too,
  except that the filter doesn't do interlaced MC yet and doesn't do a
  good job on interlaced frames that way... I'll fix that!)




5. Drawbacks
------------

In rare cases you'll notice very clean blocks directly aside totally
noisy ones... Seeing blocks is probably not what you want to get. 

It uses a MC with a search-radius of 32 pixels. It *will* slow down
the encoding process. (I probably will use i686 asm sometime to
increase speed any further).

I really have tested it on various source material (comics,
commercials, movies, video-clips...) I have not found material which
generally does not work -- but you may encounter such material. If so,
feel free to inform me about this.




Stefan Fendt
<stefan@lionfish.ping.de>

transcode info and port by Tilmann Bitterberg
<transcode@tibit.org>
