###
`#pragma config keyword=symbol,keyword=symbol,..`

This pragma allows to generate a standard `CONFIG` directive in the output code. It replaces the previous `_CONFIGxy` directive. I recommend to switch to the new pragma, because some devices cannot be configured with the old `_CONFIGxy` directive. Moreover, the old directive provokes a warning from `gpasm`.

for example,

    #pragma _CONFIG2L 0x0A
    #pragma _CONFIG2H 0x10

should be replaced with

    #pragma config WDTPS=256,WDT=OFF,BORV=27,BOR=ON,PWRT=ON

You can uses any number of `config` pragmas. For example, the previous pragma could be replaced with

    #pragma config WDTPS=256,WDT=OFF
    #pragma config BORV=27,BOR=ON,PWRT=ON

This pragma can be automatically generated by the config word generator of `PiKdev V1.4`. However, you can write the `config` parameters by yourself. In this case, you will have to refer to the device documentation. Another option is to read the `.inc` file specific to your device to know the available keywords and constants.