- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F26J11
CONFIG1L (address:0x00FFF8, mask:0xE1)
WDTEN -- Watchdog Timer
| WDTEN = OFF | 0xFE | Disabled - Controlled by SWDTEN bit. |
| WDTEN = ON | 0xFF | Enabled. |
STVREN -- Stack Overflow/Underflow Reset
| STVREN = OFF | 0xDF | Disabled. |
| STVREN = ON | 0xFF | Enabled. |
XINST -- Extended Instruction Set
| XINST = OFF | 0xBF | Disabled. |
| XINST = ON | 0xFF | Enabled. |
DEBUG -- Background Debug
| DEBUG = ON | 0x7F | Enabled. |
| DEBUG = OFF | 0xFF | Disabled. |
CONFIG1H (address:0x00FFF9, mask:0xF4)
CP0 -- Code Protect
| CP0 = ON | 0xFB | Program memory is code-protected. |
| CP0 = OFF | 0xFF | Program memory is not code-protected. |
CONFIG2L (address:0x00FFFA, mask:0xDF)
OSC -- Oscillator
| OSC = INTOSC | 0xF8 | INTOSC. |
| OSC = INTOSCO | 0xF9 | INTOSCO (CLKO-RA6). |
| OSC = INTOSCPLL | 0xFA | INTOSCPLL. |
| OSC = INTOSCPLLO | 0xFB | INTOSCPLLO (CLKO-RA6). |
| OSC = HS | 0xFC | HS. |
| OSC = HSPLL | 0xFD | HS+PLL. |
| OSC = EC | 0xFE | EC (CLKO-RA6). |
| OSC = ECPLL | 0xFF | EC+PLL (CLKO-RA6). |
T1DIG -- T1OSCEN Enforcement
| T1DIG = OFF | 0xF7 | Secondary Oscillator clock source may not be selected. |
| T1DIG = ON | 0xFF | Secondary Oscillator clock source may be selected. |
LPT1OSC -- Low-Power Timer1 Oscillator
| LPT1OSC = ON | 0xEF | Low-power operation. |
| LPT1OSC = OFF | 0xFF | High-power operation. |
FCMEN -- Fail-Safe Clock Monitor
| FCMEN = OFF | 0xBF | Disabled. |
| FCMEN = ON | 0xFF | Enabled. |
IESO -- Internal External Oscillator Switch Over Mode
| IESO = OFF | 0x7F | Disabled. |
| IESO = ON | 0xFF | Enabled. |
CONFIG2H (address:0x00FFFB, mask:0xFF)
WDTPS -- Watchdog Postscaler
| WDTPS = 1 | 0xF0 | 1:1. |
| WDTPS = 2 | 0xF1 | 1:2. |
| WDTPS = 4 | 0xF2 | 1:4. |
| WDTPS = 8 | 0xF3 | 1:8. |
| WDTPS = 16 | 0xF4 | 1:16. |
| WDTPS = 32 | 0xF5 | 1:32. |
| WDTPS = 64 | 0xF6 | 1:64. |
| WDTPS = 128 | 0xF7 | 1:128. |
| WDTPS = 256 | 0xF8 | 1:256. |
| WDTPS = 512 | 0xF9 | 1:512. |
| WDTPS = 1024 | 0xFA | 1:1024. |
| WDTPS = 2048 | 0xFB | 1:2048. |
| WDTPS = 4096 | 0xFC | 1:4096. |
| WDTPS = 8192 | 0xFD | 1:8192. |
| WDTPS = 16384 | 0xFE | 1:16384. |
| WDTPS = 32768 | 0xFF | 1:32768. |
CONFIG3L (address:0x00FFFC, mask:0xFF)
DSWDTOSC -- DSWDT Clock Select
| DSWDTOSC = T1OSCREF | 0xFE | DSWDT uses T1OSC/T1CKI. |
| DSWDTOSC = INTOSCREF | 0xFF | DSWDT uses INTRC. |
RTCOSC -- RTCC Clock Select
| RTCOSC = INTOSCREF | 0xFD | RTCC uses INTRC. |
| RTCOSC = T1OSCREF | 0xFF | RTCC uses T1OSC/T1CKI. |
DSBOREN -- Deep Sleep BOR
| DSBOREN = OFF | 0xFB | Disabled. |
| DSBOREN = ON | 0xFF | Enabled. |
DSWDTEN -- Deep Sleep Watchdog Timer
| DSWDTEN = OFF | 0xF7 | Disabled. |
| DSWDTEN = ON | 0xFF | Enabled. |
DSWDTPS -- Deep Sleep Watchdog Postscaler
| DSWDTPS = 2 | 0x0F | 1:2 (2.1 ms). |
| DSWDTPS = 8 | 0x1F | 1:8 (8.3 ms). |
| DSWDTPS = 32 | 0x2F | 1:32 (33 ms). |
| DSWDTPS = 128 | 0x3F | 1:128 (132 ms). |
| DSWDTPS = 512 | 0x4F | 1:512 (528 ms). |
| DSWDTPS = 2048 | 0x5F | 1:2,048 (2.1 seconds). |
| DSWDTPS = 8192 | 0x6F | 1:8,192 (8.5 seconds). |
| DSWDTPS = K32 | 0x7F | 1:32,768 (34 seconds). |
| DSWDTPS = K131 | 0x8F | 1:131,072 (135 seconds). |
| DSWDTPS = K524 | 0x9F | 1:524,288 (9 minutes). |
| DSWDTPS = M2 | 0xAF | 1:2,097,152 (36 minutes). |
| DSWDTPS = M8 | 0xBF | 1:8,388,608 (2.4 hours). |
| DSWDTPS = M33 | 0xCF | 1:33,554,432 (9.6 hours). |
| DSWDTPS = M134 | 0xDF | 1:134,217,728 (38.5 hours). |
| DSWDTPS = M536 | 0xEF | 1:536,870,912 (6.4 days). |
| DSWDTPS = G2 | 0xFF | 1:2,147,483,648 (25.7 days). |
CONFIG3H (address:0x00FFFD, mask:0xF9)
IOL1WAY -- IOLOCK One-Way Set Enable bit
| IOL1WAY = OFF | 0xFE | The IOLOCK bit (PPSCON<0>) can be set and cleared as needed. |
| IOL1WAY = ON | 0xFF | The IOLOCK bit (PPSCON<0>) can be set once. |
MSSP7B_EN -- MSSP address masking
| MSSP7B_EN = MSK5 | 0xF7 | 5 Bit address masking mode. |
| MSSP7B_EN = MSK7 | 0xFF | 7 Bit address masking mode. |
CONFIG4L (address:0x00FFFE, mask:0xFF)
WPFP -- Write/Erase Protect Page Start/End Location
| WPFP = PAGE_0 | 0xC0 | Write Protect Program Flash Page 0. |
| WPFP = PAGE_1 | 0xC1 | Write Protect Program Flash Page 1. |
| WPFP = PAGE_2 | 0xC2 | Write Protect Program Flash Page 2. |
| WPFP = PAGE_3 | 0xC3 | Write Protect Program Flash Page 3. |
| WPFP = PAGE_4 | 0xC4 | Write Protect Program Flash Page 4. |
| WPFP = PAGE_5 | 0xC5 | Write Protect Program Flash Page 5. |
| WPFP = PAGE_6 | 0xC6 | Write Protect Program Flash Page 6. |
| WPFP = PAGE_7 | 0xC7 | Write Protect Program Flash Page 7. |
| WPFP = PAGE_8 | 0xC8 | Write Protect Program Flash Page 8. |
| WPFP = PAGE_9 | 0xC9 | Write Protect Program Flash Page 9. |
| WPFP = PAGE_10 | 0xCA | Write Protect Program Flash Page 10. |
| WPFP = PAGE_11 | 0xCB | Write Protect Program Flash Page 11. |
| WPFP = PAGE_12 | 0xCC | Write Protect Program Flash Page 12. |
| WPFP = PAGE_13 | 0xCD | Write Protect Program Flash Page 13. |
| WPFP = PAGE_14 | 0xCE | Write Protect Program Flash Page 14. |
| WPFP = PAGE_15 | 0xCF | Write Protect Program Flash Page 15. |
| WPFP = PAGE_16 | 0xD0 | Write Protect Program Flash Page 16. |
| WPFP = PAGE_17 | 0xD1 | Write Protect Program Flash Page 17. |
| WPFP = PAGE_18 | 0xD2 | Write Protect Program Flash Page 18. |
| WPFP = PAGE_19 | 0xD3 | Write Protect Program Flash Page 19. |
| WPFP = PAGE_20 | 0xD4 | Write Protect Program Flash Page 20. |
| WPFP = PAGE_21 | 0xD5 | Write Protect Program Flash Page 21. |
| WPFP = PAGE_22 | 0xD6 | Write Protect Program Flash Page 22. |
| WPFP = PAGE_23 | 0xD7 | Write Protect Program Flash Page 23. |
| WPFP = PAGE_24 | 0xD8 | Write Protect Program Flash Page 24. |
| WPFP = PAGE_25 | 0xD9 | Write Protect Program Flash Page 25. |
| WPFP = PAGE_26 | 0xDA | Write Protect Program Flash Page 26. |
| WPFP = PAGE_27 | 0xDB | Write Protect Program Flash Page 27. |
| WPFP = PAGE_28 | 0xDC | Write Protect Program Flash Page 28. |
| WPFP = PAGE_29 | 0xDD | Write Protect Program Flash Page 29. |
| WPFP = PAGE_30 | 0xDE | Write Protect Program Flash Page 30. |
| WPFP = PAGE_31 | 0xDF | Write Protect Program Flash Page 31. |
| WPFP = PAGE_32 | 0xE0 | Write Protect Program Flash Page 32. |
| WPFP = PAGE_33 | 0xE1 | Write Protect Program Flash Page 33. |
| WPFP = PAGE_34 | 0xE2 | Write Protect Program Flash Page 34. |
| WPFP = PAGE_35 | 0xE3 | Write Protect Program Flash Page 35. |
| WPFP = PAGE_36 | 0xE4 | Write Protect Program Flash Page 36. |
| WPFP = PAGE_37 | 0xE5 | Write Protect Program Flash Page 37. |
| WPFP = PAGE_38 | 0xE6 | Write Protect Program Flash Page 38. |
| WPFP = PAGE_39 | 0xE7 | Write Protect Program Flash Page 39. |
| WPFP = PAGE_40 | 0xE8 | Write Protect Program Flash Page 40. |
| WPFP = PAGE_41 | 0xE9 | Write Protect Program Flash Page 41. |
| WPFP = PAGE_42 | 0xEA | Write Protect Program Flash Page 42. |
| WPFP = PAGE_43 | 0xEB | Write Protect Program Flash Page 43. |
| WPFP = PAGE_44 | 0xEC | Write Protect Program Flash Page 44. |
| WPFP = PAGE_45 | 0xED | Write Protect Program Flash Page 45. |
| WPFP = PAGE_46 | 0xEE | Write Protect Program Flash Page 46. |
| WPFP = PAGE_47 | 0xEF | Write Protect Program Flash Page 47. |
| WPFP = PAGE_48 | 0xF0 | Write Protect Program Flash Page 48. |
| WPFP = PAGE_49 | 0xF1 | Write Protect Program Flash Page 49. |
| WPFP = PAGE_50 | 0xF2 | Write Protect Program Flash Page 50. |
| WPFP = PAGE_51 | 0xF3 | Write Protect Program Flash Page 51. |
| WPFP = PAGE_52 | 0xF4 | Write Protect Program Flash Page 52. |
| WPFP = PAGE_53 | 0xF5 | Write Protect Program Flash Page 53. |
| WPFP = PAGE_54 | 0xF6 | Write Protect Program Flash Page 54. |
| WPFP = PAGE_55 | 0xF7 | Write Protect Program Flash Page 55. |
| WPFP = PAGE_56 | 0xF8 | Write Protect Program Flash Page 56. |
| WPFP = PAGE_57 | 0xF9 | Write Protect Program Flash Page 57. |
| WPFP = PAGE_58 | 0xFA | Write Protect Program Flash Page 58. |
| WPFP = PAGE_59 | 0xFB | Write Protect Program Flash Page 59. |
| WPFP = PAGE_60 | 0xFC | Write Protect Program Flash Page 60. |
| WPFP = PAGE_61 | 0xFD | Write Protect Program Flash Page 61. |
| WPFP = PAGE_62 | 0xFE | Write Protect Program Flash Page 62. |
| WPFP = PAGE_63 | 0xFF | Write Protect Program Flash Page 63. |
WPEND -- Write/Erase Protect Region Select (valid when WPDIS = 0)
| WPEND = PAGE_0 | 0xBF | Page 0 through WPFP<5:0> erase/write protected. |
| WPEND = PAGE_WPFP | 0xFF | Page WPFP<5:0> through Configuration Words erase/write protected. |
WPCFG -- Write/Erase Protect Configuration Region
| WPCFG = ON | 0x7F | Configuration Words page erase/write-protected. |
| WPCFG = OFF | 0xFF | Configuration Words page not erase/write-protected. |
CONFIG4H (address:0x00FFFF, mask:0xF1)
WPDIS -- Write Protect Disable bit
| WPDIS = ON | 0xFE | WPFP<5:0>/WPEND region erase/write protected. |
| WPDIS = OFF | 0xFF | WPFP<5:0>/WPEND region ignored. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:28 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.