- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F1828
CONFIG1 (address:0x8007, mask:0xFFFF)
FOSC -- Oscillator Selection
| FOSC = LP | 0xFFF8 | LP Oscillator, Low-power crystal connected between OSC1 and OSC2 pins. |
| FOSC = XT | 0xFFF9 | XT Oscillator, Crystal/resonator connected between OSC1 and OSC2 pins. |
| FOSC = HS | 0xFFFA | HS Oscillator, High-speed crystal/resonator connected between OSC1 and OSC2 pins. |
| FOSC = EXTRC | 0xFFFB | EXTRC oscillator: External RC circuit connected to CLKIN pin. |
| FOSC = INTOSC | 0xFFFC | INTOSC oscillator: I/O function on CLKIN pin. |
| FOSC = ECL | 0xFFFD | ECL, External Clock, Low Power Mode (0-0.5 MHz): device clock supplied to CLKIN pin. |
| FOSC = ECM | 0xFFFE | ECM, External Clock, Medium Power Mode (0.5-4 MHz): device clock supplied to CLKIN pin. |
| FOSC = ECH | 0xFFFF | ECH, External Clock, High Power Mode (4-32 MHz): device clock supplied to CLKIN pin. |
WDTE -- Watchdog Timer Enable
| WDTE = OFF | 0xFFE7 | WDT disabled. |
| WDTE = SWDTEN | 0xFFEF | WDT controlled by the SWDTEN bit in the WDTCON register. |
| WDTE = NSLEEP | 0xFFF7 | WDT enabled while running and disabled in Sleep. |
| WDTE = ON | 0xFFFF | WDT enabled. |
PWRTE -- Power-up Timer Enable
| PWRTE = ON | 0xFFDF | PWRT enabled. |
| PWRTE = OFF | 0xFFFF | PWRT disabled. |
MCLRE -- MCLR Pin Function Select
| MCLRE = OFF | 0xFFBF | MCLR/VPP pin function is digital input. |
| MCLRE = ON | 0xFFFF | MCLR/VPP pin function is MCLR. |
CP -- Flash Program Memory Code Protection
| CP = ON | 0xFF7F | Program memory code protection is enabled. |
| CP = OFF | 0xFFFF | Program memory code protection is disabled. |
CPD -- Data Memory Code Protection
| CPD = ON | 0xFEFF | Data memory code protection is enabled. |
| CPD = OFF | 0xFFFF | Data memory code protection is disabled. |
BOREN -- Brown-out Reset Enable
| BOREN = OFF | 0xF9FF | Brown-out Reset disabled. |
| BOREN = SBODEN | 0xFBFF | Brown-out Reset controlled by the SBOREN bit in the BORCON register. |
| BOREN = NSLEEP | 0xFDFF | Brown-out Reset enabled while running and disabled in Sleep. |
| BOREN = ON | 0xFFFF | Brown-out Reset enabled. |
CLKOUTEN -- Clock Out Enable
| CLKOUTEN = ON | 0xF7FF | CLKOUT function is enabled on the CLKOUT pin. |
| CLKOUTEN = OFF | 0xFFFF | CLKOUT function is disabled. I/O or oscillator function on the CLKOUT pin. |
IESO -- Internal/External Switchover
| IESO = OFF | 0xEFFF | Internal/External Switchover mode is disabled. |
| IESO = ON | 0xFFFF | Internal/External Switchover mode is enabled. |
FCMEN -- Fail-Safe Clock Monitor Enable
| FCMEN = OFF | 0xDFFF | Fail-Safe Clock Monitor is disabled. |
| FCMEN = ON | 0xFFFF | Fail-Safe Clock Monitor is enabled. |
CONFIG2 (address:0x8008, mask:0xFFFF)
WRT -- Flash Memory Self-Write Protection
| WRT = ALL | 0xFFFC | 000h to FFFh write protected, no addresses may be modified by EECON control. |
| WRT = HALF | 0xFFFD | 000h to 7FFh write protected, 800h to FFFh may be modified by EECON control. |
| WRT = BOOT | 0xFFFE | 000h to 1FFh write protected, 200h to FFFh may be modified by EECON control. |
| WRT = OFF | 0xFFFF | Write protection off. |
PLLEN -- PLL Enable
| PLLEN = OFF | 0xFEFF | 4x PLL disabled. |
| PLLEN = ON | 0xFFFF | 4x PLL enabled. |
STVREN -- Stack Overflow/Underflow Reset Enable
| STVREN = OFF | 0xFDFF | Stack Overflow or Underflow will not cause a Reset. |
| STVREN = ON | 0xFFFF | Stack Overflow or Underflow will cause a Reset. |
BORV -- Brown-out Reset Voltage Selection
| BORV = HI | 0xFBFF | Brown-out Reset Voltage (Vbor), high trip point selected. |
| BORV = LO | 0xFFFF | Brown-out Reset Voltage (Vbor), low trip point selected. |
LVP -- Low-Voltage Programming Enable
| LVP = OFF | 0xDFFF | High-voltage on MCLR/VPP must be used for programming. |
| LVP = ON | 0xFFFF | Low-voltage programming enabled. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.