- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F1782
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 10 |  | Bank 16 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PORTE | 0x010
PIR1 | 0x011
PIR2 | 0x012
PIR4 | 0x014
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TMR2 | 0x01A
PR2 | 0x01B
T2CON | 0x01C
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
TRISE | 0x090
PIE1 | 0x091
PIE2 | 0x092
PIE4 | 0x094
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCTUNE | 0x098
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
ADCON2 | 0x09F
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
CM1CON0 | 0x111
CM1CON1 | 0x112
CM2CON0 | 0x113
CM2CON1 | 0x114
CMOUT | 0x115
BORCON | 0x116
FVRCON | 0x117
DACCON0 | 0x118
DACCON1 | 0x119
APFCONAPFCON0 | 0x11D
CM3CON0 | 0x11E
CM3CON1 | 0x11F
ANSELA | 0x18C
ANSELB | 0x18D
EEADREEADRL | 0x191
EEADRH | 0x192
EEDATEEDATL | 0x193
EEDATH | 0x194
EECON1 | 0x195
EECON2 | 0x196
VREGCON | 0x197
RC1REGRCREG RCREG1 | 0x199
TX1REGTXREG TXREG1 | 0x19A
SP1BRGSP1BRGL SPBRG SPBRG1 SPBRGL | 0x19B
SP1BRGHSPBRGH SPBRGH1 | 0x19C
RC1STARCSTA RCSTA1 | 0x19D
TX1STATXSTA TXSTA1 | 0x19E
BAUD1CONBAUDCON BAUDCON1 BAUDCTL BAUDCTL1 | 0x19F
WPUA | 0x20C
WPUB | 0x20D
WPUC | 0x20E
WPUE | 0x210
SSP1BUFSSPBUF | 0x211
SSP1ADDSSPADD | 0x212
SSP1MSKSSPMSK | 0x213
SSP1STATSSPSTAT | 0x214
SSP1CONSSPCON SSPCON1 | 0x215
SSP1CON2SSPCON2 | 0x216
SSP1CON3SSPCON3 | 0x217
ODCONA | 0x28C
ODCONB | 0x28D
ODCONC | 0x28E
CCPR1CCPR1L | 0x291
CCPR1H | 0x292
CCP1CON | 0x293
CCPR2CCPR2L | 0x298
CCPR2H | 0x299
CCP2CON | 0x29A
SLRCONA | 0x30C
SLRCONB | 0x30D
SLRCONC | 0x30E
INLVLA | 0x38C
INLVLB | 0x38D
INLVLC | 0x38E
INLVLE | 0x390
IOCAP | 0x391
IOCAN | 0x392
IOCAF | 0x393
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
IOCCP | 0x397
IOCCN | 0x398
IOCCF | 0x399
IOCEP | 0x39D
IOCEN | 0x39E
IOCEF | 0x39F
OPA1CON | 0x511
OPA2CON | 0x513
CLKRCON | 0x51A
PSMC1CON | 0x811
PSMC1MDL | 0x812
PSMC1SYNC | 0x813
PSMC1CLK | 0x814
PSMC1OEN | 0x815
PSMC1POL | 0x816
PSMC1BLNK | 0x817
PSMC1REBS | 0x818
PSMC1FEBS | 0x819
PSMC1PHS | 0x81A
PSMC1DCS | 0x81B
PSMC1PRS | 0x81C
PSMC1ASDC | 0x81D
PSMC1ASDL | 0x81E
PSMC1ASDS | 0x81F
PSMC1INT | 0x820
PSMC1PHPSMC1PHL | 0x821
PSMC1PHH | 0x822
PSMC1DCPSMC1DCL | 0x823
PSMC1DCH | 0x824
PSMC1PRPSMC1PRL | 0x825
PSMC1PRH | 0x826
PSMC1TMRPSMC1TMRL | 0x827
PSMC1TMRH | 0x828
PSMC1DBR | 0x829
PSMC1DBF | 0x82A
PSMC1BLKR | 0x82B
PSMC1BLKF | 0x82C
PSMC1FFA | 0x82D
PSMC1STR0 | 0x82E
PSMC1STR1 | 0x82F
PSMC2CON | 0x831
PSMC2MDL | 0x832
PSMC2SYNC | 0x833
PSMC2CLK | 0x834
PSMC2OEN | 0x835
PSMC2POL | 0x836
PSMC2BLNK | 0x837
PSMC2REBS | 0x838
PSMC2FEBS | 0x839
PSMC2PHS | 0x83A
PSMC2DCS | 0x83B
PSMC2PRS | 0x83C
PSMC2ASDC | 0x83D
PSMC2ASDL | 0x83E
PSMC2ASDS | 0x83F
PSMC2INT | 0x840
PSMC2PHPSMC2PHL | 0x841
PSMC2PHH | 0x842
PSMC2DCPSMC2DCL | 0x843
PSMC2DCH | 0x844
PSMC2PRPSMC2PRL | 0x845
PSMC2PRH | 0x846
PSMC2TMRPSMC2TMRL | 0x847
PSMC2TMRH | 0x848
PSMC2DBR | 0x849
PSMC2DBF | 0x84A
PSMC2BLKR | 0x84B
PSMC2BLKF | 0x84C
PSMC2FFA | 0x84D
PSMC2STR0 | 0x84E
PSMC2STR1 | 0x84F
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.