- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F57
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| Shared 0x000 - 0x00F 16 bytes GPR 0x010 - 0x01F 16 bytes |  | Shared 0x020 - 0x02F 16 bytes GPR 0x030 - 0x03F 16 bytes |  | Shared 0x040 - 0x04F 16 bytes GPR 0x050 - 0x05F 16 bytes |  | Shared 0x060 - 0x06F 16 bytes GPR 0x070 - 0x07F 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 16 bytes Shared 16 bytes Unimplemented 0 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.