- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PICRF509AG
CONFIG (address:0x0FFF, mask:0xFFFF)
OSC -- Oscillator selection bits
| OSC = LP | 0x0FFC | LP oscillator. |
| OSC = XT | 0x0FFD | XT oscillator. |
| OSC = IntRC | 0x0FFE | internal RC oscillator. |
| OSC = ExtRC | 0x0FFF | external RC oscillator. |
WDT -- Watchdog timer enable bit
| WDT = OFF | 0x0FFB | WDT disabled. |
| WDT = ON | 0x0FFF | WDT enabled. |
CP -- Code protection bit
| CP = ON | 0x0FF7 | Code protection on. |
| CP = OFF | 0x0FFF | Code protection off. |
MCLRE -- MCLR enable bit
| MCLRE = OFF | 0x0FEF | MCLR tied to VDD, (Internally). |
| MCLRE = ON | 0x0FFF | MCLR pin enabled. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:30 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.