- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F96J99
| Coff ID of device | 0x9699 |
| Last address of ROM/FLASH | 0x017FEF (98288 bytes)
| Address space of Configuration Bytes | 0x017FF0 - 0x017FFF (16 bytes)
| Address space of Device ID | 0x3FFFFE - 0x3FFFFF (2 bytes)
| Number of RAM Banks | 16 (256 bytes/banks)
| Number of SFRs | 512
| Size of GPRs | 3578 bytes
| Joint size of SFRs + GPRs | 4090 bytes
| Last address of lower Access RAM | 0x5F

This page generated automatically by the device-help.pl program (2013-08-01 15:50:29 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.