- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16HV616
| Bank 0 |  | Bank 1 |
| SFR 0x000 - 0x005 6 bytes Unimplemented 0x006 SFR 0x007 Unimplemented 0x008 - 0x009 2 bytes SFR 0x00A - 0x00C 3 bytes Unimplemented 0x00D SFR 0x00E - 0x017 10 bytes Unimplemented 0x018 SFR 0x019 - 0x01C 4 bytes Unimplemented 0x01D SFR 0x01E - 0x01F 2 bytes GPR 0x020 - 0x06F 80 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x085 6 bytes Unimplemented 0x086 SFR 0x087 Unimplemented 0x088 - 0x089 2 bytes SFR 0x08A - 0x08C 3 bytes Unimplemented 0x08D SFR 0x08E Unimplemented 0x08F SFR 0x090 - 0x092 3 bytes Unimplemented 0x093 - 0x094 2 bytes SFR 0x095 - 0x096 2 bytes Unimplemented 0x097 - 0x098 2 bytes SFR 0x099 - 0x09A 2 bytes Unimplemented 0x09B - 0x09D 3 bytes SFR 0x09E - 0x09F 2 bytes GPR 0x0A0 - 0x0BF 32 bytes Unimplemented 0x0C0 - 0x0EF 48 bytes Shared 0x0F0 - 0x0FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 26 bytes GPR 80 bytes Shared 16 bytes Unimplemented 6 bytes |  | SFR 20 bytes GPR 32 bytes Shared 16 bytes Unimplemented 60 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.