- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12HV752
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
PORTA | 0x005
IOCAF | 0x008
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
PIR2 | 0x00D
TMR1TMR1L | 0x00F
TMR1H | 0x010
T1CON | 0x011
T1GCON | 0x012
CCPR1CCPR1L | 0x013
CCPR1H | 0x014
CCP1CON | 0x015
ADRESADRESL | 0x01C
ADRESH | 0x01D
ADCON0 | 0x01E
ADCON1 | 0x01F
OPTION_REG | 0x081
TRISA | 0x085
IOCAP | 0x088
PIE1 | 0x08C
PIE2 | 0x08D
OSCCON | 0x08F
FVRCON | 0x090
DACCON0 | 0x091
DACCON1 | 0x092
C2CON0CM2CON0 | 0x09B
C2CON1CM2CON1 | 0x09C
C1CON0CM1CON0 | 0x09D
C1CON1CM1CON1 | 0x09E
CMOUTMCOUT | 0x09F
LATA | 0x105
IOCAN | 0x108
WPUA | 0x10C
SLRCONA | 0x10D
PCON | 0x10F
TMR2 | 0x110
PR2 | 0x111
T2CON | 0x112
HLTMR1 | 0x113
HLTPR1 | 0x114
HLT1CON0 | 0x115
HLT1CON1 | 0x116
ANSELA | 0x185
APFCON | 0x188
OSCTUNE | 0x189
PMCON1 | 0x18C
PMCON2 | 0x18D
PMADRPMADRL | 0x18E
PMADRH | 0x18F
PMDATPMDATL | 0x190
PMDATH | 0x191
COG1PH | 0x192
COG1BLK | 0x193
COG1DB | 0x194
COG1CON0 | 0x195
COG1CON1 | 0x196
COG1ASD | 0x197
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.