Informations about the PIC microcontrollers

- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

| name | config word size (bit) | class |
| PIC10F200 | 12 | regular |
| PIC10F202 | 12 | regular |
| PIC10F204 | 12 | regular |
| PIC10F206 | 12 | regular |
| PIC10F220 | 12 | regular |
| PIC10F222 | 12 | regular |
| PIC12C508 | 12 | regular |
| PIC12C508A | 12 | regular |
| PIC12C509 | 12 | regular |
| PIC12C509A | 12 | regular |
| PIC12CE518 | 12 | regular |
| PIC12CE519 | 12 | regular |
| PIC12CR509A | 12 | regular |
| PIC12F508 | 12 | regular |
| PIC12F509 | 12 | regular |
| PIC12F510 | 12 | regular |
| PIC12F519 | 12 | regular |
| PIC12F520 | 12 | regular |
| PIC12F529T39A | 12 | enhanced |
| PIC12F529T48A | 12 | enhanced |
| PIC16C505 | 12 | regular |
| PIC16F54 | 12 | regular |
| PIC16F57 | 12 | regular |
| PIC16F59 | 12 | regular |
| PIC16F505 | 12 | regular |
| PIC16F506 | 12 | regular |
| PIC16F526 | 12 | regular |
| PIC16F527 | 12 | enhanced |
| PIC16F570 | 12 | enhanced |
| PIC16HV540 | 12 | regular |
| PICRF509AF | 12 | regular |
| PICRF509AG | 12 | regular |

12 bit MCU

14 bit MCU

16 bit MCU

12 bit enhanced MCU

14 bit enhanced MCU

16 bit extended MCU

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.