- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12CE674
| Bank 0 |  | Bank 1 |
INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
GPIO | 0x005
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
ADRES | 0x01E
ADCON0 | 0x01F
OPTION_REG | 0x081
TRISIO | 0x085
PIE1 | 0x08C
PCON | 0x08E
OSCCAL | 0x08F
ADCON1 | 0x09F
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.