- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1904
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 7 |  | Bank 15 |  | Bank 31 |
INDF0 | 0x000
INDF1 | 0x001
PCL | 0x002
STATUS | 0x003
FSR0FSR0L | 0x004
FSR0H | 0x005
FSR1FSR1L | 0x006
FSR1H | 0x007
BSR | 0x008
WREG | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PORTA | 0x00C
PORTB | 0x00D
PORTC | 0x00E
PORTD | 0x00F
PORTE | 0x010
PIR1 | 0x011
PIR2 | 0x012
TMR0 | 0x015
TMR1TMR1L | 0x016
TMR1H | 0x017
T1CON | 0x018
T1GCON | 0x019
TRISA | 0x08C
TRISB | 0x08D
TRISC | 0x08E
TRISD | 0x08F
TRISE | 0x090
PIE1 | 0x091
PIE2 | 0x092
OPTION_REG | 0x095
PCON | 0x096
WDTCON | 0x097
OSCCON | 0x099
OSCSTAT | 0x09A
ADRESADRESL | 0x09B
ADRESH | 0x09C
ADCON0 | 0x09D
ADCON1 | 0x09E
LATA | 0x10C
LATB | 0x10D
LATC | 0x10E
LATD | 0x10F
LATE | 0x110
BORCON | 0x116
FVRCON | 0x117
ANSELA | 0x18C
ANSELB | 0x18D
ANSELE | 0x190
PMADRPMADRL | 0x191
PMADRH | 0x192
PMDATPMDATL | 0x193
PMDATH | 0x194
PMCON1 | 0x195
PMCON2 | 0x196
RC1REGRCREG RCREG1 | 0x199
TX1REGTXREG TXREG1 | 0x19A
SP1BRGLSPBRG SPBRGL SPBRGL1 | 0x19B
SP1BRGHSPBRGH SPBRGH1 | 0x19C
RC1STARCSTA RCSTA1 | 0x19D
TX1STATXSTA TXSTA1 | 0x19E
BAUD1CONBAUDCON BAUDCON1 | 0x19F
WPUB | 0x20D
WPUE | 0x210
IOCBP | 0x394
IOCBN | 0x395
IOCBF | 0x396
LCDCON | 0x791
LCDPS | 0x792
LCDREF | 0x793
LCDCST | 0x794
LCDRL | 0x795
LCDSE0 | 0x798
LCDSE1 | 0x799
LCDSE2 | 0x79A
LCDSE3 | 0x79B
LCDDATA0 | 0x7A0
LCDDATA1 | 0x7A1
LCDDATA2 | 0x7A2
LCDDATA3 | 0x7A3
LCDDATA4 | 0x7A4
LCDDATA5 | 0x7A5
LCDDATA6 | 0x7A6
LCDDATA7 | 0x7A7
LCDDATA8 | 0x7A8
LCDDATA9 | 0x7A9
LCDDATA10 | 0x7AA
LCDDATA11 | 0x7AB
LCDDATA12 | 0x7AC
LCDDATA15 | 0x7AF
LCDDATA18 | 0x7B2
LCDDATA21 | 0x7B5
STATUS_SHAD | 0xFE4
WREG_SHAD | 0xFE5
BSR_SHAD | 0xFE6
PCLATH_SHAD | 0xFE7
FSR0L_SHAD | 0xFE8
FSR0H_SHAD | 0xFE9
FSR1L_SHAD | 0xFEA
FSR1H_SHAD | 0xFEB
STKPTR | 0xFED
TOSL | 0xFEE
TOSH | 0xFEF
The mirror of [PCL, STATUS, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.