- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12HV615
CONFIG (address:0x2007, mask:0xFFFF)
FOSC -- Oscillator Selection bits
| FOSC = LP | 0x3FF8 | LP oscillator: Low-power crystal on GP4/OSC2/CLKOUT and GP5/OSC1/CLKIN. |
| FOSC = XT | 0x3FF9 | XT oscillator: Crystal/resonator on GP4/OSC2/CLKOUT and GP5/OSC1/CLKIN. |
| FOSC = HS | 0x3FFA | HS oscillator: High-speed crystal/resonator on GP4/OSC2/CLKOUT and GP5/OSC1/CLKIN. |
| FOSC = EC | 0x3FFB | EC: I/O function on GP4/OSC2/CLKOUT pin, CLKIN on GP5/OSC1/CLKIN. |
| FOSC = INTOSCIO | 0x3FFC | INTOSCIO oscillator: I/O function on GP4/OSC2/CLKOUT pin, I/O function on GP5/OSC1/CLKIN. |
| FOSC = INTOSCCLK | 0x3FFD | INTOSC oscillator: CLKOUT function on GP4/OSC2/CLKOUT pin, I/O function on GP5/OSC1/CLKIN. |
| FOSC = EXTRCIO | 0x3FFE | RCIO oscillator: I/O function on GP4/OSC2/CLKOUT pin, RC on GP5/OSC1/CLKIN. |
| FOSC = EXTRCCLK | 0x3FFF | RC oscillator: CLKOUT function on GP4/OSC2/CLKOUT pin, RC on GP5/OSC1/CLKIN. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x3FF7 | WDT disabled and can be enabled by SWDTEN bit of the WDTCON register. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FEF | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
MCLRE -- MCLR Pin Function Select bit
| MCLRE = OFF | 0x3FDF | MCLR pin function is digital input, MCLR internally tied to VDD. |
| MCLRE = ON | 0x3FFF | MCLR pin function is MCLR. |
CP -- Code Protection bit
| CP = ON | 0x3FBF | Program memory code protection is enabled. |
| CP = OFF | 0x3FFF | Program memory code protection is disabled. |
IOSCFS -- Internal Oscillator Frequency Select
| IOSCFS = 4MHZ | 0x3F7F | 4 MHz. |
| IOSCFS = 8MHZ | 0x3FFF | 8 MHz. |
BOREN -- Brown-out Reset Selection bits
| BOREN = OFF | 0x3CFF | BOR disabled. |
| BOREN = NSLEEP | 0x3EFF | BOR enabled during operation and disabled in Sleep. |
| BOREN = ON | 0x3FFF | BOR enabled. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.