- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12F752
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |
| SFR 0x000 - 0x005 6 bytes Unimplemented 0x006 - 0x007 2 bytes SFR 0x008 Unimplemented 0x009 SFR 0x00A - 0x00D 4 bytes Unimplemented 0x00E SFR 0x00F - 0x015 7 bytes Unimplemented 0x016 - 0x01B 6 bytes SFR 0x01C - 0x01F 4 bytes Unimplemented 0x020 - 0x03F 32 bytes GPR 0x040 - 0x06F 48 bytes Shared 0x070 - 0x07F 16 bytes |  | SFR 0x080 - 0x085 6 bytes Unimplemented 0x086 - 0x087 2 bytes SFR 0x088 Unimplemented 0x089 SFR 0x08A - 0x08D 4 bytes Unimplemented 0x08E SFR 0x08F - 0x092 4 bytes Unimplemented 0x093 - 0x09A 8 bytes SFR 0x09B - 0x09F 5 bytes Unimplemented 0x0A0 - 0x0EF 80 bytes Shared 0x0F0 - 0x0FF 16 bytes |  | SFR 0x100 Unimplemented 0x101 SFR 0x102 - 0x105 4 bytes Unimplemented 0x106 - 0x107 2 bytes SFR 0x108 Unimplemented 0x109 SFR 0x10A - 0x10D 4 bytes Unimplemented 0x10E SFR 0x10F - 0x116 8 bytes Unimplemented 0x117 - 0x16F 89 bytes Shared 0x170 - 0x17F 16 bytes |  | SFR 0x180 Unimplemented 0x181 SFR 0x182 - 0x185 4 bytes Unimplemented 0x186 - 0x187 2 bytes SFR 0x188 - 0x197 16 bytes Unimplemented 0x198 - 0x1EF 88 bytes Shared 0x1F0 - 0x1FF 16 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 22 bytes GPR 48 bytes Shared 16 bytes Unimplemented 42 bytes |  | SFR 20 bytes GPR 0 bytes Shared 16 bytes Unimplemented 92 bytes |  | SFR 18 bytes GPR 0 bytes Shared 16 bytes Unimplemented 94 bytes |  | SFR 21 bytes GPR 0 bytes Shared 16 bytes Unimplemented 91 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.