- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F610
| Coff ID of device | 0xF610 |
| Number of ROM/FLASH pages | 0 (2048 words/pages)
| Last address of ROM/FLASH | 0x03FF (1024 words)
| Address space of User ID | 0x2000 - 0x2003 (4 bytes)
| Address of Device ID | 0x2006 (1 byte)
| Address of Configuration Word | 0x2007 (1 word)
| Number of RAM Banks | 2 (128 bytes/banks)
| Number of SFRs | 28
| Size of GPRs | 86 bytes
| Joint size of SFRs + GPRs | 114 bytes

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.