- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F570
CONFIG (address:0x0FFF, mask:0x03FF)
FOSC -- Oscillator
| FOSC = LP | 0x0FF8 | LP oscillator and 18 ms DRT. |
| FOSC = XT | 0x0FF9 | XT oscillator and 18 ms DRT. |
| FOSC = HS | 0x0FFA | HS oscillator and 18 ms DRT. |
| FOSC = EC | 0x0FFB | EC oscillator with I/O function on OSC2/CLKOUT. |
| FOSC = INTRC_IO | 0x0FFC | INTRC with I/O function on OSC2/CLKOUT. |
| FOSC = INTRC_CLKOUT | 0x0FFD | INTRC with CLKOUT function on OSC2/CLKOUT. |
| FOSC = EXTRC_IO | 0x0FFE | EXTRC with I/O function on OSC2/CLKOUT. |
| FOSC = EXTRC_CLKOUT | 0x0FFF | EXTRC with CLKOUT function on OSC2/CLKOUT. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x0FF7 | Disabled. |
| WDTE = ON | 0x0FFF | Enabled. |
CP -- Code Protection bit
| CP = ON | 0x0FEF | Code protection on. |
| CP = OFF | 0x0FFF | Code protection off. |
IOSCFS -- Internal Oscillator Frequency Select
| IOSCFS = 4MHz | 0x0FBF | 4 MHz INTOSC Speed. |
| IOSCFS = 8MHz | 0x0FFF | 8 MHz INTOSC Speed. |
CPSW -- Code Protection bit - Flash Data Memory
| CPSW = ON | 0x0F7F | Code protection on. |
| CPSW = OFF | 0x0FFF | Code protection off. |
BOREN
| BOREN = OFF | 0x0EFF | BOR Disabled. |
| BOREN = ON | 0x0FFF | BOR Enabled. |
DRTEN
| DRTEN = OFF | 0x0DFF | DRT Disabled. |
| DRTEN = ON | 0x0FFF | DRT Enabled. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.