- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16LF1847
| Coff ID of device | 0xA847 |
| Number of ROM/FLASH pages | 4 (2048 words/pages)
| Last address of ROM/FLASH | 0x1FFF (8192 words)
| Address space of User ID | 0x8000 - 0x8003 (4 bytes)
| Address of Device ID | 0x8006 (1 byte)
| Address space of Configuration Words | 0x8007 - 0x8008 (2 words)
| Address space of EEPROM | 0xF000 - 0xF0FF (256 bytes)
| Number of RAM Banks | 32 (128 bytes/banks)
| Number of SFRs | 134
| Size of GPRs | 1892 bytes
| Joint size of SFRs + GPRs | 2026 bytes
| Start address of Linear RAM | 0x2000
| Size of Linear RAM | 1008 bytes
| Number of Linear RAM sections | 13

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.