- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16C554
CONFIG (address:0x2007, mask:0xFFFF)
FOSC -- Oscillator selection bits
| FOSC = LP | 0x3FFC | LP oscillator. |
| FOSC = XT | 0x3FFD | XT oscillator. |
| FOSC = HS | 0x3FFE | HS oscillator. |
| FOSC = RC | 0x3FFF | RC oscillator. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x3FFB | WDT disabled. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FF7 | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
CP -- Code protection bits
| CP = ON | 0x00CF | 0000h:01FFh code protected. |
| CP = OFF | 0x3FFF | Program Memory code protection off. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.