- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC16F720
CONFIG1 (address:0x2007, mask:0xFFFF)
FOSC -- Oscillator Selection bits
| FOSC = INTOSCIO | 0x3FFC | INTOSCIO oscillator: I/O function on RA4/CLKO pin, I/O function on RA5/CLKI. |
| FOSC = INTOSCCLK | 0x3FFD | INTOSC oscillator: CLKO function on RA4/CLKO pin, I/O function on RA5/CLKI. |
| FOSC = ECIO | 0x3FFE | EC oscillator: I/O function on RA4/CLKO pin, CLKI on RA5/CLKI. |
| FOSC = ECCLK | 0x3FFF | EC oscillator: CLKO function on RA4/CLKO pin, CLKI on RA5/CLKI. |
WDTE -- Watchdog Timer Enable bit
| WDTE = OFF | 0x3FF7 | WDT disabled. |
| WDTE = ON | 0x3FFF | WDT enabled. |
PWRTE -- Power-up Timer Enable bit
| PWRTE = ON | 0x3FEF | PWRT enabled. |
| PWRTE = OFF | 0x3FFF | PWRT disabled. |
MCLRE -- RA3/MCLR/VPP Pin Function Select bit
| MCLRE = OFF | 0x3FDF | RA3/MCLR/VPP pin function is digital input; MCLR internally disabled; Weak pull-up disabled. |
| MCLRE = ON | 0x3FFF | RA3/MCLR/VPP pin function is MCLR; Weak pull-up enabled. |
CP -- Flash Program Memory Code Protection bit
| CP = ON | 0x3FBF | 0000h to 07FFh code protection on. |
| CP = OFF | 0x3FFF | Code protection off. |
BOREN -- Brown-out Reset Enable bits
| BOREN = OFF | 0x3CFF | Brown-out Reset disabled (Preconditioned State). |
| BOREN = NSLEEP | 0x3EFF | Brown-out Reset enabled during operation and disabled in Sleep. |
| BOREN = ON | 0x3FFF | Brown-out Reset enabled. |
PLLEN -- INTOSC PLLEN Enable Bit
| PLLEN = OFF | 0x2FFF | INTOSC Frequency is 500 kHz. |
| PLLEN = ON | 0x3FFF | INTOSC Frequency is 16 MHz (32x). |
CONFIG2 (address:0x2008, mask:0xFFFF)
WRTEN -- Flash memory self-write protection bits
| WRTEN = FULL | 0x3FFC | 0h to FFFh of flash memory write protected, no address may be modified. |
| WRTEN = HALF | 0x3FFD | 0h to 7FFh of flash memory write protected, 800h to FFFh may be modified. |
| WRTEN = BOOT | 0x3FFE | 0h to 1FFh of flash memory write protected, 200h to FFFh may be modified. |
| WRTEN = OFF | 0x3FFF | Write protection off. |

This page generated automatically by the device-help.pl program (2013-08-01 15:50:27 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.