- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC18F2525
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |  | Bank 8 |  | Bank 9 |  | Bank 10 |  | Bank 11 |  | Bank 12 |  | Bank 13 |  | Bank 14 |  | Bank 15 |
| GPR 0x000 - 0x0FF 256 bytes |  | GPR 0x100 - 0x1FF 256 bytes |  | GPR 0x200 - 0x2FF 256 bytes |  | GPR 0x300 - 0x3FF 256 bytes |  | GPR 0x400 - 0x4FF 256 bytes |  | GPR 0x500 - 0x5FF 256 bytes |  | GPR 0x600 - 0x6FF 256 bytes |  | GPR 0x700 - 0x7FF 256 bytes |  | GPR 0x800 - 0x8FF 256 bytes |  | GPR 0x900 - 0x9FF 256 bytes |  | GPR 0xA00 - 0xAFF 256 bytes |  | GPR 0xB00 - 0xBFF 256 bytes |  | GPR 0xC00 - 0xCFF 256 bytes |  | GPR 0xD00 - 0xDFF 256 bytes |  | GPR 0xE00 - 0xEFF 256 bytes |  | GPR 0xF00 - 0xF7F 128 bytes SFR 0xF80 - 0xF82 3 bytes Unimplemented 0xF83 SFR 0xF84 Unimplemented 0xF85 - 0xF88 4 bytes SFR 0xF89 - 0xF8B 3 bytes Unimplemented 0xF8C - 0xF91 6 bytes SFR 0xF92 - 0xF94 3 bytes Unimplemented 0xF95 - 0xF9A 6 bytes SFR 0xF9B Unimplemented 0xF9C SFR 0xF9D - 0xFA2 6 bytes Unimplemented 0xFA3 - 0xFA5 3 bytes SFR 0xFA6 - 0xFB8 19 bytes Unimplemented 0xFB9 SFR 0xFBA - 0xFD3 26 bytes Unimplemented 0xFD4 SFR 0xFD5 - 0xFFF 43 bytes |

| SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 0 bytes GPR 256 bytes Unimplemented 0 bytes |  | SFR 105 bytes GPR 128 bytes Unimplemented 23 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

Special Function Register on Access Area.

General-purpose RAM on Access Area.

In this place no RAM on Access Area.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:29 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.