- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12F508
| Bank 0 |
| SFR 0x000 - 0x006 7 bytes GPR 0x007 - 0x01F 25 bytes |

| SFR 7 bytes GPR 25 bytes Unimplemented 0 bytes |

Special Function Register.

General-purpose RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2013-08-01 15:50:26 UTC) from the 8bit_device.info file (rev: 1.14) of mpasmx and from the gputils source package (rev: svn 983:985). The mpasmx is included in the MPLAB X.