# @...SAY

Displays data to specified coordinates of the current device.

Syntax

  @ <nRow>,<nCol> SAY <xValue> [ PICTURE <cPict> ] [COLOR <cColor>]

Arguments

  <nRow> Row coordinate
  <nCol> Column coordinate
  <xValue> Value to display
  <cPict> PICTURE format
  <cColor> Color string

Returns

  None

Description

  This command displays the contents of <xValue> at row column coordinates <nRow>, <nCol>. A PICTURE clause may be speclfied in <cPict>. If the current device is set to the printer, the output will go to the printer; the default is for all output to go to the screen.
  For a complete list of PICTURES templates and functions, see the @...GET command.

Examples

          Function Main
          Cls
          @ 2,1 SAY "Harbour"
          @ 3,1 SAY "is" COLOR "b/r+"
          @ 4,1 SAY "Power" PICTURE "@!"
          Return NIL
    Tests
          See Examples

Status

  Ready

Compliance

  This command is Ca-Clipper compliant

Platforms

  All

Files

See Also

- @...GET
- SET DEVICE
- TRANSFORM()