            segment .bss
    set     resq    10
            segment .text
            global  main
    main:
            push    rbp
            mov     rbp, rsp
            sub     rsp, 32            ; shadow registers
            bts     qword [set], 4     ; set bit 4 of set
            bts     qword [set], 7     ; set bit 7 of set
            bts     qword [set], 8     ; set bit 8 of set
            bts     qword [set+8], 12  ; set bit 76 of set
            mov     rax, 76            ; test bits 4, 76, 77
            mov     rbx, rax           ; copy bit number to rbx
            shr     rbx, 6             ; qword number of set to test
            mov     rcx, rax           ; copy bit number to rcx
            and     rcx, 0x3f          ; extract rightmost 6 bits
            xor     edx, edx           ; set rdx to 0
            bt      [set+8*rbx], rcx   ; test bit
            setc    dl                 ; edx equals the tested bit
            bts     [set+8*rbx], rcx   ; set the bit, insert into set
            btr     [set+8*rbx], rcx   ; clear the bit, remove
            xor     rax, rax
            leave
            ret