## orps - or packed singles

    dest[0] = dest[0] | source[0]
    dest[1] = dest[1] | source[1]
    dest[2] = dest[2] | source[2]
    dest[3] = dest[3] | source[3]

The orps instruction ors the 4 source values (second operand) to the 4 values of the destination (an XMM register). The source can be an XMM register or a 32 bit memory location. There is also vorps on CPUs with AVX instructions which allows using 3 XMM registers or 2 XMM registers and a memory location which can simplify coding and which ors 8 pairs of values if you use YMM registers.

There is also orpd which ors packed doubles. The result is the same so pick your favorite.

            orps   xmm0, xmm1          ; or 4 pairs of values from xmm0 & xmm1
                                       ; leave the rest of ymm0 as is
            orps   xmm0, [x]           ; or 4 pairs of values from xmm0 & x
                                       ; x is an array of floats
                                       ; leave the rest of ymm0 as is
            vorps  xmm3, xmm0, xmm15   ; or 4 pairs of values from xmm0 & xmm15
                                       ; store results in xmm3
            vorps  ymm3, ymm0, [x]     ; or 8 pairs of values from ymm0 & x
                                       ; store results in ymm3
            vorps  ymm3, ymm0, [rsi]   ; or 8 pairs of values from ymm0 & [rsi]
                                       ; rsi contains the address of an array
                                       ; store results in ymm3

### flags: none