TV Diagnostic for Hauppauge Celebrity Video Capture Hardware
Version 1.3 Copyright (c) Abbotsbury Software Ltd. UK 1995
OS/2 Version 2.30
VGA Adapter : VGA Adapter Indeterminate chip type 4139
VGA RAM size : 0x100000
Date 20/6/1997
VCAI DLL version = 3.8
Product Name   =  WinCast Video Capture Driver  
Manufacturer   =  Abbotsbury Software Ltd.      
Version Number =  1.016E.á  
Tuner Type = 255, with Unknown Clock, running at Unknown MHz, 2a8e5f
IO address set to 0x500
Board memory address set to 0x000000
Colours = 65536
Resolution = 1024 by 768 Pixels
Image Format = 32323459
BitsPerPel = 16
Overlay support = 1
Video Brightness 50, Hue 50, Saturation 50, Contrast 50
Colour Key currently set to 13
Video Input source Ext Composite 2
Sound On, Volume 50/50, Bass 50/50, Treble 50/50
Tuner Region 0, Channel 0 Frequency 325451776, FineTune 0
