

This READ.ME contains supplements to the "WaveRunner Digital Modem

Installation and Testing Instructions".  Additional information and

software updates may be obtained from the IBM Personal Computer Company

Bulletin Board System via a modem by calling 1-919-517-0001.

Information may also be obtained over the INTERNET by anonymous FTP to

www.raleigh.ibm.com and accessing subdirectory pub/standards/waverun.







Installation Prerequisite

===================================



     If you are installing THE ISDN Digital Modem in a PS/2 Model P70,

     the Reference Diskette must be Version 1.04 or higher to successfully

     update from the Startup Option Diskette.  If you have an earlier

     version of this Reference Diskette, contact an IBM Authorized Service

     Representative to obtain a new one.



Testing the WaveRunner Adapter

======================



     Diagnostic Test

     ------------------

     The NT1 Loopback test requires an NT1 that supports the S&Q maintenance

     channel.  Support of the S&Q maintenance channel is an option provided

     by some NT1 manufacturers.  Check the documentation supplied with your

     NT1 to determine if the S&Q maintenance channel is supported.  If not,

     then bypass this test.



     DMA Channel Switch Setting for ISA machines

     --------------------------------------------

     If the DMA Channel Switch Settings on the Adapter (Switch Block S2)

     do not match the DMA Channel that the Diagnostics program is

     testing, the diagnostics may not be able to complete the ISDN Hardware

     Tests.  When running Diagnostics, if the screen will not advance past

     "Testing ISDN Hardware... ", check that the DMA channel that you specified

     in Diagnostics is the same one that is selected on the adapter (Switch

     Block S2).



Configuring your Communications Application

===============================================



     Configure your communications application for a Hayes compatible

     modem or Mwave compatible.

     Also, configure the application to use the same Com Port that adapter

     is configured for.





LAN Distance

============





    Installation

    ------------



    Installation for use with IBM LAN Distance is easier if the LAN

    Distance product is installed first.  This allows the installation

    program to make required modifications to LAN Distance

    configuration files.  Refer to online help for more information on

    configuring LAN Distance for use with ISDN Digital Modem.





    LAN Distance Compatability

    --------------------------



    The version of the WaveRunner GCCI/ANDIS interface is compatible

    with LAN Distance.  To use this code with LAN Distance do

    the following:



       This code requires your LAN Distance installation to be running

       at CSD level LD08175 or later.  Earlier versions of LAN

       Distance will not work properly.  To get CSD 8175, FTP to:



       service.boulder.ibm.com/ps/products/landist/fixes/v1.1/



       From there, follow the directories for your specific country.







IBM Communications Manager/2 (CM/2) Configuration Instructions

==============================================================



    This is not intended to be an exhaustive configuration guide for

    CM/2.  It is intended to explain only the ISDN specific

    configuration options.  The specific protocol and application you

    intend to use must be configured in addition to the items

    mentioned below.



    1. Shut down CM/2 if it is started.



    2. Double click on the Communications Manager Setup icon to start

       the CM/2 configuration utility.



    3. Click on 'Setup'.  Verify that you are modifying the correct

       configuration and click on 'OK'.  You may be asked if the

       configuration you specified is to be used on the current

       workstation.  Answer appropriately.



    4. The PCM is configured through the SNA Phone Connect (SPC)

       options.  These are configured as follows:



       SPC - Connection Manager:  This is where incoming and outgoing

       phonebook entries are defined.  For outgoing calls, the bearer

       capability and called party number subfields are required.  For

       incoming calls, defining no subfields will indicate that all

       incoming calls are to be answered.



       SPC - Port Connection Manager:  From the Modem Connection

       pulldown, select ISDN.  'IBM Mwave WaveRunner' should appear in

       the PCM window.  Select this line and click on 'Configure'.  On

       the panel that appears, you should enter the local ISDN

       telephone number for your WaveRunner adapter.  Do not include

       non-numeric characters such as dashes or parentheses.



       SPC - Protocol Driver:  Select and configure the protocol

       driver desired.



    5. The ISDN specific portions of the protocol definitions are

       simply a matter of specifying the desired phonebook entries

       that were created under SNA Phone Connect - Connection Manager.

       How this is done will depend on which protocol is to be used.



       SDLC/IDLC:  Use the SNA Phone Connect version of these protocol

       definitions.  Specify the desired phonebook entries on the

       configuration panel.



       X.25:  The phonebook entries are under the X.25 Links panel.

       On this panel, choose ISDN as the adapter type.  Under

       'Additional parameters', select ISDN and configure the desired

       phonebook entries.



    6. Other configuration parameters should not be ISDN-specific.



