This READ.ME contains important supplements to your "WaveRunner PCMCIA
Digital Modem Installation and Testing Instructions."  Additional
information and software updates may be obtained from the IBM Personal
Computer Company Bulletin Board System via a modem by calling
1-919-517-0001.  Information may also be obtained over the INTERNET by
anonymous FTP to www.raleigh.ibm.com and accessing subdirectory
pub/standards/waverun.



Restrictions
============

The WaveRunner PCMCIA cannot be installed in IBM ThinkPads that have an
IBM Mwave Digital Signal Processor (DPS) integrated on the system board.
WaveRunner PCMCIA also uses the Mwave DSP and both DSPs cannot operate at
the same time.


Configuring your Communications Application
===============================================

     Configure your communications application for a Hayes compatible
     modem or Mwave compatible.
     Also, configure the application to use the same Com Port that adapter
     is configured for.


LAN Distance
============


    Installation
    ------------

    Installation for use with IBM LAN Distance is easier if the LAN
    Distance product is installed first.  This allows the installation
    program to make required modifications to LAN Distance
    configuration files.  Refer to online help for more information on
    configuring LAN Distance for use with ISDN Digital Modem.


    LAN Distance Compatability
    --------------------------

    The version of the WaveRunner GCCI/ANDIS interface is compatible
    with LAN Distance.  To use this code with LAN Distance do
    the following:

       This code requires your LAN Distance installation to be running
       at CSD level LD08175 or later.  Earlier versions of LAN
       Distance will not work properly.  To get CSD 8175, FTP to:

       service.boulder.ibm.com/ps/products/landist/fixes/v1.1/

       From there, follow the directories for your specific country.



IBM Communications Manager/2 (CM/2) Configuration Instructions
==============================================================

    This is not intended to be an exhaustive configuration guide for
    CM/2.  It is intended to explain only the ISDN specific
    configuration options.  The specific protocol and application you
    intend to use must be configured in addition to the items
    mentioned below.

    1. Shut down CM/2 if it is started.

    2. Double click on the Communications Manager Setup icon to start
       the CM/2 configuration utility.

    3. Click on 'Setup'.  Verify that you are modifying the correct
       configuration and click on 'OK'.  You may be asked if the
       configuration you specified is to be used on the current
       workstation.  Answer appropriately.

    4. The PCM is configured through the SNA Phone Connect (SPC)
       options.  These are configured as follows:

       SPC - Connection Manager:  This is where incoming and outgoing
       phonebook entries are defined.  For outgoing calls, the bearer
       capability and called party number subfields are required.  For
       incoming calls, defining no subfields will indicate that all
       incoming calls are to be answered.

       SPC - Port Connection Manager:  From the Modem Connection
       pulldown, select ISDN.  'IBM Mwave WaveRunner' should appear in
       the PCM window.  Select this line and click on 'Configure'.  On
       the panel that appears, you should enter the local ISDN
       telephone number for your WaveRunner adapter.  Do not include
       non-numeric characters such as dashes or parentheses.

       SPC - Protocol Driver:  Select and configure the protocol
       driver desired.

    5. The ISDN specific portions of the protocol definitions are
       simply a matter of specifying the desired phonebook entries
       that were created under SNA Phone Connect - Connection Manager.
       How this is done will depend on which protocol is to be used.

       SDLC/IDLC:  Use the SNA Phone Connect version of these protocol
       definitions.  Specify the desired phonebook entries on the
       configuration panel.

       X.25:  The phonebook entries are under the X.25 Links panel.
       On this panel, choose ISDN as the adapter type.  Under
       'Additional parameters', select ISDN and configure the desired
       phonebook entries.

    6. Other configuration parameters should not be ISDN-specific.

