 Switch settings for ISA Xem (PC/Xem) DigiBoard 

 DS1 switch sets I/O port address - Memory & IRQ are done with software. 
 Make sure you have latest driver to use these boards. Old drivers will
 not have support for these new boards.

 DS1 - Switches 1-4 on 4 position dipswitch 
 OFF: Switch flipped away from board  ON: Switch flipped toward board

 DS1    Switch: 1 2 3 4   DS1   Switch: 1 2 3 4   DS1   Switch: 1 2 3 4 
 I/O Port  off: - - - -   I/O Port off: - - x -   I/O Port off: - x - -
 324h       on: x x x x   304h      on: x x - x   224h      on: x - x x

 DS1    Switch: 1 2 3 4   Pick non-conflicting I/O port address, best choices 
 I/O Port  off: - x x -   are 324h or 304h. Use 104h as last choice this is
 204h       on: x - - x   reserved or used by a number of devices. 

 DS1    Switch: 1 2 3 4   DS1   Switch: 1 2 3 4   DS1   Switch: 1 2 3 4 
 I/O Port  off: x x - -   I/O Port off: x - x -   I/O Port off: x - - -
 104h       on: - - x x   114h      on: - x - x   124h      on: - x x x

 Jumper Settings for ISA Xem (PC/Xem) DigiBoard

 There are two jumpers on the PC/Xem host adapter. These jumpers should be
 left in the factory default position, between pins 1 and 2 (top 2 pins).
 ----------------------------------------------------------------------------
 System configuration for EISA Xem DigiBoard 

 1. Boot your EISA system with the EISA configuration diskette. These 
    steps only need to be done for EISA boards, ISA boards in an EISA
    system are configured as if it were a ISA system. There are no EISA
    .cfg files for any DigiBoard ISA board.

 2. Copy the file !DBI0201.cfg from the DigiBoard EISA .cfg file diskette. 
    This should have come with your board. If not, download from DigiBoard's
    BBS 612-943-0812, or call Customer Service to have it mailed to you
    612-943-0577.

 3. Run configuration program and addd the board.
    
    Pick non-conflicting memory address from menu.
    Leave Dual-Port Mem Enbl/Dsbl at Disabled.
    Leave Interrupt Configuration at Disabled.

    Exit and Save new configuration.


 Jumper Settings for EISA Xem DigiBoard

 There is only one jumper on the EISA/Xem host adapter. This must be left
 in the factory set position, between pins 1 and 2 (left & middle pins).
 ----------------------------------------------------------------------------
 System configuration for MC Xem DigiBoard 

 1. Boot system from your copy of your IBM Reference Diskette.

 2. Select from menu "Copy an Option Diskette". Follow instruction to add
    DigiBoard ADF file to Reference Diskette.
 
 3. Select Set Configuration, Run Automatic Configuration. Save and reboot.


 Jumper Settings for MC Xem DigiBoard

 There is one jumper on the MC/Xem host adapter. This must be left in the
 factory set position, between pins 2 and 3 (right & middle pins).
