Iomega OS/2 OAD (Open Architecture Drivers) Driver V2.33 (OS/2 2.0+)
Iomega OAD Driver for OS/2 2.33
Iomega Zip Drive SCSI/Parallel driver for OS/2.
1995/03/27

It hase the following folders:
- Images: Contains the floppy images as it was distribuited
- Files: Contains the files without being compressed into a diskette images. 

Includes support for:
- Iomega PC1600*, PC800, PC2, PC4 and PPA-I adapters
- Bernoulli 230MB, 150 Multidisk, 90MB, 44MB, 20MB and 10MB drives.
- Iomega LaserSafe, LaserSage Pro and LaserSage Plus drives.
- Iomega Floptical drives.


Made by Iomega Coporation on 1995.