MAKE720.BAT or MAKE144.BAT are used to create a Device Support Diskette
containing the Iomega OS/2 OAD Drivers version 2.33. 

To create a 720K diskette:
(To create a 1.44MB diskette see below)

        1. Place a FORMATTED 720k floppy diskette into drive A: or B:.
        
        2. From a DOS window or DOS full screen session type the
           following command:

                MAKE720 a:
                   or
                MAKE720 b:
                 
           depending on the drive containing the formatted floppy. 

        3. After confirming that a formatted floppy is contained in the
           desired drive, press any key to continue.

        4. The diskette can now be used by the OS/2 DDINSTL.EXE utility
           to install the Iomega OS/2 OAD Drivers. Refer to the README
           file on the diskette for more information.

To create a 1.44MB diskette:

        1. Place a FORMATTED 1.44MB floppy diskette into drive A: or B:.
        
        2. From a DOS window or DOS full screen session type the
           following command:

                MAKE144 a:
                   or
                MAKE144 b:
                 
           depending on the drive containing the formatted floppy. 

        3. After confirming that a formatted floppy is contained in the
           desired drive, press any key to continue.

        4. The diskette can now be used by the OS/2 DDINSTL.EXE utility
           to install the Iomega OS/2 OAD Drivers. Refer to the README
           file on the diskette for more information.
