IBM released a critial update for users of their ServeRAID 4 series
controllers, and released it to their web site.  Unfortunately, the images
placed in the OS/2 support area are useable only in Win9x or NT.

Fortunately, I have a Win98 laptop, so I was able to recreate the necessary
floppy disks.  Not every OS/2 user will be so fortunate.

So, I went to HOBBES and downloaded the LOAD/SAVE DSK utilities from IBM.
I then used SAVEDSKF to copy the disk data to an image file.

These two files are images for use with IBM's LOADDSKF utility to recreate
the target disk images.

Create the disk images, then place DISK 1 (image SV610701) in your drive A:
floppy disk drive, shutdown and reboot to install the update.  This will
update the Controller BIOS to 6.10.70.

Robert Gammon
Houston, TX
