*----------------------------------------------------------------------------
* Response File for installation of Cirrus Video Card drivers.
*
* Only two lines are required in order to automate installation. 
*
* The first is the write mode.  The two choices are:
*    REFRESH   = Will not overwrite a file a newer date than the source file.
*    OVERWRITE = Will overwrite all files regardless of the date.
*
* Examples are:
*    write_mode = REFRESH
*    write_mode = OVERWRITE
*----------------------------------------------------------------------------

write_mode = OVERWRITE

*----------------------------------------------------------------------------
* The second is the selection of the initial resolution.
*
* Initial Resolution is specified as follows
*
* initial_resolution = (
*                         x   = 640
*                         y   = 480
*                         bpp = 8
*                         refreshrate = 60;
*                      )
*
* Please be aware when selection these modes that there are no guarentees
* that the mode selected will work on every video card/monitor combination
* so choosing a lower resolution / refreshrate / bits per pixel might be
* a good thing to do during automated installation.
*
* Choices for these should be valid, so please consult your manual and choose
* a valid x, y, bpp, and refreshrate value for your configuration.
*----------------------------------------------------------------------------

initial_resolution = ( x = 800
                       y = 600
                       bpp = 8
                       refreshrate = 70 )
