COPYRIGHT INTELLIGRAPHICS, INC. 1998

This is release R4.24.94 of the NeoMagic 22xx/23xx OS/2 3.x/4.x SBCS driver,
released on 11/25/98.

For installation instructions please see INSTALL.TXT, which is on the
installation diskette.

To create the installation diskette, unzip INSTALL.ZIP to a formatted,
blank diskette.  The command is:

  pkunzip -do install.zip a:


New features/functionality:
Build 94:
	Fix Warp3 installation problem.
	Support for NMG6 plus boards which have 0x16 as the chip id and 6mb of memory.
        Fixed Warp 3.0 - AVI playback and focus change gives system error message
			Fix is also in tmpput.c.  Both NMG4 and main branch needed the fix.


Build 90:
Fixed 1. Re-pack the latest WindowFS/Seamless dirver for both NMG4 and NMG5. 
Fixed 2. Use the Japanese version of VCFGMRI.DLL for DBCS installs.


Build 88:
Fixed - 
	NMG5-OS2-036, Added NMG6 support

Build 86:
Fixed -
	NMG5-OS2-018, NMG5-OS2-022, NMG5-OS2-040


Build 84:
Fixed - 
        Update svgadata.pmi files in NMG5 install.
        Update setup.cmd in NMG5 install. (for both DBCS and SBCS)
        Put in a new set of source code for VSVGA.SYS.
	        The source directory is vdev_jp which replaces vdev_n2f.
        Take out the fixes for NMG5 Shakey Cursor.
        	(eddmcurs.c eddcursr.asm)



Build 82:
Fixed NMG5-OS2-039 DBCS char on top left corner of the window is corrupted. (eddfsubr.asm)


Build 80:
Fixed # NMG5-OS2-038 : The problem is in DBCS AVIO, font selection are sometimes wrong.
	The files modified are: eddvbur.c and softavio.asm.


Build 78:

Fixed -
	NMG5 d24051 Dotted outline on right click not cleared.
	    (eddlpoly.c)

	NMG5 OS2-018 Overlay garbage when playback with Digital Video
	    (cacheman.h cacheman.inc cacheman.c tmpput.c)


	OS2-021 Green noise when playback MS Video-1 64K with MediaPlayer
	    (eddbgetp.c eddcsubr.c eddefpdb.c modeinfo.c)


	OS2-008 Incorrect display when open System in System Setup folder
	    (Re-pack magic.pak and magic_db.pak for video.cfg update setup.cmd for all NMG4/NMG5 dbcs and sbcs.)


	"OS/2 lockup" failing after ped lock start moving.
	    (pointer2.asm)


11/25/98
Dave Mitchell

