Installation Instructions
S3 OS/2 Driver (For OS/2 2.11, 2.1, 2.1 for Windows, and Warp)

Date:      03/20/95

INSTALLATION CONSIDERATIONS:

1.  It is assumed that the user knows the maximum vertical refresh rate 
as well as the maximum resolution of the monitor.

2.  The standard IBM VGA driver must be installed first unless there is 
an S3 driver is already installed.

3.  The volum name for the first driver diskette must be labeled as "S3 DRV1"
and the second as "S3 DRV2". If they are not correctly labeled, the
installation will fail.

4.  An S3 chip-based card need be installed in the machine at the time of 
the driver installation. 

5.  Save all data files and closed Win-OS/2 session and all Seamless Windows 
applications (Seamless applications are windows applications that run on top 
ofthe PM Desktop.)


INSTALLATION STEPS:

1.  Open an OS/2 command prompt (windowed or full screen).

2.  Insert the driver diskette 1 (S3 DRV1) into a floppy drive. 

3.  Change to the floppy drive (A: or B:) into which you have inserted 
driver diskette 1.  Verify that the diskette is labeled "S3 DRV1" (do the 
same for disk #2).  If it is not labeled then enter "label S3 DRV1" or 
"label S3 DRV2".

4.  Type S3INST A: C: and press "Enter" key.  ("A" is the source floppy 
drive; "C" is the drive where OS/2 is installed.  If OS/2 is installed on 
a different drive, then use that letter instead).

Note: You may see an error message stating could not locate files. Please 
ignore this message.

5.  When prompted, insert Disk 2.  It must be labeled "S3 DRV2".

6.  When prompted, exit the OS/2 command prompt, remove the driver diskette 
from the floppy drive, shutdown and reboot the system.

7.  After bootup, open an OS/2 command prompt (windowed or full screen).  
Insert Disk 1 (S3 DRV1) into the floppy drive which contains the updated 
SVGA.EXE.  Copy this file into the \OS2 subdirectory of your OS2 drive.

8.  Exit OS/2 command prompt.

9.  Double click on the the "OS/2 System" icon.

10. Double click on the "System Setup" icon.

11. Click on the "Display Driver Install" (not the Device Driver Install.) 

12. When prompted by the Display Driver Install dialog, select Primary 
Display and then click the OK button.

13. Select the "32 Bit S3 Display Drivers" option from the Primary Display 
Adapter Type dialog and click the OK button.

14. Select the appropriate option from the Monitor Configuration/Selection 
Utility dialog, and click the OK button.  Select "Default" for the prompt.

15. The Source Directory dialog will be displayed.  Set the source directory 
to the location of disk 1 (S3 DRV1).  Double click on the "Install" button.

16. Insert disk 2 (S3 DRV2) into the floppy drive when prompted.

17. The Installation Program may pause and display prompts to overwrite 
certain files.  Please answer YES for each file.

18. You will be given a message stating that you "Must Shutdown and Restart 

your system for the changes to take effect". Click "OK" button.

19. Remove the driver diskette from the floppy drive.  

20. Shut down and reboot system.  

Note:  You can double click the "System" Icon in the System Setup  to 
change resolution before shutting down.

After you reboot, your system will come up with your newly installed driver.


CHANGING RESOLUTIONS:

1.  Double click on the "System" icon in the System Setup Folder.

2.  Highlight the resolution and close the dialog.

3.  Shut down and reboot for the changes to take effect.

