/==============================================================================
Note 1:
   The following list provides a brief abstract of each APAR fixed
   in OS/2 Warp Device Drivers FixPaks. Every effort has been made to
   include all APARs fixed in OS/2 Warp Device Drivers in this list, how
   ever some APAR numbers could be omitted from this list but are fixed in this
   FixPak. The list of APARs below consists of all Device Drivers APARs
   fixed from Warp v3 base Fixpaks XR_W005 through XR_W040 and Warp v4 base
   FixPaks XR_M001 through XR_M010.

   If you have a concern with a particular APAR number not listed,
   please contact IBM OS/2 Support for verification.

Note 2:
   OS/2 Warp Device Drivers (DD) FixPak XR_D001 is the first DD FixPak
   produced as a seperate stand alone FixPak for OS/2 Warp products.
   This FixPak services OS/2 Warp Server, Warp Server SMP, Warp v4, WSOD Rel 1
   and WSOD Rel 2.
===============================================================================

==============================
OS/2 Warp Device Driver APARs
FixPak Name = XR_D001
==============================

=============================
Warp v3 Device Drivers APARs
=============================

APAR= JR09500
 IPSRAID WILL NOT ALLOW BOOT RECORD TO BE WRITTEN IF ADAPTER IS
 IN WRITEBACK MODE.

APAR= JR10165
 OS2SCSI COUNTS ONLY SCSI ADAPTERS IN THE SYSTEM.

APAR= JR10380
 AHA7870.ADD DRIVER (12/96 VERSION) WON'T BOOT ON AN IBM PC SERVER
 704 NON-RAID SYSTEM.

APAR= JR10392
 TRAP IN OS2DASD.DMD UNDER WARP SERVER SMP WHEN USING HPFS386.IFS
 AND DISK FAULT TOLERANCE DRIVER.

APAR= JR11867
 DOSTMRQUERYTIME RETURNS BOGUS INFO ON SMP BOXES THAT USE
 CLOCK02.SYS.

APAR= JR12449
 WHEN PUSHED SHIFT+ALT+ALT+SPACE, SHIFT WAS KEPT LOCKED.

APAR= PJ16503
 FAST TYPING IN A DOS / WIN-OS2 SESSIONS CAUSES THE KEYBOARD TO
 LOCKUP IN SESSION WHEN CAPSLOCK USED.

APAR= PJ16803
 BUSLOGIC.ADD UNLOADS UNDER WARP 3.0 WITH REV C CARD, AND
 APAR-PJ15841 DRIVER.

APAR= PJ16864
 COMPAQ LTE ELITE & AST ASCENTIA 900N PCMCIA SUPPORT NOT WORKING.
 SYS1201 DURING BOOT FOR VCOM.SYS & AUTODRV2.SYS BEEN REPORTED.

APAR= PJ17403
 USING PCMCIA MODEM CAUSES TRAP 0000, HANGS AND OTHER STRANGE
 BEHAVIOR ON TP 720.

APAR= PJ17407
 PROBLEMS ACCESSING CDROM AND/OR DRIVES ATTACHED TO A FUTURE
 DOMAIN SCSI CONTROLLER.

APAR= PJ17610
 KEYBOARD LOCKS AFTER USE OF LED KEYS, OR FAST TYPING USING
 LED KEYS MOUSE IS STILL ACTIVE AND RESPONSIVE.

APAR= PJ17767
 PCM+ (PHOENIX TECHNOLOGIES) CAUSES PCMCIA.SYS TO HANG.  THE
 APPLICATION HANGS AS A RESULT OF THIS PROBLEM.

APAR= PJ17840
 USING PCMCIA MODEM CAUSES TRAP 0000, HANGS AND OTHER STRANGE
 BEHAVIOR ON TP 720.

APAR= PJ17958
 INT 3 IN IBM1FLPY AT _SETUPDMA + 7E ( 598 : 00000CF2 WHEN ATTEMP
 TING A READ VERIFY OPERATION.

APAR= PJ18135
 ERROR "CD-ROM CAN NOT BE FOUND" DISPLAYED WHEN IDE CDROM
 CONNECTED TO SECONDARY IDE PORT.

APAR= PJ18249
 TRAP000D IN OS2DASD.DMD ON SYSTEM WITH HPFS386, LANSTREAMER AND
 USING FAULT TOLERANCE ON LS SERVER.

APAR= PJ18302
 WARP TRAPS IN KBD  AT EIP = 000000E2 WHEN STARTING OSI3270.
 OSI3270 IS A 3270 EMULATOR.

APAR= PJ18314
 PCMCIA MODEM DOES NOT GENERATE SOUNDS WHEN DIALING. PROBLEM ONLY
 ON CIRRUS LOGIC SOCKET CONTROLLER.

APAR= PJ18348
 WHEN IN SPANISH KEYBOARD LAYOUT AND IN A DOS WINDOW THE ACCENTED
 KEYS ARE DISPLAYED CORRECTLY, BUT SYSTEM BEEPS DUE TO CAPSLOCK.

APAR= PJ18349
 WHEN IN SPANISH KEYBOARD LAYOUT AND IN A DOS WINDOW THE ACCENTED
 KEYS ARE DISPLAYED CORRECTLY, BUT SYSTEM BEEPS DUE TO CAPSLOCK.

APAR= PJ18400
 SYS1201 COM.SYS NOT LOADED DURING BOOT AND NO MOUSE SUPPORT ON
 THE DESKTOP. DESKTOP FUNCTIONS CORRECTLY WITH KEYBOARD.

APAR= PJ18470
 PCMCIA FLASH / SRAM CARDS WHICH DO NOT CARRY THE IBM LOGO WILL
 NOT WORK UNDER OS/2 WARP.

APAR= PJ18472
 PCMCIA MODEMS ASSIGNED COM PORT NOT ASSOCIATED WITH USUAL
 I/O ADDRESS.  TP 755CD OR NOTEBOOKS WITH SERIAL TRACKBALL MSE

APAR= PJ18506
 FULLPACK TRAP D  IN KBD$  AT EIP = 000000E2  CSLIM=2F6A.
 STARTING OSI3270 IS A 3270 EMULATOR.

APAR= PJ18617
 SERIAL PORT OPENED MULTIPLE TIMES WHILE ANOTHER APPLICATION HAS
 PORT IN USE CAUSES COM.SYS TO KEEP PORT UNAVAILABLE.

APAR= PJ18718
 SYS1201 VMOUSE.SYS : IBM PC 330 466/DX2 WILL NOT BOOT OS/2 IN
 UNATTENDED START MODE USING POWER ON PASSWORD FEATURE.

APAR= PJ18913
 BTC CD ROM NOT FUNCTIONING.

APAR= PJ19070
 CAN'T INSTALL SONY CDU 55E CD ROM TO MCA IBM 750 SYSTEM
 BY USING SELECTIVE INSTALL

APAR= PJ19190
 BUSLOGIC PCI  SCSI HANGS SYSTEM WHEN A CDROM RESET IS DONE ON
 CERTAIN SYSTEMS.

APAR= PJ19224
 CUSTOMER CANNOT LOAD SOCKET SERVICES ON A MIDWESTMICRO LAPTOP
 WITH MODEL TS38S & FCCID IIRTE38S.

APAR= PJ19305
 INCORRECT INFORMATION RETURNED FROM READ PARMS, 0X43, WHEN TWO
 SCSI ADAPTERS OF SAME MODEL ARE USED CONNECT TO SAME TYPE DEVICE.

APAR= PJ19356
 INCORRECT INFO RETURNED FROM OS2SCSI.DMD READ PARMS, 0X43, WHEN
 TWO DIFFERENT SCSI ADAPTERS IN SYSTEM HAVE SAME TYPES OF DEVICES.

APAR= PJ19409
 DATA CORRUPTION DURING I/O ON HARD DRIVE CONNECTED TO PCI IDE
 PORT.

APAR= PJ19520
 TRAP0008 WITH STACK = E8:00000000 ON PS/2 9557-OBA. SERIAL MOUSE
 & SDLC ADAPTER PRESENT.

APAR= PJ19545
 TRAP000D IN OS2DASD.DMD ON SYSTEM WITH HPFS386, LANSTREAMER AND
 USING FAULT TOLERANCE ON LS SERVER.

APAR= PJ19574
 TRAP000D IN OS2DASD.DMD ON SYSTEM WITH HPFS386, LANSTREAMER AND
 USING FAULT TOLERANCE ON LS SERVER.

APAR= PJ19658
 BTSEIDE.FLT CANNOT RELIABLY SUSPEND/RESUME WITH IBM1S506.ADD
 WHEN AN ATAPI CDROM IS USED WITH IBMIDECD.FLT.

APAR= PJ19669
 TRAP IN CD-ROM2$ ON THINKPAD 760.

APAR= PJ19723
 MOUSE.SYS IN WARP CONNECT BREAKS LAN SERVER UPS SERVICES.

APAR= PJ19807
 HAYES ACCURA 24 B HANGS UNDER WARP.  USING THE COM.SYS FROM
 OS/2 2.11 IT WORKS.

APAR= PJ19823
 IDE DISK CAN INCUR POSSIBLE DATA READ CONFLICTS THAT CAN CAUSE.

APAR= PJ20144
 MULTI SESSION CDS NOT PROPERLY RECOGNIZED ON PLEXTOR 4-PLEX.

APAR= PJ20250
 TRAP 000D IN DPT20XX.ADD DURING SHUTDOWN

APAR= PJ20405
 TRAP 000D IN OS2DASD.DMD IN FT_NOTIFYDONEIORB_RP DUE TO A FAILURE
 TO CHECK A RETURN.

APAR= PJ20598
 HP OMNIBOOK 5000 HANGS DURING BOOT WHILE LOADING IBM2MAT1.SYS.
 THE CIRRUS LOGIC CL-PD6729 PCI PCMCIA SOCKET CONTROLLER IS USED.

APAR= PJ20893
 FLOPPY DRIVE A: NOT RECOGNIZED UNDER WARP AFTER
 SUCCESSFUL INSTALL FROM DISKETTES IF APM AND VAPM.SYS ENABLED.

APAR= PJ20921
 RESTORE NETVIEW ALERTS ERROR LOGGING CAPABILITES FOR SCSI
 HARD DISK FAILURES.

APAR= PJ20933
 THE FLAGS3 SETTING IN THE COM.SYS DRIVER CAUSES THE RX FIFO
 TRIGGER TO SET AT THE WRONG LEVEL.

APAR= PJ21135
 PASSPORT/2 FAILS AFTER APPLYING FIXPAK 10 WITH THE MESSAGE:
 'CONNECT FAILED AFTER 1 RETRIES'.

APAR= PJ21543
 SNI NOTEBOOK GETS CRC AND SECTOR NOT FOUND ERRORS AFTER
 WRITING FILES TO IT.

APAR= PJ21774
 POP-UP KEYBOARD LOCKS UP SYSTEM ON IBM 730T WITH PEN OS/2 V1.03.

APAR= PJ21816
 IBM ENHANCED CDROMS MODELS CDRM00103 AND CDROM00203
 CAPABILITIES NOT RECOGNIZED.

APAR= PJ22084
 TRAP IN _VMFREEKSHB + 0X53 WHEN CLOSING A VDM OR IN EM86OUTBIMM.

APAR= PJ22595
 TRAP IN DPT DRIVER DPT20XX.ADD ON SHUTDOWN WITH SETBOOT /B.

APAR= PJ22789
 HANG ON SYSTEMS USING TRIBBLE CARD AND OPTICAL DRIVE.

APAR= PJ23196
 COM.SYS NOT WORKING WITH MCA MULTI-PROTOCOL ADAPTER.

APAR= PJ23270
 RANDOM TRAP 8 OCCURES AFTER INSTALLATION OF IBM1S506.ADD SHIPPED
 WITH FIXPACK 22.

APAR= PJ23304
 KBDFLUSHBUFFER(0) HANGS THE OS/2 FULL SCREEN SESSSION WITH A KEY
 BOARD MONITOR INSTALLED.

APAR= PJ23387
 IN THE BINARY MODE, SHIFT-REPORT STATE GIVES WRONG VALUE
 WHEN BOTH THE ALT KEYS ARE PRESSED DOWN.

APAR= PJ23516
 NEW MERGE OF BUSLOGIC DRIVER CODE.

APAR= PJ23608
 TRAP 0003 OS2CDROM.DMD WHEN OVERLAPPING ACCESSES OCCUR AT THE
 SAME TIME.

APAR= PJ23633
 PRESSING "WINDOWS 95" KEY IN DOS SESSION CAUSES TRAP.

APAR= PJ23652
 ON IBM THINKPAD 365E MODEL PRESSING CAPSLOCK+ANY LETTER KEY FEW
 TIMES HANGS SESSION. NO KEYBOARD RESPONSE, MOUSE WORKS.

APAR= PJ23656
 DIVE TRUNCATES ADDRESS RETURNED TO IT FROM MATROX DRIVER.

APAR= PJ23684
 NO SUPPORT FOR SECOND PCMCIA CONTROLLER WHEN NOTEBOOK PORT
 REPLICATOR IS ATTACHED.

APAR= PJ23696
 IBM2MAT.SYS CAUSES TRAP E WHEN IBM SSF PC CARD IS INSERTED ON
 COLD BOOT.

APAR= PJ23787
 RANDOM TRAP 8 OCCURES AFTER INSTALLATION OF IBM1S506.ADD SHIPPED
 WITH FIXPACK 22.

APAR= PJ24054
 PRESSING THE PRINTSCREEN AND SCROLLLOCK KEYS TOGETHER CAUSES
 THE KEYS TO CONVER TO UPPERCASE OR LOCKSUP KEYBOARD.

APAR= PJ24093
  MOUSE CURSOR NOT SHOWN IN OS/2 FULL-SCREEN SESSION USING KEDIT.

APAR= PJ24216
 REMOTE TELNET CLIENT CAN'T ENTER KEYSTROKES UNTIL THE TELNET
 SESSION IS CHOSEN FROM THE WINDOW LIST ON LOCAL HOST.

APAR= PJ24241
 ASPI API "SCAN" DOES NOT WORK FINE IN WIN-OS2.

APAR= PJ24484
 INTEGER DIVIDE BY 0 AT INIT TIME IN ICMEMMTD (TRAP)
 INIT_CMD +F1  DIV BX.

APAR= PJ24485
  OS2SCSI COUNTS ONLY SCSI ADAPTERS IN THE SYSTEM.

APAR= PJ24611
  IBM2SCSI.ADD DOES NOT CONSIDER CONDITION MET A SUCCESS
 AND EVOKES RETRY LOGIC 5 TIMES BEFORE PASSING IT ON.

APAR= PJ24776
 IPE LINE 926 FILE 4019 PGALLOC.C.

APAR= PJ24931
 TRAP IS OCCURRING USEING SHIFT LEFT BRACKET UNDER US SYSTEM
 USEING SPANISH CODEPAGE.

APAR= PJ24937
 SOME CASES OF IPE LINE 970 FILE 4059 VMLOCK.C IN ALLSTRICT
 DEBUG KERNEL.

APAR= PJ24986
 RTS/CTS NOT PROPERLY WORKING ON SOME INTERNAL MODEMS.

APAR= PJ25016
 TRAP 00D IN IPSRAID DRIVER WHILE RUNNING WITH FIXPAK XR_W031.

APAR= PJ25031
 HARD DRIVE LIGHT DOES NOT LIGHT AFTER INSTALLATION OF FIXPAK 30.

APAR= PJ25420
 MACHINE WITH 12 DRIVES FAILS TO BOOT DUE TO TRAP IN IBM1FLPY.ADD.

APAR= PJ25443
 AIC7870.ADD FAILS TO RECOGNIZE SOME ATTACHED DEVICES.

APAR= PJ25495
 DOSGETDATETIME RETURNS BAD VALUES OR EXPERIENCES SUDDEN JUMPS IN VALUES.

APAR= PJ25510
 TRAP D IN KBD$ (ACCESS VIOLATION IN ROUTINE PURGEKIB OF KBDBASE);
 LOOK FOR  EAX=0000FFEC.

APAR= PJ25555
 TRAP000D IN KBD$ IN FUNCTION PUTINKIB.

APAR= PJ25576
 JAZ DRIVE NOT USEABLE IF BOOTED WITHOUT MEDIA.

APAR= PJ25594
 HANG WHEN PRESSING CTL-ALT-DEL TO SHUTDOWN OR REBOOT THE
 SYSTEM.

APAR= PJ25725
 SYSTEM HANGS WHEN COPYING DATA TO JAZ DRIVE CONTAINING
 A DEFECTIVE CARTRIDGE.

APAR= PJ25836
 TRAP000D IN IBM1S506.ADD AT ADD_CONVRBATOCHS + 25 WHEN
 KILLING VDM THREAD STARTED BY IBM1S506 DURING BOOT.

APAR= PJ25865
 TRAP0003 ON IBM 6589 MACHINES AFTER APPLICATION OF XR_M006.

=============================
Warp v4 Device Drivers APARs
=============================

APAR= JR09305
LEXMARK PRINTERS NOT AUTOMATICALLY RECOGNIZED BY SNOOP FUNCTION.

APAR= JR09323
 CSSCSI.SYS AND FD16-700.ADD RESOURCE CONFLICT.

APAR= JR09341
 NEW MERGE OF BUSLOGIC DRIVER CODE.

APAR= JR09368
 MSCDEX FUNCTIONS DON'T RETURN CF SET.

APAR= JR09401
 3RD, AND 4TH EIDE DRIVE GEOMETRY NOT MAPPED CORRECTLY BY
 IBM1S506.ADD.

APAR= JR09431
 AIC7870.ADD SUPPORT > 1 GB DRIVES DURING PARTITION CREATION.

APAR= JR09432
 TRAP IN _VMFREEKSHB + 0X53 WHEN CLOSING A VDM OR IN EM86OUTBIMM.

APAR= JR09438
 AHA152X.ADD SUPPORT > 1GB DRIVES DURRING PARTITION CREATION.
 MERGER ADAPTEC CODE INTO MERLIN CODE.

APAR= JR09440  SER= 007
 SUSPEND NOTIFICATION NOT SENT AFTER FIRST SUSPEND ON MERLIN.

APAR= JR09501
 IPSRAID.ADD SHIPPED WITH MERLIN DOES NOT WORK.

APAR= JR09573
 TRAP AT MACRO$GETUNCFSDFROMPATH + 0X37.

APAR= JR09691
 RTS/CTS NOT PROPERLY WORKING ON SOME INTERNAL MODEMS.

APAR= JR09767
 BIDI ECP PORT DRIVER.

APAR= JR09769
 QLOGIC SNOOPER NOT DETECTING QLOGIC SCSI CARD.

APAR= JR09770
BYTE AND ECP MODES BROKEN.

APAR= JR09771
 QUERY DEVICE ID IN ECP MODE FAILS.

APAR= JR09776  SER=
 WARP V4 FAILS TO RECOGNIZE DIAMOND 8X CDROM.

APAR= JR09987
 MOUSE CURSOR NOT SHOWN IN OS/2 FULL-SCREEN SESSION USING KEDIT.

APAR= JR10034
 REMOTE TELNET CLIENT CAN'T ENTER KEYSTROKES UNTIL THE TELNET
 SESSION IS CHOSEN FROM THE WINDOW LIST ON LOCAL HOST.

APAR= JR10154
 PROBLEMS WITH VKBD.SYS IN FP1.

APAR= JR10346
 FLUSHING COM BUFFERS TAKES UP TO ONE SECOND THEREBY CAUSING LOST
 DATA.

APAR= JR10365
 TRACKPOINT 4 / SCROLLING MOUSE DOES NOT WORK
 PCCO_THINKPAD.

APAR= JR10487
 PCCO_THINKPAD WITH DVD/MPEG2 CARD INSTALLED HANGS DURING WARP V4
 INSTALLATION.

APAR= JR10605
 COM.SYS DOES NOT ALLOW FOR 16 BIT I/O ADDRESSES ON ISA SYSTEMS
 (I.E. 3220).

APAR= JR10614
 DOS BUNSYO CANNOT CHANGE TO EISUU NYUURYOKU MODE AFTER REPEATING
 OPEN AND CLOSE DOS SESSION.

APAR= JR10616
 IBM1S506 3RD & 4 TH DRIVE GEOMETRY MAPPING.

APAR= JR10725
 NO KEYBOARD RESPONSE IN A BOOTED VDM SESSION WITH NON-US COUNTRY CODE.

APAR= JR11031
 CTRL-ALT-F10 CTRL-ALT-F10 CAUSES DUMP.

APAR= JR11047
 IBM1S506.ADD TIMES OUT TO FAST ON A SYSJET EIDE WHICH HAS SPUN
 DOWN TO POWER SAVING MODE.

APAR= JR11383
 Y2000:DUAL BOOTING FROM OS2 TO DOS AFTER YEAR 2000 RESULTS IN
 TIME IN BIOS DATA AREA TO BE RESET TO 1-4-1980.

APAR= JR11406
 WARP4 FIXPAK5 ON IBM THINKPAD 760 XD W/DOCKING STATION DOES NOT
 RECOGNIZE DRIVES ON 2ND CONTROLLER.

APAR= JR11450
 SYSTEM HANGS WHEN LOADING IBM1S506.ADD AFTER APPLICATION OF FIXPAK WHEN
 ATAPI DEVICE IS INSTALLED.

APAR= JR11635
 THINKPAD MACHINES WITH PIIX4 IDE DISK CONTROLLERS DO NOT BOOT
 WARP V4.0 WHEN CONNECTED TO A PCI DOCKING STATION.

APAR= JR11771
 ALT+HOME KEY NOT DISABLED VIA KBD_ALTHOME_BYPASS=ON.

APAR= JR11776
 FLOPPY NOT WORKING IF PLUGGED DURING SUSPEND STATE ON THINKPAD.

APAR= JR11866
 ON THKPADS WITH FP6, TYPING TOO FAST RESULTS IN THE KEYBOARD
 LOCKING UP AND BEEPING ON SUBSEQUENT INPUT.

APAR= JR11943
TRAP0003 ON IBM 6589 MACHINES AFTER APPLICATION OF XR_M006.

APAR= JR12031
 TRAP AT SYIREADATFILE + 59.

==============================
OS/2 Warp Device Driver APARs
FixPak Name = XR_D002
==============================
*************************************************************************
* Note: The APARs listed below are fixed in OS/2 Warp Device Driver     *
* Pak XR_D002.                                                          *
* Verification of these APARs is incomplete for this Beta release.      *
*************************************************************************

APAR= IC24071
 CACHE FLUSHING PROBLEM.

APAR= JR13109
 TRAP D IN PRINT01.SYS WHEN USE IRQ AND PRINT INTENSIVE.

APAR= JR13245
 CACHE FLUSHING PROBLEM.

APAR= JR13303
 TRAP D IN KBDBASE.SYS.

APAR= JR13366
 TRAP 3 IN IBMKBD.SYS.

APAR= JR13410
 UKRAINE KEYBOARD LAYOUT DOES NOT WORK IN DOS SESSIONS.

APAR= JR13646
 TRAP D IN MOUSE.SYS FUNCTION PARSEPNP.

APAR= JR13802
 USBCOM.SYS MODEM DRIVER TRAPS WHEN MODEM ATTACHED.

APAR= JR13839
 IBM1S506.ADD SLOWING DOWN WITH A TIME.

APAR= JR13911
 SYSTEM HANGS FOR 2 MIN WHEN PRINTING FROM FS IF NO PRINT OBJECT
 INSTALLED

APAR= JR14014
 USB MOUSE DON'T WAKE UP AFTER SUSPEND - RESUME.

APAR= JR14227
 OS2ASPI.DMD SOMETIMES FREES SCSI DEVICES ALLOCATED BY ANOTHER
 DEVICE MANAGER.

APAR= JR14319
 UNABLE TO PASTE GERMAN UMLAUTE CHARACTER IN DOS WINDOW.

APAR= PJ26138
 CACHE FLUSHING PROBLEM.

APAR= PJ26493
 ATA PCMCIA DRIVER DOES NOT ALLOW LARGE FLOPPY SUPPORT.

APAR= PJ26561
 MOUSE FAILS ON COM3 WITH FAST PII 433MHZ.

APAR= PJ26835
 DPT I2O SCSI CARDS HANG ON BOOT.

==============================
OS/2 Warp Device Driver APARs
FixPak Name = XR_D002
Build Level = 10.042
==============================

APAR= IC24071
 CACHE FLUSHING PROBLEM.

APAR= JR13109
 TRAP D IN PRINT01.SYS WHEN USE IRQ AND PRINT INTENSIVE.

APAR= JR13245
 CACHE FLUSHING PROBLEM.

APAR= JR13303
 TRAP D IN KBDBASE.SYS.

APAR= JR13366
 TRAP 3 IN IBMKBD.SYS.

APAR= JR13410
 UKRAINE KEYBOARD LAYOUT DOES NOT WORK IN DOS SESSIONS.

APAR= JR13646
 TRAP D IN MOUSE.SYS FUNCTION PARSEPNP.

APAR= JR13802
 USBCOM.SYS MODEM DRIVER TRAPS WHEN MODEM ATTACHED.

APAR= JR13839
 IBM1S506.ADD SLOWING DOWN WITH A TIME.

APAR= JR13911
 SYSTEM HANGS FOR 2 MIN WHEN PRINTING FROM FS IF NO PRINT OBJECT
 INSTALLED.

APAR= JR14014
 USB MOUSE DON'T WAKE UP AFTER SUSPEND - RESUME.

APAR= JR14227
 OS2ASPI.DMD SOMETIMES FREES SCSI DEVICES ALLOCATED BY ANOTHER
 DEVICE MANAGER.

APAR= JR14319
 UNABLE TO PASTE GERMAN UMLAUTE CHARACTER IN DOS WINDOW.

APAR= PJ26138
 CACHE FLUSHING PROBLEM.

APAR= PJ26493
 ATA PCMCIA DRIVER DOES NOT ALLOW LARGE FLOPPY SUPPORT.

APAR= PJ26561
 MOUSE FAILS ON COM3 WITH FAST PII 433MHZ.

APAR= PJ26835
 DPT I2O SCSI CARDS HANG ON BOOT.
