OS/COM Installation and Configuration

NOTE on ISA adapters:
  All adapter(s) must be setup with the "interrupt status register" set for
  "SWITCH" mode, not the "PAL" mode.  Up to eight ports per interrupt level is
  supported.  See your adapter's documentation on how to set it up for shared
  interrupts.
  
  There are no interrupt issues for PCI adapters.  PCI adapter interrupt
  levels are assigned by the BIOS at boot time.  PCI interrupts are sharable
  and no user input is required.

  This version of the device driver is for use with Sealevel Systems serial 
  adapters that have an interrupt ID/status register only.

To install the Sealevel Systems OS/COM asynchronous serial device driver, do
one of the following:

Method One:

1. Open the OS/2 System folder

2. Open the Drives folder

3. Double click on the drive you inserted the distribution
   diskette.

4. Double click on the INSTALL.EXE icon.

5. Once INSTALL is loaded, use the "Install..." menu item to setup the
   installation for your system requirements and transfer the required
   files to your system.

    Select "Installation | Install..."

6. Use the "Configuration | OS/COM..." menu item to configure the OS/COM 
   device driver. The configuration process has plenty of on-line help
   to help with setting up OS/COM.

7. Shutdown and re-boot your system.

Method Two:

1. Open an OS/2 command prompt session.

2. Make the disk drive containing the distribution diskette the default drive.

    Example:  [C:\]A: [ENTER)
              (assuming the distribution diskette is in drive A:)

3. Start INSTALL.EXE by typing INSTALL [ENTER]

4. Follow the instructions from item five, above.

OS/COM, COMi, and INSTALL are the property of OS/tools Incorporated and are
copyrighted (c) 1989-95 by OS/tools Incorporated, with all rights reserved.

These programs are licensed to you on a per CPU basis.  One license is 
required for each CPU on which they are installed.  

We know nothing and are responsible for nothing, except for any increased 
productivity and/or pleasure brought about by the use of these programs.  This
is the only disclaimer you have to read.

For additional information about the OS/COM device driver and other OS/tools
products please contact:  

OS/tools Incorporated
7145 Yorktown Drive
Gilroy, CA 95020
Phone: (500)446-7257, FAX: (408)847-7480, BBS: (408)847-7484
Internet: products@os-tools.com or URL: http://www.os-tools.com

For more information on products from Sealevel Systems Incorporated please 
contact:  

Sealevel Systems Incorporated
P.O.  Box 830
Liberty, SC 29657
Phone (864)843-4343 FAX (864)843-3067 

OS/tools, COMscope, COMspool, COMsuite, and COMi are trademarks of OS/tools Incorporated.

OS/2 is a trademark of International Business Machines, Incorporated.

