This is port of the smartmontools package version 6.6 r4424 (SVN).

If you are using DANIS506 driver use hdX device names, e.g.

smartctl -i hd0

If you are using OS2AHCI driver use ahciX device names, e.g.

smartctl -i ahci0

To get list of the drives in the system use "smartctl --scan" command.

Smartctl depends on klibc 0.6.6 (http://trac.netlabs.org/libc/wiki). If you do
not have them - use libs from the "dll" folder in the archive.

To get more information visit www.smartmontools.org website.

Alex Samorukov, samm@os2.kiev.ua
