!---- Try out Energuide requirememts
!
! Set up
*RST                            !Initialize the settings
@750
SAMPLE:HOLD OFF                 !Hold off
SAMPLE:RATE 0.25                !Seconds
MODE RMS                        !Measurment Mode = RMS
FILTER OFF                      !Frequency Filter off
LFILTER OFF                     !Line Filter off
SCALING OFF;AVERAGING OFF       !Scaling & Averaging off
VOLTAGE:RANGE 200V              !Voltage range = 200V
CURRENT:RANGE 15A               !Current range = 15A
MEASURE:ITEM:PRESET NORMAL
MEASURE:ITEM:V:ELEMENT1 ON      !Read volts
MEASURE:ITEM:A:ELEMENT1 ON      !Read amps
MEASURE:ITEM:W:ELEMENT1 ON      !Read watts
MEASURE:ITEM:WH:ELEMENT1 ON     !Read watt-hr
MEASURE:ITEM:VHZ:ELEMENT1 ON    !Read frequency
MEASURE:ITEM:PF:ELEMENT1 ON     !Read power factor
INTEGRATE:MODE NORMAL
INTEGRATE:RESET
INTEGRATE:START
STATUS:EESR?
!
@500
MEASURE:NORMAL:VALUE?
@500
MEASURE:NORMAL:VALUE?
@500
INTEGRATE:STOP
MEASURE:NORMAL:VALUE?

