### Chrono-log K-series WWVB receiver

#### Synopsis

Address: 127.127.32.u
Reference ID: `CHRONOLOG`
Driver ID: `CHRONOLOG`
Serial Port: `/dev/chronologu`; 2400 bps, 8-bits, no parity
Features: `(none)`

#### Description

This driver supports the Chrono-log K-series WWVB receiver. This is a very old receiver without provisions for leap seconds, quality codes, etc. It assumes output in the local time zone, and that the C library mktime()/localtime() routines will correctly convert back and forth between local and UTC. There is a hack in the driver for permitting UTC, but it has not been tested.

Most of this code is originally from refclock_wwvb.c with thanks. It has been so mangled that wwvb is not a recognizable ancestor.

    Timecode format: Y yy/mm/ddCLZhh:mm:ssCL
    Y - year/month/date line indicator
    yy/mm/dd -- two-digit year/month/day
    C - \r (carriage return)
    L - \n (newline)
    Z - timestamp indicator
    hh:mm:ss - local time

Last modified: Sun Feb 14 11:57:27 EST 1999