### NTP PARSE clock data formats

The parse driver currently supports several clocks with different query mechanisms. In order for you to find a sample that might be similar to a clock you might want to integrate into parse i'll sum up the major features of the clocks (this information is distributed in the parse/clk_*.c and ntpd/refclock_parse.c files).

#### Meinberg clocks

    Meinberg: start=<STX>, end=<ETX>, sync on start
          pattern="\2D:  .  .  ;T: ;U:  .  .  ;    \3"
          pattern="\2  .  .  ;  ;   :  :  ;        \3"
          pattern="\2  .  .  ;  ;   :  :  ;    :  ;        ;   .         .       "

Meinberg is a German manufacturer of time code receivers. Those clocks have a pretty common output format in the stock version. In order to support NTP Meinberg was so kind to produce some special versions of the firmware for the use with NTP. So, if you are going to use a Meinberg clock please ask whether there is a special Uni Erlangen version. You can reach Meinberg via the Web. Information can also be ordered via eMail from info@meinberg.de

General characteristics:
Meinberg clocks primarily output pulse per second and a describing ASCII string. This string can be produced in two modes. either upon the reception of a question mark or every second. NTP uses the latter mechanism. The DCF77 variants have a pretty good relationship between RS232 time code and the PPS signal while the GPS receiver has no fixed timeing between the datagram and the pulse (you need to use PPS with GPS!) on DCF77 you might get away without the PPS signal.

The preferred tty setting for Meinberg is:

    		CFLAG		(B9600|CS7|PARENB|CREAD|HUPCL)
    		IFLAG		(IGNBRK|IGNPAR|ISTRIP)
    		OFLAG		0
    		LFLAG		0

The tty setting for Meinberg GPS 166/167 receivers is:

    		CFLAG		(B19200|CS8|PARENB|CREAD|HUPCL)
    		IFLAG		(IGNBRK|IGNPAR|ISTRIP)
    		OFLAG		0
    		LFLAG		0

The clock is run at datagram once per second. Stock dataformat is:

        <STX>D:<dd>.<mm>.<yy>;T:<w>;U:<hh>:<mm>:<ss>;<S><F><D><A><ETX>
    pos:  0  00 00 0 00 0 11 111 1 111 12 2 22 2 22 2 2  2  3  3   3
          1  23 45 6 78 9 01 234 5 678 90 1 23 4 56 7 8  9  0  1   2

    <STX>           = '\002' ASCII start of text
    <ETX>           = '\003' ASCII end of text
    <dd>,<mm>,<yy>  = day, month, year(2 digits!!)
    <w>             = day of week (sunday= 0)
    <hh>,<mm>,<ss>  = hour, minute, second
    <S>             = '#' if never synced since powerup else ' ' for DCF U/A 31
                      '#' if not PZF sychronisation available else ' ' for PZF 535
    <F>             = '*' if time comes from internal quartz else ' '
    <D>             = 'S' if daylight saving time is active else ' '
    <D>             = 'U' if UTC time code is deliverd else ' '
    <A>             = '!' during the hour preceeding an daylight saving time
                          start/end change
    <A>             = 'A' if a leap second is announced

            <STX><dd>.<mm>.<yy>; <w>; <hh>:<mm>:<ss>; <U><S><F><D><A><L><R><ETX>
        pos:  0   00 0 00 0 00 11 1 11 11 1 11 2 22 22 2  2  2  2  2  3  3   3
              1   23 4 56 7 89 01 2 34 56 7 89 0 12 34 5  6  7  8  9  0  1   2
        <STX>           = '\002' ASCII start of text
        <ETX>           = '\003' ASCII end of text
        <dd>,<mm>,<yy>  = day, month, year(2 digits!!)
        <w>             = day of week (sunday= 0)
        <hh>,<mm>,<ss>  = hour, minute, second
        <U>             = 'U' UTC time display
        <S>             = '#' if never synced since powerup else ' ' for DCF U/A 31
                          '#' if not PZF sychronisation available else ' ' for PZF 535
        <F>             = '*' if time comes from internal quartz else ' '
        <D>             = 'S' if daylight saving time is active else ' '
        <A>             = '!' during the hour preceeding an daylight saving time
                              start/end change
        <L>             = 'A' LEAP second announcement
        <R>             = 'R' alternate antenna

Meinberg GPS166 receiver
You must get the Uni-Erlangen firmware for the GPS receiver support to work to full satisfaction !

            <STX><dd>.<mm>.<yy>; <w>; <hh>:<mm>:<ss>; <+/-><00:00>; <U><S><F><D><A><L><R><L>; <position...><ETX>
     *
               000000000111111111122222222223333333333444444444455555555556666666
               123456789012345678901234567890123456789012345678901234567890123456
            \x0209.07.93; 5; 08:48:26; +00:00;        ; 49.5736N  11.0280E  373m\x03
     *

        <STX>           = '\002' ASCII start of text
        <ETX>           = '\003' ASCII end of text
        <dd>,<mm>,<yy>  = day, month, year(2 digits!!)
        <w>             = day of week (sunday= 0)
        <hh>,<mm>,<ss>  = hour, minute, second
        <+/->,<00:00>   = offset to UTC
        <S>             = '#' if never synced since powerup else ' ' for DCF U/A 31
                          '#' if not PZF sychronisation available else ' ' for PZF 535
        <U>             = 'U' UTC time display
        <F>             = '*' if time comes from internal quartz else ' '
        <D>             = 'S' if daylight saving time is active else ' '
        <A>             = '!' during the hour preceeding an daylight saving time
                              start/end change
        <L>             = 'A' LEAP second announcement
        <R>             = 'R' alternate antenna (reminiscent of PZF535) usually ' '
        <L>		   = 'L' on 23:59:60

For the Meinberg parse look into clock_meinberg.c

#### Raw DCF77 Data via serial line

RAWDCF: end=TIMEOUT>1.5s, sync each char (any char),generate psuedo time codes, fixed format

direct DCF77 code input

In Europe it is relatively easy/cheap the receive the german time code transmitter DCF77. The simplest version to process its signal is to feed the 100/200ms pulse of the demodulated AM signal via a level converter to an RS232 port at 50Baud. parse/clk_rawdcf.c holds all necessary decoding logic for the time code which is transmitted each minute for one minute. A bit of the time code is sent once a second.

    	The preferred tty setting is:
    		CFLAG           (B50|CS8|CREAD|CLOCAL)
    		IFLAG		0
    		OFLAG		0
     		LFLAG		0

#### DCF77 raw time code

From "Zur Zeit", Physikalisch-Technische Bundesanstalt (PTB), Braunschweig und Berlin, M„rz 1989

Timecode transmission:

    	AM:

    	time marks are send every second except for the second before the
    	next minute mark
    	time marks consist of a reduction of transmitter power to 25%
    	of the nominal level
    	the falling edge is the time indication (on time)
    	time marks of a 100ms duration constitute a logical 0
    	time marks of a 200ms duration constitute a logical 1

see the spec. (basically a (non-)inverted psuedo random phase shift) encoding:

    	FM:

    	Second	Contents
    	0  - 10	AM: free, FM: 0
    	11 - 14	free
    	15		R     - alternate antenna
    	16		A1    - expect zone change (1 hour before)
    	17 - 18	Z1,Z2 - time zone
    		 0  0 illegal
    		 0  1 MEZ  (MET)
    		 1  0 MESZ (MED, MET DST)
    		 1  1 illegal
    	19		A2    - expect leap insertion/deletion (1 hour before)
    	20		S     - start of time code (1)
    	21 - 24	M1    - BCD (lsb first) Minutes
    	25 - 27	M10   - BCD (lsb first) 10 Minutes
    	28		P1    - Minute Parity (even)
    	29 - 32	H1    - BCD (lsb first) Hours
    	33 - 34      H10   - BCD (lsb first) 10 Hours
    	35		P2    - Hour Parity (even)
    	36 - 39	D1    - BCD (lsb first) Days
    	40 - 41	D10   - BCD (lsb first) 10 Days
    	42 - 44	DW    - BCD (lsb first) day of week (1: Monday -> 7: Sunday)
    	45 - 49	MO    - BCD (lsb first) Month
    	50           MO0   - 10 Months
    	51 - 53	Y1    - BCD (lsb first) Years
    	54 - 57	Y10   - BCD (lsb first) 10 Years
    	58 		P3    - Date Parity (even)
    	59		      - usually missing (minute indication), except for leap insertion

#### Schmid clock

Schmid clock: needs poll, binary input, end='\xFC', sync start

The Schmid clock is a DCF77 receiver that sends a binary time code at the reception of a flag byte. The contents if the flag byte determined the time code format. The binary time code is delimited by the byte 0xFC.

    	TTY setup is:
    		CFLAG		(B1200|CS8|CREAD|CLOCAL)
    		IFLAG		0
    		OFLAG		0
     		LFLAG		0

The command to Schmid's DCF77 clock is a single byte; each bit allows the user to select some part of the time string, as follows (the output for the lsb is sent first).

    	Bit 0:	time in MEZ, 4 bytes *binary, not BCD*; hh.mm.ss.tenths
    	Bit 1:	date 3 bytes *binary, not BCD: dd.mm.yy
    	Bit 2:	week day, 1 byte (unused here)
    	Bit 3:	time zone, 1 byte, 0=MET, 1=MEST. (unused here)
    	Bit 4:	clock status, 1 byte,	0=time invalid,
    					1=time from crystal backup,
    					3=time from DCF77
    	Bit 5:	transmitter status, 1 byte,
    					bit 0: backup antenna
    					bit 1: time zone change within 1h
    					bit 3,2: TZ 01=MEST, 10=MET
    					bit 4: leap second will be
    						added within one hour
    					bits 5-7: Zero
    	Bit 6:	time in backup mode, units of 5 minutes (unused here)

#### Trimble SV6 ASCII time code (TAIP)

Trimble SV6: needs poll, ascii timecode, start='>', end='<', query='>QTM<', eol='<'

Trimble SV6 is a GPS receiver with PPS output. It needs to be polled. It also need a special tty mode setup (EOL='<').

    	TTY setup is:
    		CFLAG            (B4800|CS8|CREAD)
    		IFLAG            (BRKINT|IGNPAR|ISTRIP|ICRNL|IXON)
    		OFLAG            (OPOST|ONLCR)
    		LFLAG            (ICANON|ECHOK)

Special flags are:

    		PARSE_F_PPSPPS	    - use CIOGETEV for PPS time stamping
    		PARSE_F_PPSONSECOND - the time code is not related to
    				      the PPS pulse (so use the time code
    				      only for the second epoch)

    	Timecode
    	0000000000111111111122222222223333333	/ char
    	0123456789012345678901234567890123456	\ posn
    	>RTMhhmmssdddDDMMYYYYoodnnvrrrrr;*xx<	Actual
    	----33445566600112222BB7__-_____--99-	Parse
    	>RTM                      1     ;*  < 	Check

#### ELV DCF7000

ELV DCF7000: end='\r', pattern=" - - - - - - - \r"

The ELV DCF7000 is a cheap DCF77 receiver sending each second a time code (though not very precise!) delimited by '`r'

    	Timecode
    	  YY-MM-DD-HH-MM-SS-FF\r

    		FF&0x1	- DST
    		FF&0x2	- DST switch warning
    		FF&0x4  - unsynchronised

#### HOPF 6021 und Kompatible

HOPF Funkuhr 6021 mit serieller Schnittstelle Created by F.Schnekenbuehl <frank@comsys.dofn.de> from clk_rcc8000.c Nortel DASA Network Systems GmbH, Department: ND250 A Joint venture of Daimler-Benz Aerospace and Nortel.

     hopf Funkuhr 6021
          used with 9600,8N1,
          UTC via serial line
          "Sekundenvorlauf" ON
          ETX zum Sekundenvorlauf ON
          dataformat 6021
          output time and date
          transmit with control characters
          transmit evry second

Type 6021 Serial Output format

          000000000011111111 / char
          012345678901234567 \ position
          sABHHMMSSDDMMYYnre  Actual
           C4110046231195     Parse
          s              enr  Check

      s = STX (0x02), e = ETX (0x03)
      n = NL  (0x0A), r = CR  (0x0D)

      A B - Status and weekday

      A - Status

          8 4 2 1
          x x x 0  - no announcement
          x x x 1  - Summertime - wintertime - summertime announcement
          x x 0 x  - Wintertime
          x x 1 x  - Summertime
          0 0 x x  - Time/Date invalid
          0 1 x x  - Internal clock used
          1 0 x x  - Radio clock
          1 1 x x  - Radio clock highprecision

      B - 8 4 2 1
          0 x x x  - MESZ/MEZ
          1 x x x  - UTC
          x 0 0 1  - Monday
          x 0 1 0  - Tuesday
          x 0 1 1  - Wednesday
          x 1 0 0  - Thursday
          x 1 0 1  - Friday
          x 1 1 0  - Saturday
          x 1 1 1  - Sunday

#### Diem Computime Clock

The Computime receiver sends a datagram in the following format every minute

       Timestamp	T:YY:MM:MD:WD:HH:MM:SSCRLF
       Pos          0123456789012345678901 2 3
    		0000000000111111111122 2 2
       Parse        T:  :  :  :  :  :  :  \r\n

       T	Startcharacter "T" specifies start of the timestamp
       YY	Year MM	Month 1-12
       MD	Day of the month
       WD	Day of week
       HH	Hour
       MM   Minute
       SS   Second
       CR   Carriage return
       LF   Linefeed

#### WHARTON 400A Series Clock with a 404.2 Serial interface

The WHARTON 400A Series clock is able to send date/time serial messages in 7 output formats. We use format 1 here because it is the shortest. We set up the clock to send a datagram every second. For use with this driver, the WHARTON 400A Series clock must be set-up as follows :

      					Programmable	Selected
      					Option No	Option
    	BST or CET display		3		9 or 11
    	No external controller		7		0
    	Serial Output Format 1		9		1
    	Baud rate 9600 bps		10		96
    	Bit length 8 bits		11		8
    	Parity even			12		E

WHARTON 400A Series output format 1 is as follows :

       Timestamp	STXssmmhhDDMMYYSETX
       Pos		0  12345678901234
      		0  00000000011111

       STX	start transmission (ASCII 0x02)
       ETX	end transmission (ASCII 0x03)
       ss	Second expressed in reversed decimal (units then tens)
       mm	Minute expressed in reversed decimal
       hh	Hour expressed in reversed decimal
       DD	Day of month expressed in reversed decimal
       MM	Month expressed in reversed decimal (January is 1)
       YY	Year (without century) expressed in reversed decimal
       S	Status byte : 0x30 +
    		bit 0	0 = MSF source		1 = DCF source
    		bit 1	0 = Winter time		1 = Summer time
    		bit 2	0 = not synchronised	1 = synchronised
    		bit 3	0 = no early warning	1 = early warning