NVRAM ERROR
Prev | Chapter 1. | Next

## NVRAM ERROR

This message indicates that the NVRAM (Non-Volatile Random Access Memory) could not be updated with new values. This may be due to invalid values being read from the NVRAM segment or because of a failing NVRAM.

Some brief information on NVRAM is available in chapter 10 of Irix Admin: System Configuration and Operation.

If the problem persists, contact your System Administrator or your service provider.

For information on how to configure or disable System Alerts, click here.

Prev | Table of Contents | Next
Cannot Communicate with the Network |  | PCI Self Test Error