About ICONS Displayed in Confidence Test Window
Prev | Chapter 1. Confidence Test Help | Next

## About ICONS Displayed in Confidence Test Window

The Confidence test panel displays icons for the devices that have been properly installed on the system and are recognized through `hinv(1M)`. The devices that the Confidence test recognizes are:

- Audio

- Video

- Flat panel

- ISDN

- Floptical

- Tape drives

- CD-ROM

- Keyboard

- Mouse

- Monitor

- Dials and buttons

- Spaceball

- Tablet

If you have recently installed one of the preceding devices but you do not see an icon for the device in the Confidence test panel, verify the following:

- If the Confidence test was launched remotely, some of the devices that communicate with the X server do not appear in the Confidence test panel. See “About the Confidence Test Panel” for more information.

- Does the system recognize the device? Execute the `hinv` command to see if the system recognizes the device. Refer to the `hinv(1M)` man page for further information.

  The system output should be similar to:

      % hinv
      CPU: MIPS R5000 Processor Chip Revision: 2.1
      FPU: MIPS R5000 Floating Point Coprocessor Revision: 1.0
      1 250 MHZ IP32 Processor
      Main memory size: 128 Mbytes
      Secondary unified instruction/data cache size: 1 Mbytes on Processor 0
      Instruction cache size: 32 Kbytes
      Data cache size: 32 Kbytes
      FLASH PROM version 4.10
      Integral SCSI controller 0: Version ADAPTEC 7880
        Disk drive: unit 1 on SCSI controller 0
        CDROM: unit 4 on SCSI controller 0
      Integral SCSI controller 1: Version ADAPTEC 7880
      On-board serial ports: tty1
      On-board serial ports: tty2
      On-board EPP/ECP parallel port
      CRM graphics installed
      Integral Ethernet: ec0, version 1
      Iris Audio Processor: version A3 revision 0
      Video: MVP unit 0 version 1.4
      AV: AV1 Card version 1, O2Cam type 1 version 0 connected.
      Vice: TRE
      1600SW Flat Panel adapter board and display.

- A few devices are not recognized by the `hinv` command. Dials and buttons, tablet, and spaceball devices are not displayed through `hinv`.

  | Note: Make sure the `eoe.sw.optinput` subsystem is loaded by using the `versions eoe.sw.optinput` command. After verifying that, make sure the serial port is properly configured for the device by launching the System Manager from the Toolchest, selecting the Hardware and Devices items, and then selecting the Serial Device Manager. Configure the port for your device.

- The ISDN interface is not recognized by the system unless the `isdn_eoe` subsystem is installed.

  | Note: Make sure the `isdn_eoe.sw.isdn` subsystem is loaded by using the `versions isdn_eoe.sw.isdn` command.

- SCSI devices that have been added to the system require that the peripheral device be powered on prior to the system booting. If you have just installed a SCSI peripheral, try shutting down the system and powering it off, and then powering it back on after the SCSI peripheral device is powered on.

For additional information on adding SCSI devices, see the Personal System Administration Guide or IRIX Admin: Peripheral Devices. For additional questions or assistance, contact your local support provider.

Prev | Table of Contents | Next
Dials and Buttons Confidence Test |  | Audio Confidence Test