1 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Description:

The R4300 is an ultra low-cost RISC micr oprocessor optimized for demanding consumer applications. The R4300 provides performance equivalent to a high-end PC at a cost point to enable set-top terminals, games and portable consumer devices. The R4300 is compatible with the MIPS R4000 family of RISC micr oprocessors and will r un all existing softwar e. Unlike its pr edecessors designed for use in workstations, however , the R4300 is tailor ed to lower the cost of systems it is used in, a r equir ement for price-sensitive consumer pr oducts. The R4300 is also an ef fective embedded processor, supported by curr ently available development tools and pr oviding very high performance at a low price-point.

Features:

Low Power Dissipation:

• 1.8W (normal)

High Performance:

• 55 SPECint92 • 50 SPECfp92

High integration on-chip:

• 16K I-cache, 8K D-cache • Unified datapath • 32 double-entry J-TLB • 2 entry micr o I-TLB

Power Management Featur es:

• Reduced Power Mode • Instant On/Of f

R4000 family compatibility:

• R4000 softwar e compatible • Runs W indows NT/UNIX

Addr/Data Controls

32-bit System Interface

Instruction

Cache

Data Cache

Co-Processor 0

Instruction Address

Pipeline Control

Clk Gen

Consumer Applications:

Set-top terminals

Game systems

Personal Digital Assistants

Embedded Applications

X-terminals

Laser printers

Factory automation

Networking: r outers, bridges

Graphics acceleration

Packaging:

R4300 (120-pin PQFP)

R4300-test (179-pin C-PGA)

Overview:

The success of the MIPS R3000 pr ocessor and derivatives has established the MIPS ar chitectur e as an attractive high-performance choice in emer ging consumer applications such as interactive TV and games. The R4300 is the 64-bit successor to the R3000 for this class of applications. It is specifically designed to be extr emely lowcost from the outset, yet supply the performance necessary for full interactivity .

The R4300 achieves its low-cost goal by holding to a very small die size, simple package and low testing costs. It is further enabled for consumer applications by easily interfacing to other low-cost components. Its low power consumption also r educes system cost by combining high clock speed with limited power drawn, saving on power supply and heat dissipation costs.

The R4300 has a number of design featur es to r educe power . These include an all-dynamic design, unified integer and floating-point datapath, a r educed power mode of operation, and caches partitioned into separate banks.

Printers, networking devices and other embedded applications will also benefit fr om the high-performance, low-cost and high-bandwidth interface of the R4300. The R4300 will become the next standar d in low-cost processing on MIPS.

mips

Open RISC T echnology

PRODUCT INFORMA TION

R4300 MICROPROCESSOR

MasterClock

64-bit

Unit

Execution

2 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

R4300 ARCHITECTURE

DATA FORMA T

The R4300 defines a 64-bit double-wor d, a 32-bit wor d, a 16-bit halfwor d and an 8-bit byte. The byte or dering is configurable in either Big-endian or Little-endian format. Figur es 1 & 2 show the or dering of bytes for Big-endian and Little-endian conventions.

PROCESSOR RESOURCES

The R4300 CPU pr ovides sixty-four 64-bit wide registers. Thirty-two of these r egisters, r eferred to as General Purpose Register (GPRs), ar e reserved for integer operations while the other thirty-two r egister , referred to as Floating Point General Purpose Register (FGRs), ar e reserved for floating point operations.

The width of these r egisters depends on the mode of operation. In 32-bit mode, they ar e treated as 32 bits wide. In 64-bit mode, they ar e treated as 64 bits wide.

The R4300 also contains six special r egisters: the program counter (PC), multiply/divide r esult Hi and LO, load/link (LL) bit, and floating point implementation and contr ol registers FCR0 and FCR31; shown in Figur e 4. The program counter r egister contains the addr ess of the

31 24 23 16 15 8 7 0

byte-0 byte-1 byte-2 byte-3 byte-4 byte-5 byte-6 byte-7 byte-8 byte-9 byte-A byte-B byte-C byte-D byte-E byte-F

Word Address C 8 4 0

High Addr

Low Addr Most significant byte is at lowest address

Word is addressed by byte address of most significant byte

Figure 1: Big-endian Byte Alignment

31 24 23 16 15 8 7 0

byte-3 byte-2 byte-1 byte-0 byte-7 byte-6 byte-5 byte-4 byte-B byte-A byte-9 byte-8 byte-F byte-E byte-D byte-C

Word Address C 8 4 0

High Addr

Low Addr Least significant byte is at lowest address

Word is addressed by byte address of least significant byte

Figure 2: Little-endian Byte Alignment

0 31 32 63 r0 r1 r2

r30 r31

General Purpose Regs (GPRs) 0 31 32 63 FGR0 FGR1 FGR2

FGR30 FGR31

FP General Purpose Regs (FGRs)

Figure 3: General Purpose Registers curr ent instr uction. The multiply/divide r egisters stor e the result of integer multiply operations and the quotient and remainder of integer divide operations. The load/link bit is dedicated for load-link and stor e-conditional instr uctions which can be used to perform SYNC operations. The two floating point contr ol register FCR0 and FCR31 pr ovide the implementation/r evision information and contr ol/status of the floating point copr ocessor (CP1)

In addition, the R4300 operates with up to four tightly coupled copr ocessors (designated CP0 thr ough CP3). Copr ocessor zer o (CP0) is implemented as an integral part of the CPU and supports the virtual memory system together with exception handling. Copr ocessor one (CP1) is reserved for the floating point unit, while copr ocessor two and thr ee are reserved for futur e use.

Copr ocesssor zer o contains r egisters shown in Figur e 5 plus a 32-entry TLB with each entry consisting of an even/ odd pair of physical addr esses and tag field.

The CP0 r egisters can be consider ed as two distinct functional sets. The first set comprises those which support the TLB operations. The second set is formed fr om those registers that r eflect the status of the pr ocessor. All of the CP0 registers ar e accessible by softwar e.

INSTRUCTION SET

All R4300 instr uctions ar e 32 bits (single wor d) long aligned on a wor d boundary . This appr oach simplifies instr uction decoding, mor e complicated operations and addr essing modes ar e synthesized by the compiler . There are thr ee instr uction formats: I-type (immediate), J-type

0 31 32 63 PC Program Counter (PC)

0 31 32 63 MultHI MultLO

Multiply/Divide Registers

0 31 FCR0 FCR31

Floating Point

Impl/Rev Control/Status

Registers 0 LLbit

Figure 4: Special Registers

PageMask 5* EntryHi 10* EntryLo0 2*

EntryLo1 3*

Index 0*

Random 1*

Wired 6*

Context 4*

Count 9*

TagHi 29*

WatchHi 19*

SR 12*

CacheErr 27*

EPC 14* Config 16* BadVAddr 8*

Compare 11*

TagLo 29*

WatchLo 18*

Cause 13*

PErr 26*

ErrEPC 30* PRId 15*

LLAddr 17*

Safe Entries Safe Entries

EVEN ENTRIES ODD ENTRIES

CP0 REGISTERS

XContext 20*

Figure 5: Coprocessor-0 Registers

3 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

(jump), and R-type (r egister), as shown in Figur e 6.

Load and Stor e instr uctions move data between memory and the general r egisters. They ar e all immediate (I-type) instr uctions. The only addr essing mode that load and stor e instr uctions dir ectly support is base register plus 16-bit signed extended immediate offset.

Load and store instr uction opcodes determines the access type which indicates the size of data item to be loaded or stor ed. Regar dless of the access type or bytenumbering or der (endianess), the addr ess field specifies the lowest byte of the addr ess location being accessed. Table 10 lists all load and stor e instr uctions defined by the MIPS Instr uction Set Ar chitectur e (ISA) and ISA Extension.

Computational instr uctions perform arithmetic, logical, shift, multiply , and divide operations on values in registers. They occur in both r egister (R-Type) format, in which both operands ar e registers, and immediate (I-T ype) format, in which one operand is a 16-bit immediate. When operated in 64-bit mode, 32-bit operands must be corr ectly sign extended. T able 11 lists all computational instr uctions defined by the MIPS ISA and ISA Extensions.

Jump and branch instr uctions change the contr ol flow of a pr ogram. They occur in both r egister (R-Type) format, and immediate (I-T ype) format. All jump and branch instr uctions occur with an ar chitectur e delay of one instr uction; that is, the instr uction immediately following the jump or branch is always executed while the tar get instr uction is being fetched. T able 12 summarizes jump and branch instr uctions defined by the MIPS ISA and ISA Extensions.

Special instr uctions allow the softwar e to initiate traps

0 15 16 20 21 25 26 31

56 10 11

26

6

Immediate

Op code rs rt

0 25 26 31 target Op code

0 15 16 20 21 25 26 31 Op code rs rt

16 5 5

5 5 5 5 6

6

6

rd sa funct

I-Type (Immediate)

R-Type (Register)

J-Type (Jump)

Figure 6: Instruction Formats

Op code is a 6-bit operation code rs is a 5-bit sour ce register specifier rt is a 5-bit tar get register specifier immediate is a 16-bit immediate, branch displacement or addr ess displacement target is a 26-bit jump tar get addr ess rd is a 5-bit destination r egister specifier sa is a 5-bit shift amount funct is a 5-bit function field

and ar e always R-T ype. Special instr uctions that ar e valid for all MIPS R-Series pr ocessors ar e shown in T able 12.

Exception instr uctions of fer trapping mechanism to assist in softwar e debug. They ar e shown in T able 14.

Coprocessor instr uctions perform operations in the respective copr ocessors. Copr ocessor loads and stor es are Itype, and copr ocessor computational instr uctions have coprocessor dependent formats. T able 12 summarizes the coprocessor instr uctions that ar e valid in all MIPS R-Series processor and the extensions to the MIPS ISA.

PIPELINE

The R4300 pr ocessor has a five-stage execution pipeline. Each pipeline stage takes one pcycle (pclock r uns at twice the fr equency of MasterClock). The execution of each instr uction thus has a latency of at least five pcycle. Once the pipeline has been completely filled, five instr uctions ar e always being executed simultaneously . When the pipeline is not stalled, the pr ocessor has an throughput of one instr uction per pcycle. The pipeline is in-order issue, in-or der execution, and in-or der completion, the same or der as in the instr uction str eam.

The five stages of the R4300 pipeline ar e: Instr uction Cache (IC), Instr uction Decode and Register File Read (RF),

Figure 7: Pipeline Activities

IC RF EX DC WB

Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2

ITLB ITC

ICF IDEC RFR

ALU

DVA

BCMP IVA

DTLB DTC

DCR LA RFW

RFW

DCW

Instr . Fetch Instr . Decode Reg. File Read

Arithmetic/Logical Operations

PClock

Load/Store Operations

Jump/Branch Operations

Phase

Cycle

Cycle Phase Mnemonic Descriptions IC Φ 1 No activity

Φ 2 ICFITLB Instr uction Cache Fetch Instr uction micr o-TLB read

RF Φ 1 ITC Instr uction cache T ag Check Φ 2 RFR IDEC IVA Register File Read Instr uction Decode Instr uction V irtual Addr ess Calculation

EX Φ 1 BCMP ALU DVA Branch Compar e Arithmetic Logic Operation Data Virtual Addr ess Calculation

Φ 2 No new activity started

DC Φ 1 DCRDTLB Data Cache Read Data TLB look-up

Φ 2 LADTC Load Data Alignment Data Cache T ag Check WB Φ 1 DCWRFW Data Cache W rite Register File W rite

Φ 2 No activity

4 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Execution (EX), Data Cache Read (DC), and Register File or Data Cache W rite Back (WB). Figur e 7 shows the activities occurring during each pipeline stage for ALU, load and store, and branch instr uctions. Below ar e detail descriptions of the activities during each stage.

IC: An instr uction addr ess is pr esented by the

addr ess unit and the instr uction cache fetch begins. The instr uction micr o-TLB starts the virtual-to-physical addr ess translation.

RF: The instr uction becomes available and the

instr uction decoder decodes the instr uction and check for interlock conditions. The instr uction cache tag is checked against the page frame number obtained fr om the micr o-TLB. Any requir ed operands ar e read fr om the r egister file and the r esult fr om the EX or DC stages is bypassed to the following EX stage if r equir ed. The addr ess unit generates next instr uction addr ess.

EX: For ALU class instr uctions, the ALU performs an

arithmetic or logical operation. For load and store class instr uctions, the ALU generates the data virtual addr ess. For branch instr uctions, the ALU determines whether the branch condition is true .

DC: For load and stor e instr uctions, the data cache is

accessed and data virtual-to-physical addr ess translation is performed. At the end of DC stage, the data becomes available and the load-align shifts the data to a wor d or double-wor d boundary . In addition, the data cache tag is checked against the page frame number obtained fr om the joint TLB.

WB: For register -to-register or load instr uctions, the

result is written back to the r egister file. For stor e instr uctions, the data cache is updated with the store data.

The R4300 has a branch delay of one cycle and a load delay of one cycle. The branch delay is observed by noting that the branch compar e logic operates during the EX pipestage, pr oducing the tar get addr ess which is available for the IC pipestage of the second subsequent instr uction. The first subsequent instr uction is the instr uction in the delay slot and will be allowed to complete whether the branch is taken of not, as illustrated in Figur e 8. Similarly ,

the load delay of one is evident when the completion of a load at the end of the DC pipestage, pr oduces an operand which is available for the EX pipestage of the second subsequent instr uction. The load delay is illustrated in Figur e 9.. Har dwar e detects whether the instr uction in the branch delay slot is dependent on r egister to be loaded,

Figure 8: Branch Delay Slot

IC RF EX DC WB

IC RF EX DC WB

IC RF EX DC WB

beq r2, r3, target

addi r2, 1

target: ld r4, (r5) branch delay slot instruction

instruction branch instruction

target

and interlocks accor dingly .

The pipeline flow is interr upted when an interlock condition is detected or when an exception occurs.An interlock condition is r esolved by stalling the whole pipeline, on the other hand an exception aborts the r elevant instr uction and all those that follow . Figur e 10 illustrates the various interlock conditions and the dif ferent types of exceptions, at their pr edefined pipestage.

In the case of simultaneous stall r equests fr om dif ferent pipestages, the pipeline contr ol unit prioritizes which stall request is allowed to be r esolved, in case of possible resour ce conflict. A stall r equest fr om the DC pipestage has higher priority than a stall r equest fr om the RF pipestage.

Figure 9: Load Delay Slot

IC RF EX DC WB

IC RF EX DC WB

IC RF EX DC WB

ld r2, (r4)

addi r4, 4

add r2, r6 load delay slot

from DC to EX pipestage load instruction

load data is bypassed

Figure 10: Pipeline Interlocks and Exceptions

IC RF EX DC WB

Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2 Φ 1 Φ 2

PClock Phase

Cycle

Pipe Interlock Conditions

Descriptions Descriptions

ITM Instr uction TLB Miss ICB Instr uction Cache Busy

LDI Load Interlock MCI Multi-Cycle Interlock

CPI Copr ocessor -2 Interlock DCB Data Cache Busy

COp Cache Op DCM Data Cache Miss

DCPI Data Cache Parity Interlock CP0I CP0 Bypass Interlock

Pipe Exception Conditions

Descriptions Descriptions

IADE Instr uction Addr ess Err or ITLB Instr uction TLB Miss

ICPE Instr uction Cache Parity Err or IBE Instr uction Bus Err or

SYSC System Call Instr uction BRPT BreakPoint Instr uction

RSVD Reserved Instr uction CPU Copr ocessor Unusable

RST External Reset Exception NMI Non-Maskable Interr upt

OVFL Integer Overflow TRAP TRAP Exception

FPE Floating Point Exception CPE Copr ocessor -2 Exception

DAE Data Addr ess Err or DTLB Data TLB Exception

DCPE Data Cache Parity Err or WAT Reference Watch Addr ess

DBE Data Bus Err or INTR External Interr upt

Stalls

Exceptions

ITM ICB LDI MCI CPI DCM DCB COp

IADE ITLB ICPE IBE SYSC BRPT CPU RSVD RST NMI OVFL TRAP FPE CPE DADE DTLB DCPE WAT DBE INTR

DCPI CP0I

DCPE

5 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

EXECUTION UNIT

The execution unit is designed to r educe power consumption and simplify the har dwar e requir ements while pr oviding a high level of performance by maximizing usage of each functional element. Integer performance is optimized for the R4300’s tar get applications.

The execution unit is tightly coupled to the on-chip cache memory system, instr uction and data caches, and the on-chip memory management unit, CP0. This unit has a multifunction pipe and is r esponsible for the execution of:

• Integer arithmetic and logic instr uctions • Floating-point Copr ocessor CP1 instr uctions • Branch/Jump instr uctions • Load/Stor e instr uctions • Exception instr uctions • Special instr uctions

All floating-point instr uctions, as defined in the MIPS ISA for the floating-point copr ocessor CP1, ar e processed by the same har dwar e as used for the integer instr uctions.

However , the execution of floating-point instr uctions can still be disabled via the copr ocessor unusable CU bit defined in the CP0 Status Register .

The execution unit uses a modular design appr oach to further r educe dynamic power consumption. Contr ol logic is partitioned into small independent blocks r esponsible for a set of instr uctions. When r elevant instr uctions ar e not in the instr uction str eam, the corr esponding contr ol blocks become inactive. Also, when functional elements in the datapath ar e idle, they operate on a constant (0’s or 1’s) selected to minimize power dissipation.

The execution unit’s datapath consists of: a 64-bit integer/mantissa datapath, an operand bypass network, 32 64-bit integer r egisters, 32 64-bit floating-point r egisters, a 12-bit exponent datapath, and a 64-bit instr uction virtual addr ess generator .

The integer/mantissa datapath is 64 bits wide and is compatible with both 32-bit and 64-bit operands for integer and floating-point numbers. It has a Boolean Logic functional unit, a carry-pr opagate adder and a bidirectional shifter , as illustrated in Figur e 11.

COMBINED REGISTER FILE

SIGN EXTEND

UNPACK

SIGN EXTEND

UNPACK

SIGN EXTEND

RS RT

BYPASS MUX BYPASS MUX

BOOTH MUX ADD MUX

CARRY-PROPAGATE ADDER SHIFTER

RESULT MUX

SUM REG

SHIFT MUX

LOGICAL OPERATION

RMUX

OPMUX

LOAD ALIGNER

DBUS

SIGN EXTEND REPACK

WB REG

DVA1DC

IMMEDIA TE

SHIFT MUX SL2 SHIFT MUX

SL1, SL2

SHIFT MUX

SR3, SL1

BYPASS NETWORK

Figure 11: Integer/Mantissa Datapath 6 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The Logical Operation unit performs all integer logical operations. The carry-pr opagated adder is used for all other integer and floating-point computational instr uctions. The adder is also used to compute data virtual addr ess for load and stor e instr uctions, and to compar e two operands in trap instr uctions. The shifter is r esponsible for integer variable shifts, stor e align shifts, and floating-point post-normalization. It also has build-in guar d/r ound/ sticky collection logic for floating-point pr e-alignment shift. In addition, the datapath has a Leading Zer o Counter for floating-point normalization shift calculation, and a floating-point unpacker and r epacker .

For load and stor e class instr uctions, the datapath can handle partial-wor ds in either big- or little-endian mode. For stor e instr uctions, the main bi-dir ectional shifter performs an alignment shift on the r egister r ead data. No concatenation of r egister r ead data with the original memory data is necessary since the data cache has byte write enable contr ols. For load instr uctions, it is necessary to maintain a load delay of one pclock cycle. Due to the timing r equir ements imposed by this load delay , a dedicated byte-wide shifter (Load Aligner) is needed to shift the memory r ead data in bytes, halfwor ds, and wor ds in the right or left dir ection.

The operand bypass network is built into the datapath to allow feedback of r esults fr om the EX and DC pipestage to the instr uctions in the following EX pipestage waiting to use the r esults as sour ce operands rs and/or rt. This allows the following instr uction to pr oceed without having to wait for the r esults to be written back to the r egister file. Similarly, to maintain the minimum branch delay slot of one pipeline clock cycle for all branch instr uctions on the floating-point condition, the r esults fr om the pr eceding floating-point compar e instr uction in the EX, DC, or WB pipestage will be fed back for branch condition testing in the RF pipestage.

The exponent datapath is 12 bits wide. The twelfth bit (MSB) is used as both sign bit and overflow bit. The exponent datapath consists of a feedback mux and 2 operand muxes to select the inputs fr om the adder , constant generating logic, a carry select adder , random logic to perform exception detection, and a r egister to hold the selected r esult fr om the adder , as shown in Figur e 12.

The inputs to the exponent unit come fr om the unpack logic, wher e the exponents ar e extracted fr om single- or double-pr ecision floating-point operands. The carryselected adder performs exponent subtraction, pr ealignment shift calculation, and exponent addition for post-normalization final update. The r esult is sent to the repack logic to be mer ged with the mantissa.

The result of the exponent logic is compar ed with constants or ranges to check for various conditions by the result checker . These conditions include: underflow , overflow in single-pr ecision number , overflow in doubleprecision number , one, zer o, and convert limit check. The checks ar e performed as soon as data is available fr om the carry-select adder .

The instr uction virtual addr ess unit is r esponsible for the generation of 64-bit instr uction virtual addr esses to be used by the micr o-TLB, I-Cache and CP0. It has its own incrementor to calculate the next sequential addr ess. It also has an equality comparator and a separate ripple-carry adder to generate the branch tar get addr ess.

In addition, the addr ess unit has exception vector generator logic to decode the type of exception and then present the appr opriate vector as the next PC addr ess. It also has the exception PC r egister pipe chain to maintain a history of PC addr esses for each pipestage so that the PC addr ess associated with the exception causing instr uction can be loaded into the Exception Pr ogram Counter (EPC) register .

CACHE ORGANIZA TION

To achieve high performance, incr ease memory access bandwidth and r educe the latency of load and stor e instr uctions, the R4300 pr ocessor incorporates on-chip instr uction and data caches. Each cache has its own 64-bit datapath and can be accessed in parallel with the other

FEEDBACK MUX

ES MUX

CARRY-SELECT ADDER

ET MUX S T

EXPONENTS FROM

UNPACKER UnpExpS UnpExpT

Leading Zero Cnt

RESULT MUX

Cin=1 Cin=0

EXP SUM REG TO REPACK LOGIC

Result Check

SR1 0 1 Constant Gen

Underflow Overflow One Zero > One Convert Limit Chk

Figure 12: Exponent Datapath

7 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

cache. Both the instr uction and data caches ar e dir ect mapped, virtually indexed, and use physical tags. Ther e is no mechanism for external manipulation of the caches and no on-chip support for second level cache. The R4300 cache organization is shown in Figur e 13.

The instr uction cache is 16 kilobytes in size. It is organized as eight-wor d (32-byte) lines with a 23-bit tag entry associated with each line. The tag entry consists of one bit tag parity (P), a valid bit (V), and a 21-bit physical tag (bit 32:12 of the physical addr ess). The format of an instr uction cache line is shown in Figur e 14.

An instr uction cache line has two possible cache states: Invalid and V alid. A cache line with invalid cache state does not contain valid information. A cache line in a valid state contains valid information.

The instr uction cache is accessible in one p-cycle. Access begins on phase 2 of the IC pipestage and completes at the end of phase 1 of the RF pipestage. Each access will fetch two instr uctions. Ther efore instr uction fetching is requir ed only on every other r un cycle or when ther e is a jump/branch instr uction in the EX pipestage. When ther e

Figure 13: R4300 Cache Organization

I-Cache D-Cache

Data-Path/

Flush-Buffer

SysAD Output Data Path

Control

SysAD Input

Data Path

SysAD Input

Data Path

PAD Ring

ESysAD Bus

DSysAD Bus ISysAD Bus

Cache Cntl

DTAG ITAG

DBus IBus

64 64

64 64

64

Figure 14: R4300 Instruction Cache Line Format

0 20 21 22

21 1 1 Physical T AG

P V P Data

P Data

P Data

P Data

0 31 32 35

32 4

P Data

P Data

P Data

P Data

wher e:

P Word Parity for tag and byte parity for data. V Valid bit PTAG 21 bit physical tag (bit 32:12 of the physical addr ess) Data Data wor d

is a miss detected during an instr uction cache access, a memory block r ead will be initiated fr om the system interface to r eplace the curr ent cache line with the desir ed line.

The data cache is 8 kilobytes in size. It is or ganized as four-wor d (16-byte) lines with a 24-bit tag entry associated with each line.The tag entry consists of one bit tag parity (P), a valid bit (V), a dirty bit (D), and a 21 bit physical tag (bit 32:12 of the physical addr ess). The format of a data cache line is shown in Figur e 15.

A data cache line has thr ee possible cache states: invalid, valid clean, and valid dirty . A data cache line with an invalid state does not contain valid information. A cache line in valid clean state contains valid information and is consistent with main memory . A cache line in valid dirty state contains valid data but is not consistent with main memory . Figur e 16 illustrates the data cache state transition sequence.

The data cache uses write-back write policy . This means that stor e data is written to the cache line rather than main memory . The modified cache line will be written back to main memory only when it needs to be r eplaced. For load or stor e misses, a cache block r ead will be issued to main memory to bring in a new line and the missed line will be handled in the following manner:

Data load miss:

• If the missed line is not dirty , it will be r eplaced with the new line.

• If the missed line is dirty , the missed line will be moved to the flush-buf fer, the new line will replaced the missed line, and the data in the flushbuffer will be written back to main memory .

Figure 15: R4300 Data Cache Line Format

0 20 21 22

21 1 1 Physical T AG

P V P Data

P Data

P Data

P Data

0 31 32 35

32 4

D 23

wher e:

P Word Parity for tag and byte parity for data. V Valid bit D Dirty bit PTAG 21 bit physical tag (bit 32:12 of the physical addr ess) Data Data wor d

Figure 16: R4300 Data Cache State Transition

Invalid

Clean

Valid

Read

Store Read

Read Miss

Store

Read Hit,

Store.

Cache-op

Cache-op

Cache-op

Valid Dirty

8 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Data stor e miss:

• If the missed line is not dirty , it will be r eplaced with the new line.

• If the missed line is dirty , the missed line will be moved to the flush-buf fer, the new line will be merged with the stor e data and written to the cache, and the data in the flush-buf fer will be written back to main memory .

The data cache is accessible on r eads in one p-cycle. The access begins on phase 1 of the DC pipestage and completes at the end of phase 2 of the DC pipestage. Each access will fetch a double wor d. The data cache writes, however , execute in two p-cycles. A cache r ead is initiated in the first p-cycle, and a cache write with dirty bit set is initiated in the second p-cycle.

The data cache can be accessed for byte, half-wor d, three-byte, wor d, five-byte, six-byte, seven-byte, and double-wor d. The data size of a partial load is derived fr om the access type fr om the integer contr ol unit and the lower three addr ess bits. The data alignment is performed by the datapath load aligner .

To reduce the cache miss penalty , the addr ess of the block r ead r equest will point to location of the desir ed double-wor d. Since the data cache has a two double-wor d line size, the system interface will r eturn the critical double-wor d first, followed by the r emaining doublewor d. The r eturn data will be written to the cache as it is put on the data bus to be used by the execution unit.

The instr uction and data caches’ data RAMs ar e byte parity pr otected and the tag RAMs ar e wor d parity protected. For the data cache tag RAM, the dirty bit is not included in the parity checking or generation. Parity is checked against its r espective cache data for err ors on every cache r ead access.

During a cache r efill, a cache err or will also be r eported if the system interface pr ovides data with bad parity and parity check enabled, or an err oneous data indicator is set in SysCmd bus bit 5.

A cache err or exception is taken if a parity err or is detected during an instr uction cache access, a data cache access, or memory r ead access. When this occurs, the CacheErr r egister will be updated with information pointing to the sour ce of the err or.

The R4300 pr ocessor pr ovides a variety of cache operations for use in maintaining the state and contents of the instr uction and data caches. During the execution of the cache operation instr uctions, the pr ocessor may issue processor block r ead or write r equest to fill or write-back a cache line. T able 12 lists all cache operations supported by the R4300 pr ocessor.

FLUSH BUFFER

The R4300 pr ocessor contains an on-chip flush buf fer. This buf fer is used as a temporary data storage for outgoing data. It is capable of taking one double-wor d per pcycle. The flush buf fer is four wor ds wide, equal to data cache line size. It is capable of taking one memory r eference at a time. The format of the flush buf fer is shown in Figur e

17.

The read/write size indicator specifies the size of data to be transferr ed out. The r ead/write addr ess field pr ovide a 33 bits physical addr ess, zer o-extended to 64 bits. The data field holds the four wor ds of data. Both the addr ess and data fields ar e byte parity pr otected.

For uncached stor es, the stor e data will be held in the buffer until it is taken by the external interface. For a load or stor e miss to a cache line in dirty state, the dirty line will be moved to the flush buf fer while the pr ocessor is waiting for the data for line r efill. After r eceiving the data, the flush buffer transfers write data to the external interface.

If the flush buf fer is full and the pr ocessor attempts a load or a stor e which r equir es external r esour ces, the processor will stall until this buf fer is empty .

COPROCESSOR-0

The R4300 Copr ocessor -0 functional unit performs two major functions. The first is memory management for the processor, and the second is exception pr ocessing. CP0 is logically divided into four subunits: CP0 Register Files (Cp0reg), Translation Look-aside Buf fer (TLB), Instr uction TLB (ITLB), and CP0 Contr ol Unit (Cp0ctl). Figur e 18 shows how these subunits interact with each other and other functional units.

Figure 17: Flush Buffer Format

P Read Address 0 63 64 71

64 8 P Write Address

P Data 0 63 64 71

64 8 P Data RZ WZ 5 wher e:

RZ Read Size WZ Write Size

P Byte parity for both r ead/write addr ess and data

Figure 18: R4300 Coprocessor-0 Block Diagram

ITLB

TLB

CP0REG

CP0CTL

IVA DVA

INDEX ENHI ENLO

TLBMISS

ADDR CHK

TAD DATA

I-PFN

D-PFN

EXCEPTIONS

STATUS

DBUS

CACHE DATA

INTERRUPTS

9 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The CP0 r egisters consist of two functionally distinct sets. The first set comprises those that support the TLB operations, and the second set is formed fr om those registers that r eflect the state of the pr ocessor. All of the CP0 registers ar e readable by softwar e. All but the Random, BadV Addr , PrId, CacheErr and MskId r egisters are writable by softwar e. The definitions of the CP0 registers ar e described in a later section.

The CP0ctl subunit contr ols data transfer to and fr om the TLB, ITLB and CP0 r egisters. It takes the instr uction decode signals fr om the integer unit and interpr ets them to determine whether a CP0 r egister is to be r ead or written. It generates contr ol signals for r eading and writing TLB and ITLB entries.

In addition, the CP0ctl handles exception pr ocessing. Its function is to communicate with the pipeline contr ol unit for interr upt signalling, and notification of TLB exceptions. It also performs addr ess checking with r egard to the type of instr uction being executed, and various state bits in the Status r egister . For example, a User mode process may try to access a kernel data addr ess. In this case, a Data Addr ess Err or exception would be detected, since the addr ess Region bits would conflict with the KSU bits in the Status r egister .

The Translation Look-aside Buf fers (micr o-TLB and joint TLB) are responsible for the translation of both instr uction and data virtual addr esses into physical addr esses. The physical addr ess is needed by the cache for its tag checks, and by the system interface for of f-chip memory access, and various CP0 r egisters. The jTLB translates the lower 40 bits of the 64-bit virtual addr ess size defined in the MIPS-III ar chitectur e, and pr ovides a 33-bit physical addr ess.

The joint TLB contains 32 entries, each of which is simultaneously checked for a match with the extended virtual addr ess. Each TLB entry maps an even-odd pair of pages. The page size is 4K, 16K, 64K, 256K, 1M, 4M or 16M bytes, which is specified on a per -entry basis by the MASK bit-mask field of the entry . The valid values of the MASK field and the ef fect on the translation is documented in the description of the PageMask Register .

A virtual addr ess matches a TLB entry when the virtual page number (VPN) field of the virtual addr ess equals the VPN field of the TLB entry , and either the Global (G) bit of the TLB entry is set or the addr ess space identifier (ASID) field of the virtual addr ess (as held in the EntryHi register) matches the ASID field of the TLB entry . Although the valid (V) bit of the entry must be set for a valid translation to take place, it is not involved in the determination of a matching TLB entry .

The operation of the TLB is not defined if mor e than one entry in the TLB matches. If one TLB entry matches, the physical addr ess and access contr ol bits (N, D, and V) are retrieved; otherwise a TLB r efill exception occurs. If the access contr ol bits (D and V) indicate that the access is not valid, a TLB modification or TLB invalid exception occurs.

The format of a TLB entry in 32-bit addr essing mode is shown in Figur e 19. The format of a TLB entry in 64-bit mode is shown in Figur e 20.

The R4300 also implements a two entry micr o-TLB that is dedicated for instr uction addr ess translation. This allows instr uction addr ess translation to be done simultaneously with data addr ess translation. If ther e is a miss in the micro-TLB, the pipeline will stall while the new TLB entry is transferr ed from the joint TLB to the micr o-TLB. The two entry micr o-TLB entry is fully associative with a Least Recently Used r eplacement algorithm. Each micr o-TLB entry maps to a 4K byte page size only .

CP0 REGISTERS

The following table lists all CP0 r egisters used in the R4300. Attempting to write any unused r egister is undefined and may have an unpr edictable ef fect on the R4300 processor. Attempting to r ead any unused r egister is undefined and may r esult in unpr edictable data.

Table 1: System Contr ol Copr ocessor-0 Registers

Num Mnemonic Descriptions

0 Index Programmable pointer into TLB entry 1 Random Random pointer into TLB array 2 EntryLo0 Low half of the TLB entry for even VPN 3 EntryHi Low half of the TLB entry for odd VPN 4 Context Pointer to kernel PTE table

Figure 19: TLB Entry Format in 32-bit Addressing Mode

31 27 26 6 2 1 0 3 5

127 121 120 108 96 109

63 59 58 38 34 33 32 35 37

MASK - - 95 72 71 64 75 76 77 VPN2 G ASID -

- PFN (even) C D V -

- PFN (odd) C D V -_{1113} 21 5

1 1 1 3 21 5

8 4 1 19

13 12 7

Figure 20: TLB Entry Format in 64-bit Addressing Mode

MASK - -

VPN2 G ASID -

- PFN (even) C D V -

- PFN (odd) C D V -

192 204 205 216 217 255

128 135 136 139 140 141 167 189 168 R 190 191

64 65 66 67 69 70 90 91 127

0 1 2 3 56 26 27 63 1 1 1 3 21 37

1 1 1 3 21 37

8 4 1 22 27 2

39 12 13

Wher e:

R Is the Region used to match V Addr 63..62 MASK is the comparison MASK VPN2 is the Virtual Page Number / 2

G Global bit ASID Addr ess Space Identifier PFN Physical Page Number (upper 21 bits of the physical addr ess) C Cache Algorithm (01 1=cached; 010=uncached) D If set, page is writable V If set, entry is valid

10 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The Index r egister is a r ead/write r egister in which 6 bits specify an entry into the on-chip TLB. The high or der bit indicates the success or failur e of a TLBP operation. The TLB Index r egister is used to specify the entry in the TLB affected by the TLBR and TLBWI instr uctions. Figur e 21 shows the Index r egister format.

The Random r egister is a r ead-only r egister in which 6 bits specify an entry in the on-chip TLB. This r egister will decrement on every instr uction executed. The values range between a low value determined by the TLB W ired register , and an upper bound of TLBENTRIES-1. The TLB Random register is used to specify the entry in the TLB af fected by the TLBWR instr uction. Upon system r eset, or when the Wired register is written, this r egister will be set to the upper limit. Figur e 22 shows the Random r egister format.

The EntryLo0 and EntryLo1 r egisters ar e a read/write register that ar e used to access on-chip TLB. EntryLo0 is for the even virtual pages while EntryLo1 is for the odd virtual

5 PageMask TLB page mask 6 Wired Number of wir e TLB entries 7 ---- Unused 8 BadVAddr Bad virtual addr ess 9 Count Timer count 10 EntryHi High half of TLB entry 11 Compar e Timer compar e 12 SR Status r egister 13 Cause Cause r egister 14 EPC Exception pr ogram counter 15 PRid Processor r evision identifier 16 Config Configuration r egister 17 LLAddr Load linked addr ess 18 WatchLo Memory r eference trap addr ess lower bits 19 WatchHi Memory r eference trap addr ess upper bits 20 XContext Context r egister for MIPS-III addr essing 21-25 ---- Unused 26 PErr Parity err or in cache 27 CacheErr Cache err or and status r egister 28 TagLo Cache tag r egister 29 TagHi Cache tag r egister (Reserved) 30 ErrorEPC Error exception pr ogram counter 31 ---- Unused

Table 1: System Contr ol Copr ocessor-0 Registers

31 30 6 5 0

Figure 21: CP0 Index Register

Index 0 P 6 25 1 wher e:

P Result of last Pr obe operation. Set to 1 if last TLB Pr obe instr uction was unsuccessful.

index Index to entry in TLB

0 Must be all zer oes on r eads and writes

31 6 5 0

Figure 22: CP0 Random Register

Random 0 6 26 wher e:

Random Index to entry in TLB

0 Must be all zer oes on r eads and writes

pages. They contain the Page Frame Number , along with several configuration bits for the TLB entry . They ar e used by the TLBR, TLBWI, and TLBWR instr uctions. Figur e 23 shows the EntryLo0 and EntryLo1 r egisters format.

The Context r egister is a r ead/write r egister containing a pointer into a kernel Page T able Entry (PTE) array . It is designed for use in the TLB r efill handler . The BadVPN2 field is not writable. It contains the VPN of the most recently translated virtual addr ess that did not have a valid translation. It contains bits 31.13 of the virtual addr ess that caused the TLB miss. Bit 12 is excluded because a single TLB entry maps an even-odd page pair . This format can be used dir ectly as an addr ess for pages of size 4K bytes. For pages of 16M bytes, this value must be shifted and masked. The PTEBase field is writable as well as r eadable, and indicates the base addr ess of the PTE table of the curr ent user addr ess space. 24 shows the Context r egister format..

The PageMask r egister is a r ead/write r egister that is used when r eading or writing an on-chip TLB. The TLBR, TLBWI, and TLBWR instr uctions use this r egister as a sour ce or destination.When virtual addr esses ar e presented for translation, the corr esponding bits in the TLB specify which of virtual addr ess bits 24.13 participate in the comparison. This implements a variable page size on a per entry basis. R4300 implements 4K, 16K, 64K, 256K, 1M, 4M and 16M pages. Figur e 25 shows the PageMask r egister format..

31 30 6 5 0

Figure 23: CP0 EntryLo0 and EntryLo1 Registers

C PFN 0 3 24 2

wher e:

PFN Physical Frame Number

C Cache Algorithm. If C=01 1, then page is cached. If C=010, then it is uncached. All other values of C ar e cached.

V Page Valid if 1, invalid if 0 G If set in both Lo0 and Lo1, then ignor e ASID 0 Must be zer o on all r eads and writes D Page Dirty if 1, Clean if 0

29 D V G

1 1 1

1 2 3

31 30 6 5 0 C PFN 0 3 24 2

29 D V G

1 1 1

1 2 3

32 bit Mode:

64 bit Mode:

31 23 4 0

Figure 24: CP0 Context Register

BadVPN2 PTEBase 4 19 9

wher e:

PTEBase Base addr ess of the Page Entry T able BadVPN2 Virtual Page Number of the failed virtual addr ess divided by two 0 Must be zer o on r eads and writes

3 32 bit Mode:

64 bit Mode:

22 0

63 23 4 0

BadVPN2

PTEBase 4 19 41

3 22 0

11 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The TLB Wired register is a r ead/write r egister that specifies the boundary between the wir ed and random entries of the TLB. This r egister is set to 0 upon r eset. Writing to this r egister also sets the Random r egister to 31. Writing a value gr eater than TLBENTRIES-1 to this r egister will result in undefined behavior . Figur e 26 shows the Wired register format.

The Bad Virtual Addr ess register is a r ead-only r egister that displays the most r ecently translated virtual addr ess which failed to have a valid translation or which had an addr essing err or. Figur e 27 shows the BadV Addr r egister format.

The Count r egister is a r ead/write r egister used to implement timer services. It incr ements at a constant rate based on the clock cycle. On R4300, it will incr ement at one-half the PClock speed. When the Count r egister has reached all ones, it will r oll over to all zer oes and continue counting. This r egister is both r eadable and writable. It is writable for diagnostic purposes. Figur e 28 shows the Count r egister format..

The EntryHi Register is a r ead/write r egister that is used to access on-chip TLB. It is used by the TLBR, TLBWI, and TLBWR instr uctions. EntryHi contains the Addr ess Space Identifier (ASID) and the V irtual Page Number . Figur e 29 shows the EntryHi r egister format.

The Compar e register is a r ead/write r egister . When the value of the Count Register equals the value of the

31 25 13 0

Figure 25: CP0 Mask Register

MASK 0 13 12 7 wher e:

MASK Mask for V irtual Page Number . For R4300, this is 000000000000 for 4K pages, 00000000001 1 for 16K pages and so on up to 1 11111111111 for 16M pages.

0 Must be zer o on r eads and writes

12 24 0

31 6 0

Figure 26: CP0 Wired Register

0 6 26 wher e:

Wired TLB wired boundary

0 Must be zer o on r eads and writes

5 Wired

31 0

Figure 27: CP0 BadVAddr Register

BadVAddr 32

wher e: BadVAddr Most r ecently translated virtual addr ess that failed to have a valid translation or that had an addr essing error.

32 bit Mode:

64 bit Mode:

63 0

BadVAddr 64

Compar e register , IP_7 of the Cause r egister is set. This causes an interr upt on the next execution cycle in which interr upt is enabled. W riting to the Compar e register will clear the timer interr upt. Figur e 30 shows the Compar e register format.

The Status r egister is a r ead/write r egister that contains the various mode, enables, and status bits used on R4300. The contents of this r egister ar e undefined after a reset, except for TS, which is zer o; ERL and BEV, which ar e one; and RP , which is zer o. The SR bit is 0 after a Cold Reset, and 1 after NMI or (Soft) Reset. Figur e 31 shows the Status r egister format.

The Cause r egister is a r ead/write r egister that describes the natur e of the last exception. A five bit exception code indicates the cause of the exception and the remaining fields contain detailed information r elevant to the handling of certain types of exceptions. The Branch Delay bit indicates whether the EPC has been adjusted to point at the branch instr uction which pr ecedes the next restartable instr uction. The Copr ocessor Err or field indicates the unit number r eferenced by an instr uction causing a “Copr ocessor Unusable” exception. The Interr upt Pending field indicates which interr upts ar e pending. This field indicates the curr ent status and changes in response to external signals. IP7 is the timer interr upt bit, set when the Count r egister equals the Compar e

31 0

Figure 28: CP0 Count Register

32 wher e:

Count Constantly updating count value to be compar ed to the Compar e register .

Count

31 8 0

Figure 29: CP0 EntryHi Register

VPN2 8 19

wher e:

R Region (00=user , 01=supervisor ,11=kernal) used to match vAddr 63..62 FILL Reserved; undefined on r ead, should be 0 or -1 on write (should sign extend the virtual page number) VPN2 Virtual Page Number divided by 2

0 Must be zer o on r eads and writes ASID Addr ess Space Identifier

7 32 bit Mode:

64 bit Mode: 0 12 13 ASID 5 63 8 0

VPN2 8 27

7 0 12 13 ASID 5

62 61 40 39

2 22

FILL R

31 0

Figure 30: CP0 Compare Registers

32 wher e: Compar e Value to be compar ed to Count r egister . An interr upt will be signaled when they ar e equal.

Compare

12 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

register . IP6.2 are the external interr upts, set when the external interr upts ar e signalled. An external interr upt is set at one of the external interr upt pins or via a write request on the SysAD bus. IP1.0 ar e softwar e interr upts, and may be written to set or clear softwar e interr upts. Figur e 32 shows the Cause r egister format.

The EPC r egister is a r ead/write r egister that contains the addr ess at which instr uction pr ocessing may r esume after servicing an exception. For synchr onous exceptions, the EPC r egister contains either the virtual addr ess of the instr uction which was the dir ect cause of the exception, or when that instr uction is in a branch delay slot, the EPC contains the virtual addr ess of the immediately pr eceding branch or jump instr uction and the Branch Delay bit in the Cause r egister is set. If the exception is caused by recoverable, temporary conditions (such as a TLB miss), the EPC contains the virtual addr ess of the instr uction which caused the exception. Thus, after corr ecting the conditions, the EPC contains a point at which execution can be legitimately r esumed. Figur e 33 shows the format of EPC regsiter .

The PRId r egister is a r ead-only r egister that contains information that identifies the implementation and revision level of the pr ocessor and associated system contr ol copr ocessor. The revision number can distinguish some chip r evisions. However , MIPS is free to change this register at any time and does not guarantee that changes to its chips will necessarily change the r evision number , or

31 28

Figure 31: CP0 Status Register

CU 1 4

wher e:

CU Copr ocessor Unit usable if 1. CP0 is always usable by the kernel RP Reduced Power . Changes clock to quarter speed. FR If set, enables MIPS III additional floating point registers.

RE Reverse Endian. Changes endianess in user mode. ITS Instr uction Trace Support. Enables trace support. rsvd Reserved for futur e use. BEV Contr ols location of TLB r efill and general exception vectors. (0=normal, 1= bootstrap). Also af fects Cache Error exceptions.

TS TLB Shutdown has occurr ed. This happens to avoid destr uctive drive fights in the TLB if multiple hits occur. Once TLB shutdown has occurr ed, the pr ocessor must be r eset to r estor e TLB functionality .

SR Soft Reset or NMI has occurr ed. 0 Must be zer oes on r ead and write.

CH This is the CP0 Condition bit. It is r eadable and writable by softwar e only. It is not set or clear ed by hardwar e.

CE If set, contents of PErr r egister ar e used to set parity bits in cache. The tag parity bit will be written fr om the TagLo parity bit.

DE if set, cache parity err ors will not cause exceptions IM Interr upt Mask. Enables and disables interr upts. KX Kernel extended addr essing enabled. SX Supervisor extended addr essing enabled. UX User extended addr essing enabled. KSU Mode (10=user , 01=supervisor , 00=kernel) ERL Error Level. Normal when zer o, error if one EXL Exception Level. Normal when zer o, exception if one IE Interr upt Enable.

1 1 1

RP FR RE ITS rsvd BEV TS SR 0 CH CE DE

27 26 25 24 23 22 21 20 19 18 17 16 1 1 1 1 1 1 1 1 15 IM 2 1 1 1

KX SX UX KSU ERLEXL IE

8 7 6 5 4 3 2 1 0

1 1 1 8

that changes to the r evision number necessarily r eflect r eal chip changes. For this r eason, softwar e should not r ely on the r evision number to characterize the chip. Figur e 34 shows the Revision Identifier r egister format.

The Config r egister specifies various configuration options that ar e available for R4300. It is compatible with the R4000 Config r egister , but only a small subset of the options available on the R4000 ar e possible on R4300. For that r eason, ther e are many fields which ar e set to constant

Figure 32: CP0 Cause Register

wher e:

BD Branch Delay CE Copr ocessor Err or IP Interr upt pending ExcCode Exception Code: 0 Int Interr upt 1 Mod TLB modification exception 2 TLBL TLB Exception (Load or instr uction fetch) 3 TLBS TLB Exception (Stor e) 4 AdEL Addr ess Err or Exception (Load or instr uction fetch) 5 AdES Addr ess Err or Exception (Stor e) 6 IBE Bus Error Exception (instr uction fetch) 7 DBE Bus Error Exception (data r eference: load or stor e) 8 Sys SysCall Exception 9 Bp Breakpoint Exception 10 RI Reserved instr uction Exception 11 CpU Copr ocessor Unusable Exception 12 Ov Arithmetic Overflow Exception 13 Tr Trap Exception 14 --- Reserved 15 FPE Floating Point Exception 16-22 Reserved 23 Watch Reference to W atchHi/W atchLo addr ess 24-31 Reserved 0 Must be zer oes on r ead and write

31 0 2 51 2

IP ExcCode 0

8 7 6 2 1 0

1 1 12 0 BD CE 0 29 28 16 15 27 30

8

31 0

Figure 33: CP0 EPC Register

EPC 32

wher e:

EPC Exception Pr ogram Counter .

32 bit Mode:

64 bit Mode:

63 0 EPC 64

31 0

Figure 34: CP0 Revision Identifier Register

16 wher e:

Imp Implementation identifier: 0x0A for R4200 Rev Revision Number

0 Returns zer oes on r eads.

0 Imp Rev 78 15 16

8 8

13 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

values. The EP and BE fields ar e written by har dwar e during Reset. Softwar e only has r ead access to these fields. The CU and K0 fields ar e readable and writable by softwar e. There is no other mechanism for writing to these fields, and their values ar e undefined after Reset. Figur e 35 shows the Configuration r egister format.

The LLAddr r egister contains the physical addr ess read by the most r ecent Load Linked instr uction. This register exists for diagnostic purposes, and serves no function during normal operation. It is both r eadable and writable by softwar e. Figur e 36 shows the LLAddr r egister format.

The R4300 pr ocessor pr ovides a debugging featur e to detect r eferences to a physical addr ess. Loads or stor es to the location specified by the W atchHi/W atchLo r egister pair cause a W atch trap. Figur e 37 shows W atchHi/ WatchLo r egister formats.

31 28

Figure 35: CP0 Configuration Register

EP 1 4 wher e:

EP Pattern for writeback data on SYSAD port

0001 -> DDx 0110 -> DxxDxx All other values of EP ar e undefined.

BE BigEndianMem

0 -> Memory and kernel ar e Little Endian 1 -> Memory and kernel ar e Big Endian CU Reserved. (Read- and W rit-able by softwar e) K0 Kseg0 coher ency algorithm. This has the same format as the C field in EntryLo0 and EntryLo1. The only defined values for K0 for R4300 ar e 010 (noncacheable) and 011 (cacheable).

0 Returns 0 on r ead. 1 Returns1 on r ead.

1 3 00 0 BE 0 010 001 1 0 CU K0

27 20

24 23 8 6 5 4 3 2 0

1 2 4 4 1 1 1 1 1 0 19 18 17 15 16

14

9 11 12 13 14 1 1 0 1 1 3 3

31 0

Figure 36: CP0 LLAddr Register

wher e:

Paddr Bits 35..4 of the physical addr ess. Note that for R4200, the MSB of the physical addr ess is only 32. A load linked instr uction will write 0 into bits[31..29] of LLAddr , but a softwar e write can set all 32 bits to any value. This maintains compatibility with R4000.

PAddr

31 0

Figure 37: CP0 WatchLo and WatchHi Registers

wher e:

PAddr Physical addr ess WatchLo PAddr contains bits 31.3 WatchHi P Addr contains bit 32.

R Trap on Read Access if 1 W Trap on W rite Access if 1 0 Must be zer oes on r eads and writes

PAddr

31 0 31 PAddr 1 0

WatchLo:

WatchHi: W R 1 0 1 2 3 1 1 29

1

The XContext r egister is a r ead/write r egister containing a pointer into a kernel Page T able Entry (PTE) array. It is designed for use in the XTLB r efill handler . The R and BadVPN2 fields ar e not writable. The r egister contains the VPN of the most r ecently translated virtual addr ess that did not have a valid translation. It contains bits 39.13 of the virtual addr ess that caused the TLB miss. Bit 12 is excluded because a single TLB entry maps an even-odd page pair . This format can be used dir ectly as an addr ess for pages of size 4K bytes. For pages of 16M bytes, this value must be shifted and masked. The PTEBase field is writable as well as r eadable, and indicates the base addr ess of the PTE table of the curr ent user addr ess space. Figur e 38 shows XContext r egister format.

The PErr r egister is used to r ead or write the parity bits of the cache. It can be used for initialization, cache diagnostics, or cache err or handling. The r egister is loaded from the cache array via the Cache operation Index Load Tag.The PErr r egister is substituted for the computed parity on stor es if the CE bit of the Status r egister is set. PErr is also substituted for the computed parity on the Cache operation Fill if the CE bit is set. Figur e 39 shows PErr r egister format.

CacheErr is a 32-bit r ead-only r egister for corr ecting and logging parity err ors in the cache. The r egister provides the cache index and status bits indicating the sour ce and natur e of the err or. It is loaded when a Cache Error exception is taken. Figur e 40 shows CacheErr r egister format.

The TagLo r egister is a 32-bit r ead/write r egister used to hold the cache tag and parity during cache initialization, cache diagnostics, or cache err or handling. On the cache operation Index Stor e Tag, the PT agLo and PState bits ar e written into the cache. If the CE bit is set in the status register , the parity bit will be written into the cache tag from the T agLo r egister . If the CE bit is clear ed, parity will be recomputed for the tag. During the cache operation Fill, the parity bit fr om the T agLo will be written into the cache tag if the CE bit is set. The T agHi r egister is r eserved for

63 4 0

Figure 38: CP0 XContext Register

BadVPN2

PTEBase 27 31 wher e:

PTEBase Base addr ess of the Page Entry T able BadVPN2 Virtual Page Number of the failed virtual addr ess divided by two R Region (00=user , 01=supervisor , 11=kernel) 0 Must be zer o on r eads and writes

3 0 R 30 31 32 33

4 2

31 8 0

Figure 39: CP0 PErr Register

0 8 24 wher e:

Parity Eight bit parity field

0 Must be zer oes on all r eads and writes

7 Parity

14 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

futur e use. The T ag registers ar e written by the CACHE and MTC0 instr uctions. Figur e 41 shows T agLo and T agHi register formats.

The Err orEPC r egister is similar to the EPC, but is used on parity err or exceptions. It is also used to stor e the PC on Reset and NMI exceptions. It is r ead/write and contains the virtual addr ess at which instr uction pr ocessing may resume after servicing an Err or or Reset/NMI exceptions. The EPC r egister contains either the virtual addr ess of the instr uction which was the dir ect cause of the exception, or when that instr uction is in a branch delay slot, the EPC contains the virtual addr ess of the immediately pr eceding branch or jump instr uction. Ther e is no branch delay slot indication for Err orEPC. Figur e 42 shows Err orEPC r egister format.

MEMOR Y MANAGEMENT

The R4300 pr ocessor pr ovides a full-featur ed memory management unit (MMU) which uses an on-chip translation look-aside buf fer (TLB) to translate virtual addr ess into physical addr ess. The TLB is a fully associative memory that holds 32 entries, which pr ovide

31 30

Figure 40: CP0 CacheErr Register

ER

wher e:

ER Type of r eference (0=instr uction, 1=data) ED Error in data field ET Error in tag field EE Error on the system bus EB Error in both Data and Instr uction caches; r equir es flushing the data cache after fixing the instr uction error.

PIdx Index into cache

ED 0 PIdx

29 26

28 27 0

1 1 1 14 1 ET 0 25 24 14 13

11 1 EE EB 0 1 1

31 0

Figure 41: CP0 TagLo TagHi Registers

wher e:

PTagLo Physical addr ess bits 32.12 Pstate Primary Cache State (0=invalid, 2=Clean, 3=Dirty) P Parity bit 0 Must be zer oes on r eads and writes

PTagLo

31 0 32 TagHi = 0

TagLo:

TagHi: P 0 1 0 1 5 21 29 28 3 6 5 PState 78 2

31 0

Figure 42: CP0 ErrorEPC Register

ErrorEPC 32

wher e: ErrorEPC Exception Pr ogram Counter for parity err ors or r esets.

32 bit Mode:

64 bit Mode:

63 0 Error EPC 64

mapping to 32 odd/even pairs (64 pages). When addr ess mapping is indicated, each TLB entry is checked simultaneously for a match with the virtual addr ess that is extended with an ASID stor ed in the EntryHi r egister . The addr ess is mapped to a page of size of between 4Kbytes and 16Mbytes.

The pr ocessor virtual addr ess can be either 32 or 64 bits wide, depending on whether the pr ocessor is operating in 32-bit or 64-bit mode.

• In 32-bit mode, addr esses ar e 32 bits wide. The maximum user pr ocess size is 2 gigabytes (2^{31}).

• In 64-bit mode, addr esses ar e 64 bits wide. The maximum user pr ocess size is 1 terabyte (2^{40}).

Figur e 43 shows the translation of a virtual addr ess into a physical addr ess.

Converting a virtual addr ess to a physical addr ess begins by comparing the virtual addr ess from the processor with the virtual addr ess in the TLB; ther e is a match when the virtual page number (VPN) of the addr ess is the same as the VPN field of the entry , and either:

• the Global ( G) bit of the TLB entry is set, or • the ASID field of the virtual addr ess is the same as the ASID field of the TLB entry .

This match is r eferred to as a TLB hit. If ther e is no match, a TLB Miss exception is taken by the pr ocessor and softwar e is allowed to r efill the TLB fr om a page table of virtual/physical addr esses in memory .

If ther e is a virtual addr ess match in the TLB, the physical addr ess is output fr om the TLB and concatenated with the Offset, which r epresents an addr ess within the page frame space.

Figur e 44 shows the virtual-to-physical addr ess translation of a 32-bit mode addr ess.

• The top portion of Figur e 44 shows a virtual addr ess with a 12-bit, or 4-Kbyte, page size, labelled Offset. The remaining 20 bits of the addr ess represent the VPN, and index the 1Mentry page table.

• The bottom portion of Figur e 44 shows a virtual addr ess with a 24-bit, or 16-Mbyte, page size, labelled Offset. The remaining 8 bits of the addr ess represent the VPN, and index the 256-

1. Virtual address (VA) represented

by the virtual page number (VPN) is compared with tag in TLB.

Virtual address

2. If there is a match, the page frame

number (PFN) representing the upper bits of the physical address (PA) is output from the TLB.

VPN

TLB

Physical address

Offset

TLB 3. The Offset, which does not pass

through the TLB, is then concatenated to the PFN.

Entry

Figure 43: Virtual-to-physical address translation

G ASID

VPN G ASID

EVEN PFN

ODD PFN

PFN Offset

15 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

entry page table.

Figur e 45 shows the virtual-to-physical-addr ess translation of a 64-bit mode addr ess. This figur e illustrates the two possible page sizes: a 4-Kbyte page (12 bits) and a 16-Mbyte page (24 bits).

• The top portion of Figure 45 shows a virtual addr ess with a 12-bit, or 4-Kbyte, page size, labelled Offset. The remaining 28 bits of the addr ess represent the VPN, and index the 256Mentry page table.

• The bottom portion of Figure 45 shows a virtual addr ess with a 24-bit, or 16-Mbyte, page size, labelled Offset. The remaining 16 bits of the addr ess represent the VPN, and index the 64Kentry page table.

The pr ocessor has thr ee operating modes that function in both 32- and 64-bit operations: User mode, Supervisor mode, and Kernel mode. The address space for each mode of operation are described in the following sections.

Figure 44: 32-bit-mode virtual address translation

28 11 0

20 12

29 31 32 39

8

Virtual Address with 1M (2 20) 4-Kbyte pages

23 0

8 24

Offset 39

Virtual Address with 256 (2 8)16-Mbyte pages

8 bits = 256 pages

20 bits = 1M pages 12

ASID 8 28 29 31 32 VPN 24

Virtual-to-physical translation in TLB

Bits 31, 30 and 29 of the virtual addr ess select user , supervisor , or kernel addr ess spaces.

Offset passed unchanged to physical memory

Virtual-to-physical translation in TLB

TLB

TLB 32 0 PFN Offset

Offset passed unchanged to physical memory

33-bit Physical Address

VPN Offset ASID

Figure 45: 64-bit-mode virtual address translation

11 0

12

63 VPN Offset 64 71 ASID 8

Mapped V irtual Address with 256M (2 28) 4-Kbyte pages

23 0

24 24

Offset

Virtual Address with 64K (2 16)16-Mbyte pages

16 bits = 64K pages

28 bits = 256M pages 12

ASID VPN

61 62 40 39

28 0 or -1

63 64 71 6162 40 24

8

39

16

24

0 or -1

Virtual-to-physical translation in TLB

Virtual-to-physical translation in TLB TLB 32 0

PFN Offset

TLB

Offset passed unchanged to physical

Offset passed unchanged physical memory

33-bit Physical Address

In User mode, a single, uniform virtual addr ess space—labelled User segment—is available; its size is:

• 2 Gbytes (2^{31} bytes) in 32-bit mode (useg) • 1 Tbyte (2^{40} bytes) in 64-bit mode (x useg)

The User segment starts at addr ess 0 and the curr ent active user pr ocess resides in either useg (in 32-bit mode) or xuseg (in 64-bit mode). The TLB identically maps all references to useg/ xuseg from all modes, and contr ols cache accessibility^1. Figure 46 shows User mode virtual address space.

The pr ocessor operates in User mode when the Status register contains the following bit-values:

• KSU bits = 10_2 • EXL= 0 • ERL= 0

In conjunction with these bits, the UX bit in the Status register selects between 32- or 64-bit User mode addr essing as follows:

• when UX = 0, 32-bit useg space is selected • when UX = 1, 64-bit xuseg space is selected

Supervisor mode is designed for layer ed operating systems in which a tr ue kernel r uns in R4300 Kernel mode, and the r est of the operating system r uns in Supervisor mode. Figure 47 shows Supervisor mode address space.

The pr ocessor operates in Supervisor mode when the Status register contains the following bit-values:

1. The cached (C) field in a TLB entry determines whether the r eference is cached; see Figur e 20.

Figure 46: User mode virtual address space useg xuseg

Address Error

1 TB Mapped

32-bit 64-bit

                        0xFFFFFFFFFFFFFFFF

                        0x0000000000000000

0xFFFFFFFF

0x80000000

0x00000000

                        0x00000100 0000

Address Error

Mapped

2 GB

0000

Figure 47: Supervisor mode virtual address space

2 GB Mapped

Mapped

suseg

Address

0.5 GB error

sseg

Address

error Address

error

Mapped

xsuseg

Address

0.5 GB error

xsseg

1 TB Mapped

Address error

32-bit 64-bit

                                        csseg

                          0xFFFFFFFFFFFFFFFF

                          0x4000010000000000

                          0x0000000000000000

                          0xFFFFFFFFE0000000

                          0xFFFFFFFFC0000000

                          0x4000000000000000

                          0x0000010000000000

0xFFFFFFFF

0x80000000

0x00000000

0xE0000000

0xC0000000

0xA0000000

Address error

1 TB Mapped

16 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

• KSU= 01_2 • EXL= 0 • ERL= 0

In conjunction with these bits, the S X bit in the Status register selects between 32- or 64-bit Supervisor mode addr essing:

• when SX = 0, 32-bit supervisor space is selected • when SX = 1, 64-bit supervisor space is selected

The pr ocessor operates in Kernel mode when the Status register contains one of the following values:

• KSU= 00_2 • EXL= 1 • ERL= 1

In conjunction with these bits, the KX bit in the Status register selects between 32- or 64-bit Kernel mode addr essing:

• when KX = 0, 32-bit kernel space is selected • when KX = 1, 64-bit kernel space is selected

The pr ocessor enters Kernel mode whenever an exception is detected and it r emains in Kernel mode until an Exception Return (ERET) instr uction is executed. The ERET instr uction r estor es the pr ocessor to the mode existing prior to the exception.

Kernel mode virtual address space is divided into regions differentiated by the high-order bits of the virtual address, as shown in Figure 48 .

EXCEPTION MANAGEMENT

The R4300 pr ocessor r eceives exceptions fr om a number of sour ces, including translation lookaside buf fer (TLB) misses, arithmetic overflows, I/O interr upts, and system calls. When the CPU detects one of these exceptions, the normal sequence of instr uction execution is suspended and the pr ocessor enters Kernel mode.

Figure 48: Kernel mode virtual address space

2 GB

0.5 GB

0.5 GB

Mapped

Mapped

Unmapped

Unmapped

kuseg
kseg0
kseg1

0.5 GB

0.5 GB

Mapped

ksseg
kseg3

Uncached

Cached

32-bit*

0xFFFFFFFF

0x80000000

0x00000000

0xE0000000

0xC0000000

0xA0000000

                                       xkuseg

                                       ckseg0

                                       ckseg1

                                       xksseg

                                       ckseg3

Mapped

0.5 GB

Mapped

0.5 GB

0.5 GB Unmapped Uncached

0.5 GB Unmapped Cacheable

Address

error

cksseg

1 TB Mapped

xkseg

Mapped

xkphys

64-bit

Address

error

0xFFFFFFFFFFFFFFFF

0x4000010000000000

0x0000000000000000

0xFFFFFFFFE0000000

0xFFFFFFFFC0000000

0x4000000000000000

0x0000010000000000

0x9000000000000000

0xC000000000000000

0xFFFFFFFFA0000000

0xFFFFFFFF80000000

0xC00000FF80000000

1 TB Mapped

0x9000000200000000^{Address}error

                   xkphys

Unmapped

Cached

0x9800000000000000

0x9800000200000000^{Address}error

Address

error

Unmapped Uncached

The pr ocessor then disables interr upts and for ces execution of a softwar e exception pr ocessor (called a handler) located at a fixed addr ess. The handler saves the context of the pr ocessor, including the contents of the program counter , the curr ent operating mode (User or Supervisor), and the status of the interr upts (enabled or disabled). This context is saved so it can be r estor ed when the exception has been serviced.

When an exception occurs, the CPU loads the Exception Program Counter (EPC) register with a location wher e execution can r estart after the exception has been serviced. The restart location in the EPC register is the addr ess of the instr uction that caused the exception or , if the instr uction was executing in a branch delay slot, the addr ess of the branch instr uction immediately pr eceding the delay slot.

The R4300 separates exceptions into five vector spaces: Reset and NMI vector , TLB Refill vector , XTLB Refill vector , Cache Err or, and General exception vector . The values of each vector (except Reset and NMI) depend on the Boot Exception V ector (BEV) bit of the Status r egister , which allow two alternate sets of vectors to be used, with one set pointing to the PROM addr ess space and the other set point to cacheable addr ess space.

The Reset and NMI exceptions ar e always vector ed to location 0xBFC0 0000 in 32-bit mode, and location 0xFFFF FFFF BFC0 0000 in 64-bit mode.

The addr esses for all other exceptions ar e a combination of a vector offset and a base address. The base addr ess is determined by the BEV bit of the Status r egister , as shows in T able 2. Table 3 shows the exception vectors for the dif ferent types of exceptions. The vector base addr ess for Cache Err or Exceptions is in uncached space for either value of BEV.

While mor e than one exception can occur for a single instr uction, only the exception with the highest priority is

Table 2: Exception V ector Base Addr esses BEV R4300 Processor Exception V ector Base

32-bit mode 64-bit mode

0 0x8000 0000 0xFFFF FFFF 8000 0000

1 0xBFC0 0200 0xFFFF FFFF BFC0 0200

0(Ca. Er.) 0xa000 0000 0xFFFF FFFF a000 0000

1(Ca. Er.) 0xBFC0 0200 0xFFFF FFFF BFC0 0200

Table 3: Exception V ectors

Excpt Type

Offset BEV

R4300 Processor Exception V ector

32-bit mode 64-bit mode TLB Refill 0x000

0 0x8000 0000 0xFFFF FFFF 8000 0000

1 0xBFC0 0200 0xFFFF FFFF BFC0 0200

XTLB Refill 0x080

0 0x8000 0080 0xFFFF FFFF 8000 0080

1 0xBFC0 0280 0xFFFF FFFF BFC0 0280

Cache Error 0x100

0 0xa000 0100 0xFFFF FFFF a000 0100

1 0xBFC0 0300 0xFFFF FFFF BFC0 0300 All Other 0x180

0 0x8000 0180 0xFFFF FFFF 8000 0180

1 0xBFC0 0380 0xFFFF FFFF BFC0 0380

17 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

reported. T able 4 lists all exceptions in the or der of their priority .

Exceptions ar e logically pr ecise (the pipeline exception DCPE in the WB stage is the only impr ecise exception); the instr uction that causes an exception and all those that follow it ar e aborted, generally befor e committing any state, and can be r e-executed after servicing the exception. When following instr uctions ar e killed, exceptions associated with those instr uctions ar e also killed, so that exceptions ar e not taken in the or der detected, but in instr uction fetch or der.

The exception handling system is r esponsible for efficiently handling r elatively infr equent events, such as translation misses, arithmetic overflow , I/O interr upts, and system calls. These events cause the interr uption of the normal flow of execution; aborting instr uctions which cause exceptional conditions and all those which follow and have alr eady begun executing, and a dir ect jump into a designated handler r outine.

The ar chitectur e defines a minimal amount of additional state which is saved in copr ocessor r egisters in order to facilitate the analysis of the cause of the exception, the servicing of the event which caused it, and the resumption of the original flow of execution, when applicable.

Table 4: Exception Priority Order

Reset (highest priority) NMI Addr ess Err or -- Instr uction fetch

TLB Refill -- Instr uction fetch

TLB Invalid -- Instr uction fetch

Cache Err or -- Instr uction fetch

Bus Error -- Instr uction fetch

System Call

Breakpoint

Copr ocessor Unusable

Reserved Instr uction

Trap Instr uction

Integer Overflow

Floating-point Exception

Addr ess Err or -- Data access

TLB Refill -- Data access

TLB Invalid -- Data access

TLB Modified -- Data write

Cache Err or -- Data access

Watch

Bus Error -- Data access

Interr upt

INTERF ACE SIGNALS

The pr ocessor interface signals allow the pr ocessor to access external r esour ces needed to satisfy cache misses and uncached operations, while permitting an external agent access to some of the pr ocessor internal r esour ces. The signals include the System interface, the Clock/ Contr ol interface, the Interr upt interface, the Joint T est Action Gr oup (JTAG) interface, and the Initialization interface. Figur e 49 illustrates the functional gr ouping of the pr ocessor signals.

The system interface signals pr ovide the connection between the R4300 pr ocessor and the other components in the system. It is compatible with the R4000 System interface. The system interface consists of: 64-bit addr ess and data bus with 8-bit check bus, 9-bit command bus with a parity bit, and six handshaking signals. T able 5 lists the system interface signals. Table 5: System Interface Signals

Name Direction Description

SysAD(63:0) Input/Output

A 64-bit addr ess and data bus for communication between the processor and an external agent.

SysADC(7:0) Input/Output An 8-bit bus containing check bits for the SysAD bus.

SysCmd(8:0) Input/Output

A 9-bit bus for command and data identifier transmission between the pr ocessor and an external agent.

SysCmdP Input/Output A single, even- parity bit for the SysCmd bus.

ValidIn* Input

The external agent asserts ValidIn *when it is driving a valid addr ess or data on the SysAD bus and a valid command or data identifier on the SysCmd bus.

ValidOut* Output

The pr ocessor asserts V alidOut* when it is driving a valid addr ess or data on the SysAD bus and a valid command or data identifier on the SysCmd bus.

Figure 49: R4300 System Interface Signals

SysAD(63:0) SysADC(7:0)

SysCmd(8:0) SysCmdP

ValidIn* ValidOut*

ExtRqst* Release*

WrRdy*

TClock RClock

MasterClock

MasterOut

SyncOut

SyncIn

ColdReset*

Reset*

Status(3:0)

Int*(4:0)

NMI*

JTDI JTDO JTMS JTCK

Initialization

Interface

Interrupt/Status

System Interface

R4200 Logic Symbol

9

RdRdy*

JTAG

8 64

Clock/Control Interface

BypassPLL*

DataRate*

BigEndian

5

18 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The clock/contr ol interface signals make up the interface for clocking and clock synchr onization. T able 6 lists the Clock/Contr ol interface signals.

The initialization interface signals make up the interface by which an external agent initializes the processor operating parameters. T able 7 lists the initialization interface signals.

The interr upt/status interface signals make up the interface used by the external agent to interr upt the R4300 processor and to monitor instr uction execution for the

ExtRqst* Input

An external agent asserts ExtRqst *to request use of the System interface. The processor grants the r equest by asserting Release *.

Release* Output

In response to the assertion of ExtRqst *, the pr ocessor asserts Release *, signalling to the r equesting device that the System interface is available.

RdRdy* Input

The external agent asserts RdRdy *to indicate that it can accept a pr ocessor r ead or can accept a read followed by write request .

WrRdy* Input An external agent asserts WrRdy *when it can accept a pr ocessor write r equest.

Table 6: Clock/Contr ol Interface Signals

Name Direction Description

MasterClock Input Master clock input that establishes the processor operating fr equency .

MasterOut Output Master clock output aligned with Master- Clock .

TClock Output

Transmit clocks that establish the System interface fr equency . TClock is alignedwith MasterOut .

RClock Output

Receive clocks that establish the System interface fr equency . RClock leads Master- Out by 90 degr ees.

SyncOut Output

Synchr onization clock output. Must be connected to SyncIn through an interconnect that models the inter connect between MasterOut , TClock , RClock , and the external agent.

SyncIn Input Synchr onization clock input.

Table 7: Initialization Interface Signals

Name Direction Description

Reset* Input This signal must be asserted for any r eset sequence.

ColdReset* Input

When asserted, this signal indicates to the R4300 processor that the +3.3 volt power supply is stable and the R4300 chip should initiate a cold r eset sequence. The assertion of ColdReset* will r eset the PLL.

ByPassPLL* Input

This signal for ces MasterClock to bypass the PLL and to feed dir ectly to the clock buffers.

BigEndian* Input This signal defines the byte or der of the system interface.

DataRate* Input

This signal defines the rate at which the R4300 processor will send data to the external agent on block write transactions.

- 0 = DDx data pattern - 1 = Dxx data pattern

Table 5: System Interface Signals curr ent pr ocessor cycle. The status pins ar e zero except when ITS bit in Status r egister is one. T able 8 lists the interr upt/status interface signals.

The JTAG interface signals make up the interface that provides the JT AG boundary scan mechanism. T able 9 lists the JTAG interface signals.

Figure 50 shows the primary communication paths for the System interface: a 64-bit address and data bus, SysAD(63:0), and a 9-bit command bus, SysCmd(8:0). These buses are bidirectional; that is, they are driven by the processor to issue a processor request, and by the external agent to issue an external request .

A request thr ough the System interface consists of: an addr ess, a system interface command that specifies the precise natur e of the r equest, and a series of data elements if the r equest is for a write, or r ead r esponse.

Cycles in which the SysAD bus contains a valid address are called address cycles. Cycles in which the SysAD bus contains valid data are called data cycles. The most significant bit of the SysCmd bus is used to indicate whether the current cycle is an address cycle or a data cycle. During address cycles, the remainder of SysCmd contains a system interface command. During data cycles, the remainder of SysCmd contains the data identifier.

The processor will repeat the address cycle until the

Table 8: Interrupt/Status Interface Signals

Name Direction Description

Int*(4:0) Input

Five general pr ocessor interr upts. These are visible as bits 14 to 10 of the Cause register .

NMI* Input Non-maskable interr upt.

Status(3:0) Input

This signals change with each rising edge of pclock and indicate the decode of the instr uction occupying the WB pipestage for the curr ent pr ocessor cycle. The decode for status(3:0) ar e:

- 0 = Other integer instr uction - 1 = Integer load - 2 = Integer untaken branch - 3 = Integer taken branch - 4 = Integer stor e - 5 - 7 = reserved - 8 = Other stall type - 9 = Stall on instr uction cache access - a = Stall on data cache access - b = Reserved - c = Floating-point op - d = Killed by branch - e = Kill by exception - f = Reserved

Table 9: JTAG Interface Signals

Name Direction Description

JTDI Input Data is serially scanned in thr ough this pin.

JTCK Input

The pr ocessor r eceives a serial clock on JTCK. On the rising edge of JTCK, both JTDI and JTMS are sampled.

JTDO Output Data is serially scanned out thr ough this pin.

JTMS Input JTAG command signal, indicating the incoming serial data is command data.

19 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

external agent indicates that it is capable of accepting the request. The last address cycle is called the issue cycle. There are two types of issue cycle: processor read request issue cycles, and processor write request issue cycles. The processor samples the signal RdRdy* to determine the issue cycle for a processor read request; the processor samples the signal WrRdy* to determine the issue cycle of a processor write request. After the issue cycle, if the processor request requires data to be sent, the data transmission begins. There is only one issue cycle for any processor request.

As shown in Figur e 51, RdRdy* must be asserted two cycles prior to the addr ess cycle of the pr ocessor r ead request to define the addr ess cycle as the issue cycle.

As shown in Figur e 52, WrRdy* must be asserted two cycles prior to the addr ess cycle of the pr ocessor write request to define the addr ess cycle as the issue cycle.

When the R4300 pr ocessor is driving the SysAD and SysCmd buses, the System interface is in master state. When the external agent is driving the SysAD and SysCmd buses, the System interface is in slave state. The pr ocessor is the default master of the system interface.

The external agent becomes master of the system interface only thr ough arbitration pr otocol or uncompelled change to slave state. An uncompelled change to slave state is initiated by the pr ocessor, after it issued a r ead r equest, by asserting Release*. The arbitration cycle consists of the

Figure 50: System Interface Bus

R4300

External Agent

SysAD(63:0)

SysCmd(8:0)

SCycle 1 2 3 4 5 6

SClock

SysAD Bus Addr

RdRdy*

Figure 51: State of RdRdy* Signal for Read Requests

SCycle 1 2 3 4 5 6

SClock

SysAD Bus Addr

WrRdy*

Figure 52: State of WrRdy* Signal for Write Requests following steps:

1. The external agent asserts ExtRqst* when it wishes to submit an external r equest.

2. The processor waits until it is ready to handle an external request, whereupon it asserts Release* for one cycle.

3. The processor sets the SysAD and SysCmd buses to tri-state.

4. The external agent must begin driving the SysAD bus and the SysCmd bus two cycles after the assertion of Release*.

5. The external agent deasserts ExtRqst* two cycles after the assertion of Release*, unless the external agent wishes to perform an additional external request.

6. The external agent sets the SysAD and the SysCmd buses to tri-state at the completion of an external request.

The processor can start issuing a processor request one cycle after the external agent sets the bus to tri-state.

Figure 53 is a timing diagram of the arbitration protocol, in which slave and master states are shown. Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively .

There are two broad categories of requests: processor requests and external requests. Processor requests include: read requests, and write requests. External requests include: read responses, write requests, and null requests.

A processor r equest is a request thr ough the System interface, to access some external r esour ce. As shown in Figur e 54 processor r equests include r ead, and write.

Figure 53: Bus Arbitration Protocol for External Request

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Addr Data0

SysCmd Bus Cmd EOD

ValidIn*

ExtRqst*

Release*

1 2

3 4

5

6

Master Slave Master

R4300 External Agent

Processor Requests • Read • Write

Figure 54: Processor Requests

20 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

The following r ules apply to pr ocessor r equests.

• After issuing a pr ocessor r ead r equest, the processor cannot issue a subsequent r ead r equest until it has r eceived a r ead r esponse.

• It is possible that back-to-back write r equests can be issued by the R4300 with no idle cycles on the bus between r equests.

Processor r ead r equest asks for a block, doublewor d, partial doublewor d, wor d, or partial wor d of data either from main memory or fr om another system r esour ce. When a pr ocessor issues a r ead r equest, the external agent must access the specified r esour ce and r eturn the r equested data.

A pr ocessor r ead r equest that has been issued, but for which data has not yet been r eturned, is said to be pending. A read r emains pending until the r equested r ead data is returned. Only one pr ocessor r ead r equest may be pending at a time.

The pr ocessor transitions to slave after the issue cycle of the r ead r equest by asserting the Release* signal for one cycle. An external agent may then r eturn the r equested data via a r ead r esponse. A pr ocessor r ead r equest is completed after the last wor d of response data has been received fr om the external agent. Note that the data identifier associated with the r esponse data can signal that the r eturned data is err oneous, causing the pr ocessor to take a bus err or.

The following sequence describes the pr otocol for a processor r ead r equest (the number ed steps below correspond to Figur es 55 and 56).

1. RdRdy* is asserted low, indicating the external agent is ready to accept a read request.

2. With the System interface in master state, a processor read request is issued by driving a read command on the SysCmd bus and a read address on the SysAD bus.

3. At the same time, the processor asserts ValidOut* for one cycle, indicating valid data is present on the SysCmd and the SysAD buses.

4. The pr ocessor makes an uncompelled change to slave state either at the issue cycle of the r ead request, or sometime after the issue cycle of the read r equest by asserting the Release* signal for one cycle . NOTE: The external agent must not assert the signal ExtRqst* for the purposes of returning a read response, but rather must wait for the uncompelled change to slave state. The signal ExtRqst* can be asserted before or during a read response to perform an external request other than a read response.

5. The processor releases the SysCmd and the SysAD buses one SCycle after the assertion of Release*.

6. The external agent drives the SysCmd and the SysAD buses within two cycles after the assertion of Release*.

Once in slave state (starting at cycle 5 in Figur e 55), the external agent can r eturn the r equested data thr ough a r ead response. The r ead r esponse can r eturn the r equested data or, if the r equested data could not be successfully r etrieved, an indication that the r eturned data is err oneous. If the returned data is err oneous, the pr ocessor takes a bus err or exception.

Figur e 55 illustrates a pr ocessor r ead r equest, coupled with an uncompelled change to slave state, that occurs as the r ead r equest is issued . Figur e 56 illustrates a pr ocessor read r equest, and the subsequent uncompelled change to slave state, that occurs sometime after the r ead r equest is issued.

NOTE: Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively.

A processor r ead r equest can be split fr om the external agent’s return of the r equested data; in other wor ds, the external agent can initiate an unr elated external r equest before it returns the r esponse data for a pr ocessor r ead. This occurs when a r ead r equest is pending, ExtRqst* is asserted, and Release* is asserted for one cycle—it may be unclear if the assertion of Release* is in r esponse to ExtRqst*, or r epresents an uncompelled change to slave state. In this cases, the pr ocessor accepts either a r ead response, or any other external r equest. If any external request other than a r ead r esponse is issued, the pr ocessor performs another uncompelled change to slave state after processing the external r equest.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Addr

SysCmd Bus Read

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

2 3

4

Master Slave

5

1

6

Figure 55: Processor Read Request Protocol

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus^{Addr}

SysCmd Bus^{Read}

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

3

4

2

5

Master Slave

1

6

Figure 56: Processor Read Request Protocol, Change to Slave State Delayed

21 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

An external agent must r eturn data to the pr ocessor in response to a pr ocessor r ead r equest by using a r ead response pr otocol. A r ead r esponse pr otocol consists of the following steps:

1. The external agent waits for the processor to perform an uncompelled change to slave state.

2. The external agent returns the data through a single data cycle or a series of data cycles.

3. After the last data cycle is issued, the read

response is complete and the external agent sets the SysCmd and SysAD buses to a tri-state.

4. The System interface returns to master state.

NOTE: The processor always performs an uncompelled change to slave state after issuing a read request.

5. The data identifier for data cycles must indicate the fact that this data is response data.

6. The data identifier associated with the last data cycle must contain a last data cycle indication.

The data identifier associated with a data cycle can indicate that the data transmitted during that cycle is erroneous; however , an external agent must r eturn a data block of the corr ect size r egardless of the fact that the data may be in err or. If a read r esponse includes one or mor e erroneous data cycles, the pr ocessor then takes a bus err or.

Read r esponse data must only be deliver ed to the processor when a pr ocessor r ead r equest is pending. The behavior of the pr ocessor is undefined when a r ead response is pr esented to it and ther e is no pr ocessor r ead pending.

Figur e 57 illustrates a pr ocessor wor d read r equest followed by a wor d read r esponse. Figur e 58 illustrates a read r esponse for a pr ocessor block r ead with the System interface alr eady in slave state.

NOTE: Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Addr Data0

SysCmd Bus^{Read EOD}

ValidOut*

ValidIn*

ExtRqst*

Release*

6

1

2

3 4

Master Slave

Master

5

Figure 57: Processor Word Read Request, follow by a word Read Response Protocol

Processor write r equest provides a block, doublewor d, partial doublewor d, wor d, or partial wor d of data to be written either to main memory or to another system resour ce. When a processor issues a write request, the specified resource is accessed and the data is written to it.

A processor write r equest is complete after the last wor d of data has been transmitted to the external agent.

Processor write r equests ar e issued using one of two protocols:

• Doubleword, partial doubleword, word, or partial word writes use a wor d^1 write r equest protocol.

• Block writes use a block write r equest pr otocol.

Processor doublewor d write r equests ar e issued with the System interface in master state, as described below in the steps below; Figur e 59 shows a pr ocessor single wor d write r equest cycle.

1. A processor single word write request is issued by driving a write command on the SysCmd bus and a write address on the SysAD bus.

2. The processor asserts ValidOut*. 3. The processor drives a data identifier on the SysCmd bus and data on the SysAD bus.

4. The data identifier associated with the data cycle must contain a last data cycle indication. At the end of the cycle, ValidOut* is deasserted. NOTE: Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively.

Processor block write r equests ar e issued with the System interface in master state, as described below; a processor block r equest for four wor ds of data is illustrated in Figur es 60 and 61.

1. The pr ocessor issues a write command on the SysCmd bus and a write address on the SysAD bus 2. The processor asserts ValidOut*.

1. Called word to distinguish it fr om block request protocol. Data transferr ed can actually be doublewor d, partial doublewor d, wor d, or partial wor d.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Data2 Data3

SysCmd Bus Data EOD

ValidOut*

ValidIn*

ExtRqst*

Release*

6 2 3^4 5

Slave Master

Figure 58: Block Read Response, System Interface already in Slave State

22 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

3. The processor drives a data identifier on the SysCmd bus and data on the SysAD bus.

4. The processor asserts ValidOut* for a number of cycles sufficient to transmit the block of data.

5. The data identifier associated with the last data cycle must contain a last data cycle indication. NOTE: As shown in Figure 61, however, the first data cycle does not have to immediately follow the address cycle.

Figur es 60 and 61 illustrate a pr ocessor block r equest for four wor ds of data.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus AddrData0

SysCmd Bus WriteEOD

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

4 2 1

Master

3

Figure 59: ProcessorSingle Word Write Request Protocol

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Addr Data0 Data1

SysCmd Bus Write Data EOD

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

5 2 4 1

Master

3

Figure 60: ProcessorBlock Write Request Protocol

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus^{Addr Data0 Data1}

SysCmd Bus Write Data EOD

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

4 5

6

2 1

Master

3

Figure 61: ProcessorBlock Write Request Protocol (Delayed in Transmit Data)

The external agent uses RdRdy* and W rRdy* signals to contr ol the flow of the pr ocessor r ead and write r equests , respectively .

Figur es 62 thr ough 64 illustrate this flow contr ol, as described in the steps below .

1. The processor samples the signal RdRdy* to determine if the external agent is capable of accepting a read request.

2. The signal WrRdy* controls the flow of a processor write request.

3. The processor does not complete the issue of a read request, until it issues an address cycle in response to the request for which the signal RdRdy* was asserted two cycles earlier.

4. The processor does not complete the issue of a write request until it issues an address cycle in response to the write request for which the signal WrRdy* was asserted two cycles earlier.

Figur e 62 illustrates two pr ocessor write r equests in which the issue of the second is delayed for the assertion of WrRdy*.

Figur e 63 illustrates a pr ocessor r ead r equest in which the issue of the r ead is delayed for the assertion of RdRdy*.

Figur e 64 illustrates the issue of a pr ocessor write request delayed for the assertion of W rRdy* and the completion of an external write r equest.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus^{Addr Data0 Addr Data0}

SysCmd Bus^{Write EOD Write EOD}

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

4

2

Figure 62: Processor Write Request Protocol (Delayed by WrRdy*)

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus^{Addr}

SysCmd Bus^{Read}

ValidOut*

ValidIn*

RdRdy*

WrRdy*

Release*

1

3

Figure 63: Processor Read Request Protocol (Delayed by RdRdy*)

23 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

NOTE: Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively.

An External r equest is a request thr ough the System interface, to access the pr ocessor ’s internal r esour ces. As shown in Figur e 54 external r equests include write, and null r equests.

Mastership of the System interface always r eturns to the pr ocessor after an external r equest is issued. The processor does not accept a subsequent external r equest until it has completed the curr ent r equest. The pr ocessor can accept external r equests between the issue of a processor r ead r equest.

If ther e are no pr ocessor r equests pending, the processor decides, based on its internal state, whether to accept the external r equest, or to issue a new pr ocessor request. The pr ocessor can issue a new pr ocessor r equest even if the external agent is r equesting access to the System interface.

The external agent asserts ExtRqst* indicating that it wishes to begin an external r equest. The external agent then waits for the pr ocessor to signal that it is r eady to accept this r equest by asserting Release*. The pr ocessor signals that it is r eady to accept an external r equest based on the criteria listed below .

• The pr ocessor completes any pr ocessor r equest that is in pr ogress.

• While waiting for the assertion of RdRdy* to issue a pr ocessor r ead r equest, the pr ocessor can

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus^{Addr Addr Data0 Addr Data0}

SysCmd Bus^{Write Write EOD Write EOD}

ValidOut*

ValidIn*

RdRdy*

WrRdy*

ExtRqst*

Release*

2

4

Slave

Master Master

Figure 64: Processor Write Request Protocol Delayed for the Assertion of WrRdy* and the Completion of an External Write Request

R4300 External Agent

External Requests • Write • Null

Figure 65: External Requests accept an external r equest if the r equest is deliver ed to the pr ocessor one or mor e cycles before RdRdy* is asserted.

• While waiting for the assertion of W rRdy* to issue a pr ocessor write r equest, the pr ocessor can accept an external r equest pr ovided the r equest is deliver ed to the pr ocessor one or mor e cycles before WrRdy* is asserted.

• If waiting for the r esponse to a r ead r equest after the pr ocessor has made an uncompelled change to a slave state, the external agent can issue an external r equest befor e providing the r ead response data.

External W rite request pr ovides a wor d of data to be written to the pr ocessor ’s internal r esour ce. When an external agent issues a write r equest, the specified r esour ce is accessed and the data is written to it. An external write request is complete after the wor d of data has been transmitted to the pr ocessor.

The only pr ocessor r esour ce available to an external write r equest is the Interrupt register .

External write r equests use a pr otocol identical to the processor single wor d write pr otocol except the V alidIn* signal is asserted instead of V alidOut*. Figur e 66 shows a timing diagram of an external write r equest, which consists of the following steps:

1. The external agent asserts ExtRqst* to arbitrate for the System interface.

2. The processor releases the System interface to slave state by asserting Release*.

3. The external agent drives a write command on the SysCmd bus, a write address on the SysAD bus, and asserts ValidIn*. This write address is ignored by the R4200 as the only writable resource is the Interrupt register.

4. The external agent drives a data identifier on the SysCmd bus, data on the SysAD bus, and asserts ValidIn*.

5. The data identifier associated with the data cycle must contain a last data cycle indication.

6. After the data cycle is issued, the write request is complete and the external agent sets the SysCmd and SysAD buses to a tri-state, allowing the System interface to return to master state. Timings for the SysADC and SysCmdP buses are the same as those of the SysAD and SysCmd buses, respectively. NOTE: External write requests are only allowed to write a word of data to the processor. Processor behavior in response to an external write request for any data element other than a word is undefined.

When the pr ocessor r eleases the System interface to slave state to accept an external r equest, it also allows the external agent to use the SysAD bus for a transfer unr elated to the pr ocessor. After the transfer is completed, the external agent may use External Null request to r eturn 24 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

contr ol of the system interface to the master state without affecting the pr ocessor. This application is useful in a system that wishes to have additional drives and r eceivers on SysAD bus; as illustrated in Figur e 67.

Figur e 68 shows timing diagrams of external null request cycle, which consist of the following steps:

1. The external agent asserts ExtRqst* to arbitrate for the System interface.

2. The processor releases the System interface to slave state by asserting Release*.

3. The external agent drives a external null request command on the SysCmd bus, and asserts ValidIn* for one cycle.

4. The SysAD bus is unused (does not contain valid data) during the address cycle associated with an external null request.

5. After the address cycle is issued, the null request is completed, and the System interface returns to master state.The processor controls the flow of external requests through the arbitration signals ExtRqst* and Release*. The external agent must acquire mastership of the System interface before it is allowed to issue an external request.

The R4300 system interface supports a maximum data rate of one double wor d per cycle. The rate at which data is deliver ed to the pr ocessor may be contr olled by an external agent by driving data and asserting V alidIn* only when data is available. The pr ocessor will interpr et cycles during which ValidIn* is asserted and the SysCmd bus contains a data identifier as valid data cycles. The pr ocessor will continue to accept data until the data wor d tagged as the last data wor d is r eceived. An external agent may deliver data to the pr ocessor at the system interface maximum data rate.

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

SClock

SysAD Bus Addr Data0

SysCmd Bus Write EOD

ValidOut*

ValidIn*

ExtRqst*

Release*

4 5 6

1 2

3 4

Master Slave Master

Figure 66: External Write Request Protocol

ValidIn* R4300 External Agent

Some Device ExtRqst*

Release*

ValidIn*

SysAD

SysCmd

1 2

3 4

3

5

Figure 67: Multiple SysAD Drivers and Receivers System Application

The rate at which the pr ocessor transmits data to an external agent is pr ogrammable via the Datarate* signal. Data patterns ar e specified using the letters "D" and "x", wher e "D" indicates a data cycle and "x" indicates an unused cycle. A data pattern is specified as a sequence of letters, indicating a sequence of data and unused cycles that will be r epeated to pr ovide the appr opriate number of data cycles for a given transfer . The two data rates supported by the R4300 pr ocessor ar e: DDx and Dxx. Figur e 69 shows a pr ocessor block write with a Dxx data rate.

CLOCKS

The clocks on the R4300 pr ocessor ar e contr olled via an on-chip Phase Locked Loop cir cuit. This cir cuit keeps the internal clock edges aligned with the clock edges of the MasterClock signal, which acts as the system master clock.

Inside the R4300 pr ocessor, the MasterClock signal is multiplied by a factor of four , and then all internal clocks are derived by dividing that signal down by some factor of two. Ther e are two primary internal clocks, the pipeline clock PClock, and the system interface clock SClock. While other internal edges may be generated, these ar e transpar ent to the user .

The R4300 pr ocessor also pr ovides external clocks to the system. These clocks ar e the r eceive clock RClock and the transmit clock TClock. TClock is aligned with SClock, while RClock leads by a quarter clock cycle. This is the clocking scheme identical to that used on the R4000 system interface.

The pipeline clock PClock is normally equal to twice the

SCycle 1 2 3 4 n+1 n+2 n+3 n+4 n+5 n+6 n+7 n+8

SClock

SysAD Bus Unsd

SysCmd Bus Null

ValidOut*

ValidIn*

ExtRqst*

Release*

4 5

3

Slave Master

Master

1 2 Figure 68: External Null Request Protocol

Figure 69:Processor Block Write with Dxx Data Pattern

SCycle 1 2 3 4 5 6 7 8 9 10 11 12

Sclock

SysAD Addr Data0 Data1

SysCmd Write Data EOD

ValidOut*

DataRate*

Data0 Data0

WrRdy*

25 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

MasterClock frequency . In reduced power mode, when the RP bit in the Status r egister is set, PClock is driven at one half of the Master Clock fr equency . This is one fourth the normal PClock speed.

The system interface clock, SClock, is normally equal to one half of the PClock frequency . This is equal to the MasterClock frequency . SClock is always derived fr om PClock. Thus when PClock is in reduced power mode, SClock also reduces in fr equency by a factor of four . The R4300 processor drives its outputs on this clock edge.

RClock is generated at the same fr equency as SClock. It is an external clock used to clock input r egisters on external agents. It is skewed by the pr ocessor to lead TClock by 25% of the SClock fr equency .

TClock is generated by the pr ocessor at the same frequency as SClock. It is aligned with SClock. It is used by external agents to drive data, and as the global clock for the external agent. TClock can be thought of as the synchr onized external system interface clock.

The R4300 pr ocessor ’s clocks are contr olled by a phase locked loop cir cuit. The phase locked loop cir cuitry can be disabled by the BypassPLL* pin. In this mode, the internal clock is driven dir ectly by the MasterClock pin of the R4300 processor. This mode can be used for test purposes, as well as in systems whose MasterClock is r unning too slowly for the phase locked loop cir cuit to lock to. The phase locked loop r emains constant when the pipeline slows to one quarter of normal fr equency . Power dissipated by the PLL is r oughly estimated at 0.1W and ther efore relatively insignificant.

MODE SELECT ABLE FEATURES

The R4300 pr ocessor will support several user selectable modes, most of which can be set and r eset by writing to the CP0 Status r egister . In addition, ther e are two dedicated pins, BigEndian and BypassPLL*, which ar e used to selected byte or dering on System interface and to disable the phase-lock-loop cir cuitry during the r eset sequence. The following sections detail all modes supported by the R4300 pr ocessor.

The Reduced Power (RP) mode allows the user to change the pr ocessor operating fr equency to quarter speed. This is established by setting bit 27 of the Status r egister .

This featur e is included to allow the user to selectively reduce power when the system is not being heavily used. This featur e will r educe the power consumed by the processor chip to 25% of its normal value. The default of this mode is normal clocking. The chip will r eturn to this state after any r eset.

The Floating-point Register (FR) mode (bit 26 of the Status r egister) enables the user to access the full set of 32 64-bit floating point r egisters as defined in MIPS-III. When reset, the pr ocessor will access the r egisters as defined in the MIPS II ar chitectur e. This functionality is the same as the R4000.

The Reverse Endianess (RE) mode (bit 25 of the Status register) allows the user to switch byte or dering, between BigEndian and LittleEndian, as seen by user softwar e.

The Instruction T race Support (ITS) mode allows the user to track branches or jumps. This mode is set by writing bit 24 of the Status r egister . When the ITS bit is set, the physical addr ess to which the CPU has branched will be reported on the SysAD bus by for cing an instr uction cache miss whenever a branch, jump or exception is taken. The ITS bit will also enable the driving of the Status pins. When ITS=0, the Status pins will not be driven. By observing the status pins, it is possible to observe when the CPU has completed a Branch or Jump instr uction, in addition to other information. Instr uction T race Support mode is new in the R4200 and is not implemented in the R4000 processor.

The Bootstrap Exception V ectors (BEV), bit 22 in the Status Register , when set, causes the TLB r efill exception vector to be r elocated to a virtual addr ess of 0xbfc00200 and the general exception vector to 0xbfc00380. When cleared, these vectors ar e normally located at 0x80000000 (TLB refill), 0x00000080 (XTLB refill), and 0x80000180 (general), r espectively . This bit is used when diagnostic tests cause exceptions to occur prior to verifying pr oper operation of the cache and main memory system.

The Cache Err or check (CE), bit 17 of the Status r egister , will for ce the substitution of the 8-bit field in the PErr register for computed parity . On stor es, this will enable the user to dir ectly write the parity bits in the data cache, rather than having the computed parity bits used. The parity bits in the instr uction cache can be dir ectly written from the PErr r egister using the Cache operation Fill and having the CE bit set. If CE is set, the T ag parity bit will be written fr om the T agLo register rather than being computed form the tag. This featur e is used for test and diagnostic purposes.

The Disable Err ors (DE), bit 16 of the Status r egister , when set, will specify that the pr ocessor will not take an exception on a cache parity err or.

The Kernel Extended Addr essing (KX), bit 7 of the Status r egister , when set will enable the extended addr essing TLB r efill exception vector to be used for TLB misses on kernel addr esses.

The Supervisor Extended Addr essing (SX), bit 6 of the Status register, if set, enables MIPS III opcodes in supervisor-mode and causes TLB misses on supervisor addresses to use the Extended TLB refill exception vector.

The User Extended Addr essing (UX), bit 5 of the Status register, if set, enables MIPS III opcodes in user-mode and causes TLB misses on user addresses to use the Extended TLB refill exception vector. If clear, implements MIPS II compatibility on virtual address translation.

The Interrupt Enable (IE), bit 0 of the Status r egister , when clear , will not allow interr upts with the exception of reset and non-maskable interr upt.

LOW POWER DISSIP ATION

The R4300 is car efully designed to r estrict power dissipation to make the pr ocessor suitable for operation in battery-power ed devices. Power dissipation in the R4200 is contr olled in two ways: 26 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

- Power management: The pr ocessor may be switched into r educed-power mode or power - down mode by external system logic.

- Reduced Power: A wide variety of logic and circuit design techniques is used to r educe power consumed in normal operating mode.

POWER MANAGEMENT

The R4300 may be dynamically switched to one quarter of its normal operating fr equency by the setting Reduce Power (RP) mode bit in the Status r egister . This will slow the pipeline clock to 20 MHz and the pr ocessor clock to 10 MHz. This event is typically initiated by external logic which sets the RP bit in the status r egister via softwar e. On setting this bit, the output of the clock dividers changes to provide the slower clock rate. Pr ocessing continues at one quarter the rate as befor e. There is a corr esponding dr op in power dissipated to one quarter of that pr eviously .

The Power -down mode is typically initiated by external logic. All dirty cache lines ar e written back to main memory . All variable r egisters ar e readable and writable by softwar e. This allows them to be saved and written to nonvolatile memory while the pr ocessor is power ed down. When power is r estor ed, the pr ocessor state may be written back. State information is written using external softwar e routines.

REDUCED POWER

A variety of cir cuit and logic design techniques is used to reduce power dissipation in the R4200. Many of these techniques save only a small amount of power but it is the cumulative ef fect of these that pr oduces a significant r esult.

These techniques ar e:

• 3.3V Power supply • dynamic (rather than static) logic design • unified datapath for less capacitance • turning of f unused portions of the chip • minimized featur e set • 5-stage pipeline for high ef ficiency • write-back data cache • double instr uction fetch fr om I-cache • use of 2-entry micr o I-TLB • unused logic operates on constants • gating clocks to pipeline logic to pr eserve data in a pipeline stall • Speed de-optimization (no duplicate critical

paths) • Slew rate contr ol and optimal fanout ratios for minimized switching curr ent.

• Minimized Vcc to Vss curr ent path

These all combine to pr oduce the low average power dissipation that allows the R4200 to be a practical batterypower ed pr ocessor.

27 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

PACKAGE INFORMA TION

R4200LP - 208-pin PQFP pin-out :

1 NC 2 NC 3 VSS 4 VCC 5 SysAD45 6 SysAD13 7 Status0 8 SysAD44 9 VSSCore 10 VCCCore 11 SysAD12 12 SysCmdP 13 SysAD43 14 SysAD11 15 VSS 16 VCC 17 SysCmd8 18 SysAD42 19 SysAD10 20 SysCmd7 21 VSS 22 VCC 23 SysAD41 24 SysAD9 25 SysCmd6 26 SysAD40 27 VSSCore 28 VCCCore 29 VSS 30 VCC 31 SysAD8 32 SysCmd5 33 SysADC4 34 SysADC0 35 VSS 36 VCC 37 SysCmd4 38 SysAD39 39 SysAD7 40 SysCmd3 41 VSS 42 VCC 43 SysAD38 44 SysAD6 45 Status1 46 WrRdyB 47 SysAD37 48 SysAD5 49 VSS 50 VCC 51 NC 52 NC

157 NC 158 NC 159 VSS 160 RClock 161 SyncOut 162 SysAD30 163 VCC 164 VSS 165 SysAD62 166 MasterOut 167 SysAD31 168 SysAD63 169 VCCCore 170 VSSCore 171 Div2 172 SysADC3 173 SysADC7 174 VCC 175 VSS 176 BypassPLLB 177 VCCP 178 VSSP 179 PLLCap0 180 PLLCap1 181 VCCP 182 VSSP 183 VCCP 184 VSSP 185 MasterClock 186 VCCCore 187 VSSCore 188 Syncin 189 VCC 190 VSS 191 JTCK 192 SysADC5 193 SysADC1 194 JTDI 195 VCCCore 196 VSSCore 197 SysAD47 198 SysAD15 199 JTDO 200 SysAD46 201 VCC 202 VSS 203 SysAD14 204 JTMS 205 TClock 206 NC 207 NC 208 NC

105 NC 106 NC 107 VCCCore 108 VSSCore 109 VCC 110 VSS 111 SysAD21 112 SysAD53 113 RdRdyB 114 BigEndian 115 SysAD22 116 SysAD54 117 VCC 118 VSS 119 ReleaseB 120 SysAD23 121 SysAD55 122 NMIB 123 VCCCore 124 VSSCore 125 SysADC2 126 SysADC6 127 DataRateB 128 SysAD24 129 VCC 130 VSS 131 SysAD56 132 Status3 133 SysAD25 134 SysAD57 135 VCCCore 136 VSSCore 137 Status2 138 SysAD26 139 SysAD58 140 TestModeB 141 VCC 142 VSS 143 SysAD27 144 SysAD59 145 ColdResetB 146 SysAD28 147 VCC 148 VSS 149 SysAD60 150 ResetB 151 SysAD29 152 SysAD61 153 VCC 154 VSS 155 NC 156 NC

53 NC 54 NC 55 SysCmd2 56 SysAD36 57 SysAD4 58 SysCmd1 59 VSS 60 VCC 61 SysAD35 62 SysAD3 63 SysCmd0 64 SysAD34 65 VSS 66 VCC 67 VSSCore 68 VCCCore 69 SysAD2 70 NC 71 SysAD33 72 SysAD1 73 VSS 74 VCC 75 IntB4 76 SysAD32 77 SysAD0 78 IntB3 79 VSSCore 80 VCCCore 81 IntB2 82 SysAD16 83 SysAD48 84 IntB1 85 VSS 86 VCC 87 SysAD17 88 SysAD49 89 IntB0 90 SysAD18 91 VSS 92 VCC 93 SysAD50 94 ValidInB 95 SysAD19 96 SysAD51 97 VSS 98 VCC 99 ValidOutB 100 SysAD20 101 SysAD52 102 ExtRqstB 103 NC 104 NC

28 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Figure 70: R4200LP - 208-pin PQFP Physical Pin Location

52 NC 51 NC 50 VCC 49 VSS 48 SysAD5 47 SysAD37 46 WrRdyB 45 Status1 44 SysAD6 43 SysAD38 42 VCC 41 VSS 40 SysCmd3 39 SysAD7 38 SysAD39 37 SysCmd4 36 VCC 35 VSS 34 SysADC0 33 SysADC4 32 SysCmd5 31 SysAD8 30 VCC 29 VSS 28 VCCCore 27 VSSCore 26 SysAD40 25 SysCmd6 24 SysAD9 23 SysAD41 22 VCC 21 VSS 20 SysCmd7 19 SysAD10 18 SysAD42 17 SysCmd8 16 VCC 15 VSS 14 SysAD11 13 SysAD43 12 SysCmdP 11 SysAD12 10 VCCCore 9 VSSCore 8 SysAD44 7 Status0 6 SysAD13 5 SysAD45 4 VCC 3 VSS 2 NC 1 NC

NC 105 NC 106 VCCCore 107 VSSCore 108

VCC 109 VSS 110 SysAD21 111 SysAD53 112 RdRdyB 113 BigEndian 114 SysAD22 115 SysAD54 116

VCC 117 VSS 118 ReleaseB 119 SysAD23 120 SysAD55 121

NMIB 122 VCCCore 123 VSSCore 124 SysADC2 125 SysADC6 126 DataRateB 127 SysAD24 128

VCC 129 VSS 130 SysAD56 131

Status3 132 SysAD25 133 SysAD57 134 VCCCore 135 VSSCore 136

Status2 137 SysAD26 138 SysAD58 139 TestModeB 140

VCC 141 VSS 142 SysAD27 143 SysAD59 144 ColdResetB 145

SysAD28 146

VCC 147 VSS 148 SysAD60 149

ResetB 150 SysAD29 151 SysAD61 152

VCC 153 VSS 154 NC 155 NC 156

104 NC

103 NC

102 ExtRqstB

101 SysAD52

100 SysAD20

99 ValidOutB

98 VCC

97 VSS

96 SysAD51

95 SysAD19

94 ValidInB

93 SysAD50

92 VCC

91 VSS

90 SysAD18

89 IntB0

88 SysAD49

87 SysAD17

86 VCC

85 VSS

84 IntB1

83 SysAD48

82 SysAD16

81 IntB2

80 VCCCore

79 VSSCore

78 IntB3

77 SysAD0

76 SysAD32

75 IntB4

74 VCC

73 VSS

72 SysAD1

71 SysAD33

70 NC

69 SysAD2

68 VCCCore

67 VSSCore

66 VCC

65 VSS

64 SysAD34

63 SysCmd0

62 SysAD3

61 SysAD35

60 VCC

59 VSS

58 SysCmd1

57 SysAD4

56 SysAD36

55 SysCmd2

54 NC

53 NC

208 NC

207 NC

206 NC

205 TClock

204 JTMS

203 SysAD14

202 VSS

201 VCC

200 SysAD46

199 JTDO

198 SysAD15

197 SysAD47

196 VSSCore

195 VCCCore

194 JTDI

193 SysADC1

192 SysADC5

191 JTCK

190 VSS

189 VCC

188 Syncin

187 VSSCore

186 VCCCore

185 MasterClock

184 VSSP

183 VCCP

182 VSSP

181 VCCP

180 PLLCap1

179 PLLCap0

178 VSSP

177 VCCP

176 BypassPLLB

175 VSS

174 VCC

173 SysADC7

172 SysADC3

171 Div2

170 VSSCore

169 VCCCore

168 SysAD63

167 SysAD31

166 MasterOut

165 SysAD62

164 VSS

163 VCC

162 SysAD30

161 SyncOut

160 RClock

159 VSS

158 NC

157 NC

29 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

R4200PC 179-pin PGA Package Pinout

K1 Vcc K2 SysAD16 K3 IntB2 K16 VssP K17 VccP K18 Vss L1 Vss L2 SysAD48 L3 IntB1 L16 SysADC3 L17 SysADC7 L18 Vcc M1 Vcc M2 SysAD17 M3 SysAD49 M16 SysAD31 M17 BypassPLLB M18 Vss N1 Vss N2 IntB0 N3 SysAD50 N16 SysAD62 N17 SysAD63 N18 Vcc P1 SysAD18 P2 ValidInB P3 SysAD19 P16 SyncOut P17 MasterOut P18 Vss R1 Vcc R2 SysAD51 R3 ValidOutB R16 RClock1 R17 SysAD30 R18 Vss T1 Vss T2 SysAD20 T3 SysAD52 T4 SysAD21 T5 RdRdyB T6 SysAD54 T7 SysAD55 T8 SysADC2 T9 N/C

Pin R4200PC

Function

C10 SysAD40 C11 SysAD41 C12 SysAD10 C13 SysCmd8 C14 SysCmdP C15 SysAD44 C16 SysAD13 C17 TClock0 C18 Vss D1 Vss D2 SysAD35 D3 SysCmd1 D16 TClock1 D17 SysAD14 D18 Vcc E1 SysAD2 E2 SysCmd0 E3 SysAD3 E16 JTMS E17 SysAD46 E18 SysAD15 F1 Vcc F2 N/C F3 SysAD34 F16 JTDO F17 SysAD47 F18 Vss G1 Vss G2 SysAD1 G3 SysAD33 G16 JTDI G17 SysADC1 G18 Div2 H1 Vcc H2 SysAD32 H3 IntB4 H16 SysADC5 H17 JTCK H18 Vss J1 Vss J2 SysAD0 J3 IntB3 J16 SyncIn J17 MasterClock J18 Vcc

Pin R4200PC

Function

A1 No pin A2 Vcc A3 Vss A4 Vcc A5 SysCmd3 A6 Vss A7 Vcc A8 Vss A9 Vcc A10 Vss A11 Vcc A12 Vss A13 Vcc A14 Vss A15 SysAD43 A16 Vcc A17 Vss A18 Vss B1 Vss B2 SysCmd2 B3 SysAD37 B4 N/C B5 SysAD6 B6 SysAD7 B7 SysCmd4 B8 SysADC4 B9 SysAD8 B10 SysCmd6 B11 SysAD9 B12 SysCmd7 B13 SysAD42 B14 SysAD11 B15 SysAD12 B16 DatarateB B17 SysAD45 B18 Vcc C1 Vcc C2 SysAD4 C3 SysAD36 C4 SysAD5 C5 WrRdyB C6 SysAD38 C7 SysAD39 C8 SysADC0 C9 SysCmd5

Pin R4200PC

Function

Pin R4200PC

Function

T10 SysAD56 T11 SysAD57 T12 SysAD26 T13 N/C T14 ColdResetB T15 SysAD60 T16 SysAD29 T17 RClock0 T18 Vcc U1 Vcc U2 ExtRqstB U3 SysAD53 U4 N/C U5 SysAD22 U6 SysAD23 U7 NMIB U8 SysADC6 U9 SysAD24 U10 BigEndian U11 SysAD25 U12 N/C U13 SysAD58 U14 SysAD27 U15 SysAD28 U16 ResetB U17 SysAD61 U18 Vss V1 Vss V2 Vss V3 Vcc V4 Vss V5 ReleaseB V6 Vcc V7 Vss V8 Vcc V9 Vss V10 Vcc V11 Vss V12 Vcc V13 Vss V14 TestModeB V15 SysAD59 V16 Vss V17 Vcc V18 Vss

30 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Figure 71:R4200PC - 179-pin PGA Physical Pin Location

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • • •

• • • • • • • • • • • • • • • • •

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 V U T R P N M L K J H G F E D C B A

V U T R P N M L K J H G F E D C B A

R4200 PC Pinout x Bottom

31 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

DIFFERENCES FROM THE R4000

For a detailed list of dif ferences amomg the R4x00 series pr ocessors, please r efer to “Designing in common for R4200 (VRX), R4600 (Orion), R4000PC and R4400PC processors”, available fr om MIPS Technologies, Inc.

The R4200 pr ocessor implements the MIPS III instr uction set, as does the R4000. As with any two hardwar e implementations of the same ar chitectur e, ther e are some dif ferences between the R4200 and the R4000. While the R4200 has tried to stay as close to the R4000 implementation as possible both fr om a system design and softwar e viewpoint, ther e are some visible dif ferences. This section highlights the dif ferences between the R4200 and the R4000.

The primary dif ferences between the R4200 and the R4000 are in cache handling. This is primarily because the R4200 processor pr ovides no support for second level caches. The R4200 also pr ovides no support for multipr ocessing, which has an impact on system design.

SOFTWARE VISIBLE DIFFERENCES

The functional dif ferences between the R4000 and the R4200 processor that ar e visible to softwar e are contained in the Copr ocessor 0 implementation.

Cache Ops

Because the R4200 pr ocessor does not support secondary cache, all of the r eferences to secondary cache in the R4000 implementation do not apply to the R4200. Designating either SD or SI (secondary data or instr uction cache) for any cache op on the R4200 is undefined. All writeback operations will send data fr om primary cache to main memory . Cache op number seven (7) is undefined for the R4200.

Cache Op Index Stor e Tag will use parity bit fr om TagLo r egister bit 0 instead of computed parity if CE bit (R4000 section) of cp0 Status r egister is set.

The data cache Dirty bit, W bit in R4000, will be clear ed for cache op Hit W rite Back.

Status Register

The R4200 has a slightly dif ferent status r egister fr om the R4000. The bits that perform identical functionalities are left in the same location on the R4200 as they ar e in the R4000.

One bit of the Status Register that was pr eviously always zer o (i.e. unused) is now used. This is the Instr uction T race Support ITS bit.

The status r egister ’s CH bit, the Cp0 Condition bit used for the Branch on Co-Pr ocessor 0 BC0T/BC0F instr uctions, is writable only by softwar e in the R4200. But, in R4000, this bit can be set or clear ed by the har dwar e dependent on secondary cache operations, which the R4200 does not support.

Configuration Register

The R4200 configuration r egister implements a subset of the fields on the R4000, since the R4200 does not have as many options. The exact meaning of bits within the configuration r egister may be dif ferent.

Unimplemented Operation Exception and other cause bits

The R4000 defines the Unimplemented Operation Exception (E) in FSR supersedes all other cause bits. The Unimplemented Exception handler is expected to ignor e and clear all cause bits. Thus, during E exception, all other cause bits ar e undefined or don’t car e.

The R4200 has stricter definition than R4000. It sets no other FP exception cause bits when ther e is an Unimplemented Operation Exception.

Integer Divide-by-Zero

When dividing an integer by zer o, MIPS ISA specifies the r esult to be undefined. Under this illegal operation, the R4200 returns a dif ferent value in Register LO than the R4000:

Here is what the R4000 r eturns in Hi and Lo for all cases of dividend:

Dividend Lo Hi >= 0 0xFFFFFFFF dividend < 0 0x00000001 dividend

and the R4200 r eturns:

Dividend Lo Hi >= 0 0x7FFFFFFF dividend < 0 0x80000001 dividend

Non-restartable Cache Parity Error exception

The R4200 pr ocesses the Cache Parity Err or exception (DCPE) in the WB stage.

When a cache data parity err or occurs on a load with a cache hit, the R4200 will not pr event the cache data with a bad parity fr om writing into the r egister file in WB stage. The exception is still pr ecise, since both the EPC and CacheErr r egisters ar e updated with the corr ect virtual addr ess pointing to the of fending load instr uction. The exception handler can still determine the cause of exception and its origin. But, the pr ogram cannot be restarted since the bad cache data has clobber ed the destination r egister . Note that CacheErr exception for cache-ops, uncached access, and cache-miss r emains as Dc stage exception and exact.

SYSTEM DESIGN DIFFERENCES

Processor Initialization

The R4000 had a fairly complicated scan based processor initialization scheme.The R4200 has far fewer modes; those that ar e not available via softwar e are hardwir ed as pins on the package. The R4200 also r equir es only 16 cycles of Reset* assertion during the r eset sequence.

32 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

System Interface

The R4200 uses the same SysAD bus pr otocol as the R4000; however , since the R4200 pr ocessor does not support multipr ocessing or secondary cache, the R4200 only implements a subset of the full SysAD bus definition. Any transactions that r eference multi-pr ocessing or secondary cache featur es are undefined.

The R4200 offers an optional enhancement over the R4000 SysAD pr otocol. This enhancement can incr ease the performance of uncached memory accesses, important in graphics applications. However in or der to avail of this enhancement, the interfacing ASICs must be able to handle the incr eased traf fic on the SysAD bus. Some ASICs, designed originally for the R4000 ar e known not to be compatible with these enhancements. Details of the optional SysAD dif ferences in R4000 and R4200 ar e listed in a separate document “Designing in common for R4200 (VRX), R4600 (Orion), R4000PC and R4400PC pr ocessors”, available fr om MIPS Technologies, Inc.

For compatibility with existing R4000 ASICs, the default mode of operation does not use the enhancement mentioned above. The enhancement is set at boot time using the DataRate* pin.

The R4200 will support two data rates for write transactions: DDx and Dxx. The rate to be used by the R4200 is programmed via the DataRate* pin. A DataRate* signal of ‘0’ indicates a DDx datarate and R4200 SysAD enhancement functional. A DataRate* signal of ‘1’ indicates a Dxx datarate and R4200 SysAD enhancement disabled.

The R4200 has fixed sizes for instr uction cache lines (8 wor ds) and data cache lines (4 wor ds). Instr uction blocks will be written to the memory system as an eight wor d transaction. (The writing of instr uction cache lines to memory can be done via the Hit W rite Back Cache Op).

The R4200 handles data coming onto the pr ocessor as fast as it can be deliver ed by the SysAD bus. Ther e will never be a str eam of data pr esented to the R4200 pr ocessor exceeding four doublewor ds, and the R4200 can handle a data pattern of DDDD.

In order to conserve power , the R4200 pr ocessor will provide only a single T clock and a single R clock.

RP Bit Ef fect on System Interface

On the R4000, SClock and TClock were unaf fected by the RP bit. On the R4200, setting the RP bit will r educe the clock frequency of SClock and TClock by a factor of four . If ther e are any timing dependent featur es in an external agent that would be af fected by this (e.g., DRAM r efresh counters), the external agent must pr ovide softwar e a mechanism to accommodate the fr equency change.

OTHER DIFFERENCES

Cache Size

The R4200 will implement a 16kB, dir ect mapped, virtually indexed instr uction cache with a cache line of eight wor ds (thirty-two bytes). The data cache is 8kB, dir ect mapped, virtually indexed with a cache line of four wor ds

(sixteen bytes). This implies that any softwar e routines for initializing, invalidating, or flushing cache must take this difference into account. TLB TLB entries

The R4200 will implement a thirty-two way , fully associative TLB in which each entry maps two Page Frame Numbers, one even and one odd. While the str uctur e of this is identical to the R4000, the number of entries is reduced fr om forty-eight entries on the R4000.

Interactions between ITM & TLB Ops

When a softwar e TLB instr uction is accessing the JTLB during the same cycle as an Instr uction TLB Miss (ITM) stall, the R4000 behaves in an undefined manner , and can actually generate a bogus TLB Invalid Exception, especially when the TLB softwar e read/write operation (tlbwi, tlbwr , tlbr) is accessing a completely dif ferent entry than that accessed on behalf of the Instr uction TLB miss.The R4200 has corr ected this bogus TLB behavior .

Floating Point Coprocessor

Floating-point Datapath

The R4200 integrates the operation of Copr ocessor 1, the floating point copr ocessor, into the main pipeline and datapath of the integer pr ocessor. This means that the integer pipe will stall for any multicycle floating point instr uctions. This is invisible to softwar e and has no ef fect on integer pr ocessing.

Variable latencies

Any multicycle instr uction which experiences a sour ce exception (i.e. an exception with its sour ce operands) will not cause a stall. Instead, it will issue a default r esult on that cycle or r eport a trapped exception on the next cycle, depending on the trap enable flags. In addition, certain trivial calculations (such as 0 * 0) will be performed with less latency than non-trivial cases of the same operation. The R4000, on the other hand, always has the same latency for each particular instr uction whether an exception occurs or not.

Cvt.[s,d].l instruction

To convert a 64-bit integer to a single- or doubleprecision floating point number , R4000 initiates a FP unimplemented operation exception when bits 63...52 of an integer ar e all Ones or all Zer os.

Since it has a unified 64-bit datapath for both integer and floating-point operations, the R4200 can pr ocess mor e bits out of a 64-bit integer in the long integer to floatingpoint convert instr uction, without added cost to the design. The R4200 raises a FP unimplemented operation exception only when bits 63...55 of a 64-bit integer ar e all Ones or all Zeros.

33 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

RP Bit Ef fect on PClock

On the R4000, setting the RP bit is described as reducing the PClock frequency by a factor of two thr ough sixteen, although in fact it is non-functional. On the R4200, this bit will r educe PClock frequency by a factor of four .

Pipeline

The R4200 uses a simpler pipeline than the R4000. This pipe is a five stage pipe that str ongly r esembles the pipeline used on the R3000. The R4200 is not superpipelined. This is not visible in any functional way , but may impact how dif ferent code sequences may be optimized. This also means that ther e are fewer stalls due to the basic pipeline. This incr eases the CPI component due to cache misses, meaning that the system design of the memory system is even mor e crucial to the performance of the R4200 pr ocessor.

Interrupts

The R4200 dedicates bit 15 of the Cause Register , which is bit 7 of the Interr upt Pending field, to the timer interr upt caused when the Compar e and Count r egisters match. Because of this, the pin Int*[5] has been r emoved. W riting to Interr upt r egister bit 5 via the system interface will have no effect. The R4000 allowed the user to select whether bit 15 was dedicated to the timer interr upt or to Interr upt register bit 5. Interr upt r egister bit 5 has been eliminated on the R4200.

Kernel Physical Address Segment Organization

The R4200 implements only two cache coher ency algorithms, uncached and cacheable non-coher ent. This, and the fact that the R4200 implements only 33 physical addr ess bits as compar ed to the R4000’s 36-bit physical addr esses, is r eflected in the virtual addr ess map in the organization of the Kernel Physical Addr ess Space segment. The R4200 br eaks this segment further into two valid addr ess spaces, one per cache coher ency algorithm, while the r est of the addr ess space is unavailable. The R4000 processor, in contrast, has mor e valid addr esses in this segment. Refer to Figur e 48 for the or ganization of this virtual addr ess segment for the R4200 pr ocessor.

JTAG

When in Shift-IR and Shift-DR modes, IEEE Std1 149.1- 1990 on page 5-1 1 in Table 5-2 states that JTDO should be active. The R4200 implements the JT AG contr oller per IEEE Std1149.1-1990. But, R4000 implements an older version of the standar d and does not drive JTDO under these two modes.

CHANGES TO THIS DOCUMENT

Rev. 1.1 (June ‘93)

On P.17 and P.18, Figur e 49 and Table 7 have been updated to show that the ByPassPLL input signal has been defined as active low (now ByPassPLL* or ByPassPLLB).

On P.27, in the packaging information for the 208-pin PQFP package, the following pin-assignments have been corrected following a change in the design:

Pin 129: VCC (was VSS)

Pin 130: VSS (was VCC)

Pin 176: ByPassPLLB (was ByPassPLL)

On P.28, the above changes to the pin-assignments ar e reflected in the pin-out diagram.

A new page 29 and 30 have been added to show the pin assignments and pin-out diagram for the 179-pin PGA package which has str ong compatibility with the R4000PC.

Rev. 1.2 (July ‘93)

On P.3, Figur e 7 was corr ected to show Instr uction Virtual Addr ess calculation (IV A) commencing on phase 2 of the RF stage.

On P.4, the activity of calculating the virtual branch target addr ess is stated under the RF stage rather than the EX stage.

On P.4, an explanation of har dwar e interlocking on a load delay slot was included.

On P.4, the priority of pipeline stalls and exceptions was r eordered, reflecting the pr ocessor design.

On P.7, last line, left-hand column, text was changed to state that instr uction fetches ar e initiated if ther e is a jump or branch instr uction in the EX stage, not the RF stage.

On P.12, the implementation identifier in the PRId register was added.

On P.13, the IB and DB fields of the Configuration register had been described as r eadable and writable. They are in fact har dwir ed and ar e readable only . The reference was r emoved.

On P.14, Figur e 41 was changed to corr ectly describe the TagLo register fields.

On P.16, Figur e 48 was changed to show the corr ect Kernel Mode V irtual Addr ess Space. The pr evious figur e had shown that of the R4000.

On P.16, Table 2 and 3 wer e changed to cor eect a number of the exception vectors which had been stated incorr ectly.

On P.22 in the last line of the page, the wor d invalidate as part of the term “external invalidate r equest” was changed to “write” to corr ectly describe the transaction taking place in Figur e 64.

On P.24, Figur e 69 and the adjacent text was changed to give a better example of datarate being contr olled by the setting of their DataRate* signal. The diagram now shows a processor block write instead of a block r ead r esponse.

On P.25, the description of the operation of the phase locked loop was extended to include operation during reduced power mode.

On P.25, the Bootstrap Exception V ector values wer e corrected. 34 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

On P.31, a reference to a new additional document “Designing in common for R4x00 series pr ocessors” is included.

On P.32, an optional enhancement to the SysAD protocol is described in accor dance with a change in the design.

On P.32, the description of an Instr uction Cache Line writeback has been corr ected.

Rev. 1.3. (October ‘93)

On P.17, RdRdy* and W rRdy* signals ar e corrected to show them as inputs to the pr ocessor, not outputs.

On P. 17, P.18 and P.25, the BigEndian signal is corrected fr om “active low (BigEndian*) to normal.

On P.18, P.25, P.27 and P.29, the BypassPLL* signal name spelling is corr ected fr om “ByPassPLL*”.

On P.18, Table 6 has been corr ected to r ead that Rclock leads MasterOut by 90 degr ees and T clock is aligned with MasterOut.

Rev. 1.4. (August ‘94)

On P.4, two new interlock conditions “DCPI” and “CP0I”, and one new exception condition “DCPE” ar e added to Figur e 10 “Pipeline interlocks and exceptions”.

On P.9, the text has been amended to include all seven page sizes in the TLB, not just 4K and 16M bytes as in early versions.

On P.10, Fig. 23, C field, all values besides C=010 now are defined as cached.

On P.10, the last paragraph has been amended to include all seven page sizes in the TLB, not just 4K and 16M bytes as in early versions.

On P.11, Fig. 25, CP0 Mask Register has been amended to include all seven page sizes in the TLB, not just 4K and 16M bytes as in early versions.

On P.12, Fig. 31, a description of the IE field in the Status r egister has been included.

On P.13, Fig. 36, the description of the Paddr field has been modified.

On P.13, Fig.37, the positions of the R and W fields has been corr ected.

On P.17, Table 4 has been updated.

On P.32, a paragraph outlining dif ferences between the TLB in the R4200 and R4000 was eliminated.

35 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Table 10: Load and Stor e Instruction Summary

MIPS ISA LB rt, offset (rs) LBU rt, offset (rs)

Load Byte Load Byte Unsigned

SB rt, offset (rs) Store Byte

LH rt, offset (rs) LHU rt, offset (rs)

Load Halfwor d Load Halfwor d Unsigned

SH rt, offset (rs) Store Halfwor d

LW rt, offset (rs) Load Word SW rt, offset (rs) Store Word LWL rt, offset (rs) Load Word Left SWL rt, offset (rs) Store Word Left LWR rt, offset (rs) Load Word Right SWR rt, offset (rs) Store Word Right MIPS ISA Extensions LD rt, offset (rs) Load Double SD rt, offset (rs) Store Double-wor d LDL rt, offset (rs) Load Double Left SDL rt, offset (rs) Store Double-wor d Left LDR rt, offset (rs) Load Double Right SDR rt, offset (rs) Store Double-wor d Right LL rt, offset (rs) Load and Link SC rt, offset (rs) Store Conditional LLD rt, offset (rs) Load and Link Double-wor d SCD rt, offset (rs) Store Double-wor d Conditional LWU rt, offset (rs) Load Word Unsigned Sync Sync

Table 11: Arithmetic Instructions

MIPS ISA ADD rd, rs, rt Add ADDI rt, rs, immediate Add Immediate ADDU rd, rs, rt Add Unsigned ADDIU rt, rs, immediate Add Immediate unsigned SUB rd, rs, rt Subtract SUBU rd, rs, rt Subtract Unsigned MULT rs, rt Multiply MULTU rs, rt Multiply Unsigned DIV rs, rt Divide DIVU rs, rt Divide Unsigned MFHI rd Move Fr om Multiply Hi Register MFLO rd Move Fr om Multiply Lo Register MTHI rd Move To Multiply Hi Register MTLO rd Move To Multiply Lo Register AND rd, rs, rt Bitwise AND ANDI rs, rt, immediate Bitwise AND Immediate OR rd, rs, rt Bitwise OR ORI rs, rt, immediate Bitwise OR Immediate XOR rd, rs, rt Bitwise Exclusive XORI rs, rt, immediate Bitwise Exclusive Immediate NOR rd, rs, rt Bitwise NOR LUI rt, immediate Load upper Immediate SLT rd, rs, rt Set on Less Than SLTI rt, rs, immediate Set on Less Than Immediate SLTU rd, rs, rt Set on Less Than Unsigned SLTIU rt, rs, immediate Set on Less Than Immediate Unsigned SLL rd, rt, sa Shift Left Logical SRL rd, rt, sa Shift Right Logical SLLV rd, rt, rs Shift Left Logical V ariable SRLV rd, rt, rs Shift Right Logical V ariable SRA rd, rt, sa Shift Right Arithmetic SRAV rd, rt, rs Shift Right Arithmetic V ariable MIPS ISA Extensions DADD rd, rs, rt Double Add DADDI rt, rs, immediate Double Add Immediate DADDU rd, rs, rt Double Add Unsigned DADDIU rt, rs, immediate Double Add Immediate unsigned DSUB rd, rs, rt Double Subtract DSUBU rd, rs, rt Double Subtract Unsigned DMULT rs, rt Double Multiply DMULTUrs, rt Double Multiply Unsigned DDIV rs, rt Double Divide DDIVU rs, rt Double Divide Unsigned DSLL rd, rt, sa Double Shift Left Logical DSRL rd, rt, sa Double Shift Right Logical DSLLV rd, rt, rs Double Shift Left Logical V ariable DSRLV rd, rt, rs Double Shift Right Logical V ariable DSRA rd, rt, sa Double Shift Right Arithmetic DSRAV rd, rt, rs Double Shift Right Arithmetic V ariable DSLL32 rd, rt, sa Double Shift Left Logical+32 DSRL32 rd, rt, sa Double Shift Right Logical+32 DSRA32 rd, rt, sa Double shift Right Arithmetic+32

Table 12: Jump and Branch Instruction Summary

MIPS ISA J target Jump JAL target Jump And Link JR rs Jump Register JALR rs, rd Jump And Link Register BEQ rs, rt, of fset Branch on Equal BNE rs, rt, of fset Branch on Not Equal BLEZ rs, offset Branch on Less than or Equal Zer o BGEZ rs, offset Branch on Gr eater than or Equal Zer o BLTZ rs, offset Branch on Less than Zer o BGTZ rs, offset Branch on Gr eater than Zer o BLTZAL rs, offset Branch on Less than Zer o And Link BGEZAL rs, offset Branch on Gr eater than or Equal Zer o And Link MIPS ISA Extensions BEQL rs, rt, of fset Branch on Equal Likely BNEL rs, rt, of fset Branch on Not Equal Likely BLEZL rs, offset Branch on Less Than or Equal to Zer o Likely BGEZL rs, offset Branch on Gr eater Than or Equal to Zer o Likely BLTZL rs, offset Branch on Less Than Zer o Likely BGTZL rs, offset Branch on Gr eater Than Zer o Likely BLTZALL rs, offset Branch on Less Than Zer o And Link Likely BGEZL rs, offset Branch on Gr eater Than or Equal to Zer o And Link Likely

36 R4300 Preliminary Datasheet Rev.0.1 Jan‘95

Table 13: Special Instruction Summary

MIPS ISA SYSCALL System Call BREAK Break Point

Table 14: Exception Instruction Summary

MIPS ISA Extensions TGE rs, rt Trap if Gr eater Than or Equal TGEI rs, Immediate Trap if Gr eater Than or Equal Immediate TGEU rs, rt Trap if Gr eater Than or Equal Unsigned TGEIU rs, Immediate Trap if Gr eater Than or Equal Immediate Unsigned TLT rs, rt Trap if Less Than TLTI rs, Immediate Trap if Less Than Immediate TLTU rs, rt Trap if Less Than Unsigned TLTIU rs, Immediate Trap if Less Than Immediate Unsigned TEQ rs, rt Trap if Equal TEQI rs, Immediate Trap if Equal Immediate TNE rs, rt Trap if Not Equal TNEIU rs, Immediate Trap if Not Equal Immediate Unsigned

Table 15: Copr ocessor Instruction Summary

MIPS ISA LWCz rt, offset(rs) Load Word to Copr ocessor z SWCz rt, offset(rs) Store Word from Copr ocessor z MTCz rt, rd Move To Copr ocessor z MFCz rt, rd Move Fr om Copr ocessor z CTCz rt, rd Move Contr ol To Copr ocessor z CFCz rt, rd Move Contr ol From Copr ocessor z BCzT offset Branch on Copr ocessor True BCzF offset Branch on Copr ocessor False COPz cofun Copr ocessor z Operation MIPS ISA Extensions LDCz rt, offset(rs) Load Double to Copr ocessor z SDCz rt, offset(rs) Store Double fr om Copr ocessor z DMTCz rt, rd Double Move T o Copr ocessor z DMFCz rt, rd Double Move Fr om Copr ocessor z BCzTL offset Branch on Copr ocessor True Likely BCzFL offset Branch on Copr ocessor False Likely

Table 16: System Contr ol Copr ocessor (CP0) Instruction Summary

MIPS ISA MTC0 rt, rd Move to CP0 MFC0 rt, rd Move Fr om CP0 TLBR Read Indexed TLB Entry TLBWI Write Indexed TLB Entry TLBP Probe TLB for Matching Entry TLBWR Write Random TLB Entry ERET Return fr om Exception CACHE sub, of fset(rs) Cache Operation

Table 17: R4300 Cache Op Instruction Summary

MIPS ISA Extensions CACHE 0x0, offset(rs) op = 0: Index Invalidate; I-Cache Set the cache state of the cache line to invalid. CACHE 0x1, offset(rs) op = 1: Index W rite-back Invalidate; D-Cache Examines the cache state, if valid dirty , then that block is written back to main memory . Afterwar d, set the cache state of the cache line to invalid.

CACHE 0x4, offset(rs) op = 4: Index Load T ag; I-Cache Read the content of the tag for the cache line at the specified index and place it into the T agLo and T agHi CP0 r egisters, ignoring parity err ors.

CACHE 0x5, offset(rs) op = 5: Index Load T ag; D-Cache CACHE 0x8, offset(rs) op = 8: Index Stor e Tag; I-Cache Write the tag for the cache line at the specified index fr om with the contents of the TagLo and T agHi CP0 r egisters.

CACHE 0x9, offset(rs) op = 9: Index Stor e Tag; D-Cache CACHE 0xD, offset(rs) op = D: Create Dirty Line; D-Cache This operation is used to avoid loading data needlessly fr om main memory when writing new contents into an entir e cache line. If the cache line does not contain the specified addr ess, and the line is dirty , it will be written back to main memory . In all cases, set the cache line tag to the specified physical addr ess, and set the cache state to valid dirty .

CACHE 0x10, offset(rs) op = 10: Hit Invalidate; I-Cache If the cache line contains the specified addr ess, mark the cache line invalid. CACHE 0x11, offset(rs) op = 11: Hit Invalidate; D-Cache CACHE 0x14, offset(rs) op = 14: Fill; I-Cache Fill the instr uction cache line fr om main memory . CACHE 0x15, offset(rs) op = 15: Hit Write-back Invalidate; D-Cache If the cache line contains the specified addr ess, and it is dirty , the data will be written back to main memory . Then, then cache line is set to invalid.

CACHE 0x18, offset(rs) op = 18: Hit Write-back; I-Cache If the cache line contains the specified addr ess, and it is dirty , write back the data to memory , and clear the dirty bit. For instr uction cache, the cache line will be written back to main memory unconditionally .

CACHE 0x19, offset(rs) op = 19: Hit Write-back; D-Cache