Contents|Index|Previous|Next

Intel 960 Dependent Features

The following documentation discusses the i960 architecture’s features and options for the assembler.

Options for i960

Floating Point for i960

Machine Directives for i960

Opcodes for i960

callj

Compare-and-Branch for i960

Options for i960

-ACA | -ACA_A | -ACB | -ACC | -AKA | -AKB | -AKC | -AMC
Select the 960 architecture. Instructions or features not supported by the selected architecture cause fatal errors.

-ACA is equivalent to -ACA_A; -AKC is equivalent to -AMC.

Synonyms are provided for compatibility with other tools.

If you do not specify any of these options, as generates code for any instruction or feature that is supported by some version of the 960 (even if this means mixing architectures!).

In principle, as attempts to deduce the minimal sufficient processor type if none is specified; depending on the object code format, the processor type may be recorded in the object file.

If it is critical that the as output match a specific architecture, specify that architecture explicitly.

-b
Add code to collect information about conditional branches taken, for later optimization using branch prediction bits. (The conditional branch instructions have branch prediction bits in the CA, CB, and CC architectures.) If BR represents a conditional branch instruction, the following represents the code generated by the assembler when -b is specified.

call increment routine
.word 0 # pre-counter
Label: BR
call increment routine
.word 0 # post-counter

The counter following a branch records the number of times that branch was not taken; the difference between the two counters is the number of times the branch was taken.

A table of every such Label is also generated, so that the external postprocessor gbr960 (supplied by Intel) can locate all the counters. This table is always labeled __BRANCH_TABLE__; this is a local symbol to permit collecting statistics for many separate object files. The table is word aligned, and begins with a two-word header. The first word, initialized to 0, is used in maintaining linked lists of branch tables. The second word is a count of the number of entries in the table, which follow immediately: each is a word, pointing to one of the labels illustrated in the previous example.

*NEXT | COUNT: N | *BRLAB 1 | ... | *BRLAB N

_BRANCH_TABLE_ layout

The first word of the header is used to locate multiple branch tables, since each object file may contain one. Normally the links are maintained with a call to an initialization routine, placed at the beginning of each function in the file. The GNU C compiler generates these calls automatically when you give it a -b option. For further details, see the documentation of gbr960.

-no-relax
Normally, Compare-and-Branch instructions with targets that require displacements greater than 13 bits (or that have external targets) are replaced with the corresponding compare (or chkbit) and branch instructions. You can use the -no-relax option to specify that as should generate errors instead, if the target displacement is larger than 13 bits.
This option does not affect the Compare-and-Jump instructions; the code emitted for them is always adjusted when necessary (depending on displacement size), regardless of whether you use -no-relax.

Floating Point for i960

as generates IEEE floating-point numbers for the directives .float, .double, .extended, and .single.

Machine Directives for i960

.bss symbol, length, align
Reserve length bytes in the bss section for a local symbol, aligned to the power of two specified by align. length and align must be positive absolute expressions. This directive differs from .lcomm only in that it permits you to specify an alignment. See .lcomm symbol, length .

.extended flonums
.extended expects zero or more flonums, separated by commas; for each flonum, .extended emits an IEEE extended-format (80-bit) floating-point number.

.leafproc call-lab, bal-lab
You can use the .leafproc directive in conjunction with the optimized callj instruction to enable faster calls of leaf procedures. If a procedure is known to call no other procedures, you may define an entry point that skips procedure prolog code (and that does not depend on system-supplied saved context), and declare it as the bal-lab using .leafproc. If the procedure also has an entry point that goes through the normal prolog, you can specify that entry point as call-lab.

A .

leafproc declaration is meant for use in conjunction with the optimized call instruction callj; the directive records the data needed later to choose between converting the callj into a bal or a call.
call-lab is optional; if only one argument is present, or if the two arguments are identical, the single argument is assumed to be the bal entry point.

.sysproc name, index
The .sysproc directive defines a name for a system pro-cedure. After you define it using .sysproc, you can use name to refer to the system procedure identified by index when calling procedures with the optimized call instruction callj.

Both arguments are required;

index must be between 0 and 31 (inclusive).

Opcodes for i960

All Intel 960 machine instructions are supported; see Options for i960 for a discussion of selecting the instruction subset for a particular 960 architecture. Some opcodes are processed beyond simply emitting a single corresponding instruction: callj, and Compare-and-Branch or Compare-and- Jump instructions with target displacements larger than 13 bits.

callj

You can write callj to have the assembler or the linker determine the most appropriate form of subroutine call: call, bal, or calls. If the assembly source contains enough information—a .leafproc or .sysproc directive defining the operand—then as translates the callj; if not, it simply emits the callj, leaving it for the linker to resolve.

Compare-and-Branch for i960

The 960 architectures provide combined Compare-and-Branch instructions that permit you to store the branch target in the lower 13 bits of the instruction word itself. However, if you specify a branch target far enough away that its address won’t fit in 13 bits, the assembler can either issue an error, or convert your Compare-and-Branch instruction into separate instructions to do the compare and the branch. Whether as gives an error or expands the instruction depends on two choices you can make: whether you use the -no-relax option, and whether you use a “Compare and Branch” instruction or a “Compare and Jump” instruction. The “Jump” instructions are always expanded if necessary; the “Branch” instructions are expanded when necessary unless you specify -no-relax—in which case as gives an error instead.

The following example shows the Compare-and-Branch instructions, their “Jump” variants, and the instruction pairs into which they may expand.

Compare and
Branch Jump Expanded to

bbc chkbit; bno
bbs chkbit; bo
cmpibe cmpije cmpi; be
cmpibg cmpijg cmpi; bg
cmpibge cmpijge cmpi; bge
cmpibl cmpijl cmpi; bl
cmpible cmpijle cmpi; ble
cmpibno cmpijno cmpi; bno
cmpibne cmpijne cmpi; bne
cmpibo cmpijo cmpi; bo
cmpobe cmpoje cmpo; be
cmpobg cmpojg cmpo; bg
cmpobge cmpojge cmpo; bge
cmpobl cmpojl cmpo; bl
cmpoble cmpojle cmpo; ble
cmpobne cmpojne cmpo; bne