Contents|Index|Previous|Next

Disk space requirements for UNIX

The following documentation shows minimum disk space requirements (in megabytes) for UNIX installations of binaries only, source code only, and the sum totals. Sizes shown are for native distributions; see your distribution label for the actual disk size.

platform |  |  |  |
| target | Binaries | Source | Total
alpha-dec-osf2.0 | alpha-dec-osf2.0 | 118 | 135 | 253
alpha-dec-osf4.0 | alpha-dec-osf4.0 | 122 | 135 | 257
hppa1.1-hp-hpux10.20 | hppa1.1-hp-hpux10.20 | 106 | 135 | 241
hppa1.1-hp-hpux10 | hppa1.1-hp-hpux10 | 92 | 135 | 227
hppa1.1-hp-hpux9 | hppa1.1-hp-hpux9 | 92 | 135 | 227
mips-sgi-irix5 | mips-ecoff | 149 | 135 | 284
| mips-elf | 162 | 135 | 297
| mips-sgi-irix5 | 117 | 135 | 252
| mips64-elf | 162 | 135 | 297
| sh-hms | 128 | 135 | 263
powerpc-ibm-aix4.1 | powerpc-ibm-aix4.1 | 88 | 135 | 223
rs6000-ibm-aix3.2.5 | rs6000-ibm-aix3.2.5 | 86 | 135 | 221
rs6000-ibm-aix4.1 | rs6000-ibm-aix4.1 | 88 | 135 | 223
sparc-sun-solaris2.5 | sparc-sun-solaris2.5 | 68 | 135 | 203
sparc-sun-solaris2 | h8300-hms | 75 | 135 | 210
| i960-coff | 77 | 135 | 212
| m68k-aout | 73 | 135 | 208
| m68k-coff | 79 | 135 | 214
| mips-ecoff | 104 | 135 | 239
| mips-elf | 113 | 135 | 248
| mips64-elf | 113 | 135 | 248
| powerpc-eabi | 123 | 135 | 258
| sh-hms | 81 | 135 | 216
| sparc-sun-solaris2 | 68 | 135 | 203
sparc-sun-sunos4.1 | powerpc-ibm-aix4.1 | 88 | 135 | 223
| h8300-hms | 74 | 135 | 209
| i960-coff | 76 | 135 | 211
| m68k-aout | 71 | 135 | 206
| m68k-coff | 77 | 135 | 212
| mips-elf | 111 | 135 | 246
| mips64-elf | 111 | 135 | 246
| powerpc-eabi | 122 | 135 | 257
| sh-hms | 80 | 135 | 215
| sparc-sun-sunos4.1 | 63 | 135 | 198